(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~84~ubuntu19.04.1)
  (general
    (thickness 1.6)
    (drawings 180)
    (tracks 22534)
    (zones 0)
    (modules 1510)
    (nets 110)
  )
  (page USLedger)
  (layers
    (0 F.Cu signal)
    (1 GND power)
    (2 PWR power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.29337)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.29337)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.0889)
    (zone_clearance 0.1)
    (zone_45_only no)
    (trace_min 0.0889)
    (via_size 0.5)
    (via_drill 0.25)
    (via_min_size 0.45)
    (via_min_drill 0.2)
    (user_via 0.45 0.2)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.15 5.15)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF77F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/revA/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /RF/VDDR)
  (net 3 /RF/RX_TX)
  (net 4 "/Boost Converters/3V3_BUCK_VOUT")
  (net 5 /RF/DCDC_SW)
  (net 6 VDD)
  (net 7 "/USB Input/MSP430_TCK")
  (net 8 "/USB Input/MSP430_TDO")
  (net 9 "/USB Input/MSP430_TMS")
  (net 10 "/USB Input/MSP430_TDI")
  (net 11 /RF/RF_2_4GHZ_P)
  (net 12 /RF/RF_2_4GHZ_N)
  (net 13 /RF/RF_SUB_1GHZ_P)
  (net 14 /RF/RF_SUB_1GHZ_N)
  (net 15 "/USB Input/D-")
  (net 16 "/USB Input/D+")
  (net 17 RESET_N)
  (net 18 "Net-(AE801-Pad1)")
  (net 19 VDDS)
  (net 20 3V3)
  (net 21 "Net-(C803-Pad2)")
  (net 22 USER1)
  (net 23 V_ALT)
  (net 24 LED1)
  (net 25 LED2)
  (net 26 900M)
  (net 27 2.4G)
  (net 28 5V)
  (net 29 CC1352_TDI)
  (net 30 CC1352_TMS)
  (net 31 CC1352_TDO)
  (net 32 CC1352_TCK)
  (net 33 MISO)
  (net 34 CS_MB2)
  (net 35 SCK)
  (net 36 AN_MB2)
  (net 37 RST_MB2)
  (net 38 MOSI)
  (net 39 INT_MB2)
  (net 40 CC1352_RX_MB2_TX)
  (net 41 SDA)
  (net 42 PWM_MB2)
  (net 43 CC1352_TX_MB2_RX)
  (net 44 SCL)
  (net 45 CC1352_TX_MB1_RX)
  (net 46 PWM_MB1)
  (net 47 CC1352_RX_MB1_TX)
  (net 48 INT_MB1)
  (net 49 RST_MB1)
  (net 50 AN_MB1)
  (net 51 CS_MB1)
  (net 52 "Net-(R802-Pad1)")
  (net 53 CC1352_TX_MSP430_RX)
  (net 54 CC1352_RX_MSP430_TX)
  (net 55 "Net-(AE801-Pad3)")
  (net 56 "Net-(AE802-Pad1)")
  (net 57 "Net-(B801-Pad1)")
  (net 58 "Net-(B801-Pad4)")
  (net 59 "Net-(C602-Pad2)")
  (net 60 "Net-(C801-Pad1)")
  (net 61 "Net-(C802-Pad1)")
  (net 62 "Net-(C811-Pad2)")
  (net 63 "Net-(C813-Pad2)")
  (net 64 "Net-(C816-Pad2)")
  (net 65 "Net-(C817-Pad1)")
  (net 66 "Net-(C818-Pad2)")
  (net 67 "Net-(C821-Pad2)")
  (net 68 "Net-(D401-Pad1)")
  (net 69 "Net-(D402-Pad1)")
  (net 70 "Net-(D403-Pad1)")
  (net 71 "Net-(D404-Pad1)")
  (net 72 "Net-(D405-Pad1)")
  (net 73 "Net-(L601-Pad1)")
  (net 74 "Net-(R601-Pad1)")
  (net 75 "Net-(R803-Pad1)")
  (net 76 "Net-(R809-Pad2)")
  (net 77 "Net-(U801-Pad46)")
  (net 78 "Net-(U801-Pad47)")
  (net 79 "/USB Input/VBUS")
  (net 80 "Net-(C501-Pad2)")
  (net 81 "Net-(C504-Pad2)")
  (net 82 "Net-(C505-Pad2)")
  (net 83 "Net-(P501-PadB5)")
  (net 84 "Net-(P501-PadA5)")
  (net 85 "/USB Input/MSP_PUR")
  (net 86 "Net-(R509-Pad2)")
  (net 87 "Net-(R510-Pad2)")
  (net 88 "/USB Input/XTAL1")
  (net 89 "/USB Input/XTAL2")
  (net 90 "/USB Input/D_N")
  (net 91 "/USB Input/D_P")
  (net 92 "Net-(R1003-Pad2)")
  (net 93 "Net-(R1003-Pad1)")
  (net 94 INT_SENSOR)
  (net 95 INT_HDC2010)
  (net 96 "Net-(R1004-Pad1)")
  (net 97 "Net-(R1005-Pad1)")
  (net 98 "Net-(R1006-Pad2)")
  (net 99 INT_LIS2DE12_2)
  (net 100 INT_OPT3001)
  (net 101 "Net-(R1008-Pad2)")
  (net 102 ALT_IN)
  (net 103 "Net-(D406-Pad1)")
  (net 104 ~CHG)
  (net 105 "Net-(R506-Pad1)")
  (net 106 "/USB Input/MSP430_RST_N")
  (net 107 "Net-(R507-Pad2)")
  (net 108 "Net-(R511-Pad2)")
  (net 109 ~FLASH_CS)
  (net_class Default "This is the default net class."
    (clearance 0.0889)
    (trace_width 0.0889)
    (via_dia 0.5)
    (via_drill 0.25)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net "/Boost Converters/3V3_BUCK_VOUT")
    (add_net /RF/DCDC_SW)
    (add_net /RF/RF_2_4GHZ_N)
    (add_net /RF/RF_2_4GHZ_P)
    (add_net /RF/RF_SUB_1GHZ_N)
    (add_net /RF/RF_SUB_1GHZ_P)
    (add_net /RF/RX_TX)
    (add_net /RF/VDDR)
    (add_net "/USB Input/D+")
    (add_net "/USB Input/D-")
    (add_net "/USB Input/D_N")
    (add_net "/USB Input/D_P")
    (add_net "/USB Input/MSP430_RST_N")
    (add_net "/USB Input/MSP430_TCK")
    (add_net "/USB Input/MSP430_TDI")
    (add_net "/USB Input/MSP430_TDO")
    (add_net "/USB Input/MSP430_TMS")
    (add_net "/USB Input/MSP_PUR")
    (add_net "/USB Input/VBUS")
    (add_net "/USB Input/XTAL1")
    (add_net "/USB Input/XTAL2")
    (add_net 2.4G)
    (add_net 3V3)
    (add_net 5V)
    (add_net 900M)
    (add_net ALT_IN)
    (add_net AN_MB1)
    (add_net AN_MB2)
    (add_net CC1352_RX_MB1_TX)
    (add_net CC1352_RX_MB2_TX)
    (add_net CC1352_RX_MSP430_TX)
    (add_net CC1352_TCK)
    (add_net CC1352_TDI)
    (add_net CC1352_TDO)
    (add_net CC1352_TMS)
    (add_net CC1352_TX_MB1_RX)
    (add_net CC1352_TX_MB2_RX)
    (add_net CC1352_TX_MSP430_RX)
    (add_net CS_MB1)
    (add_net CS_MB2)
    (add_net GND)
    (add_net INT_HDC2010)
    (add_net INT_LIS2DE12_2)
    (add_net INT_MB1)
    (add_net INT_MB2)
    (add_net INT_OPT3001)
    (add_net INT_SENSOR)
    (add_net LED1)
    (add_net LED2)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(AE801-Pad1)")
    (add_net "Net-(AE801-Pad3)")
    (add_net "Net-(AE802-Pad1)")
    (add_net "Net-(B801-Pad1)")
    (add_net "Net-(B801-Pad4)")
    (add_net "Net-(C501-Pad2)")
    (add_net "Net-(C504-Pad2)")
    (add_net "Net-(C505-Pad2)")
    (add_net "Net-(C602-Pad2)")
    (add_net "Net-(C801-Pad1)")
    (add_net "Net-(C802-Pad1)")
    (add_net "Net-(C803-Pad2)")
    (add_net "Net-(C811-Pad2)")
    (add_net "Net-(C813-Pad2)")
    (add_net "Net-(C816-Pad2)")
    (add_net "Net-(C817-Pad1)")
    (add_net "Net-(C818-Pad2)")
    (add_net "Net-(C821-Pad2)")
    (add_net "Net-(D401-Pad1)")
    (add_net "Net-(D402-Pad1)")
    (add_net "Net-(D403-Pad1)")
    (add_net "Net-(D404-Pad1)")
    (add_net "Net-(D405-Pad1)")
    (add_net "Net-(D406-Pad1)")
    (add_net "Net-(L601-Pad1)")
    (add_net "Net-(P501-PadA5)")
    (add_net "Net-(P501-PadB5)")
    (add_net "Net-(R1003-Pad1)")
    (add_net "Net-(R1003-Pad2)")
    (add_net "Net-(R1004-Pad1)")
    (add_net "Net-(R1005-Pad1)")
    (add_net "Net-(R1006-Pad2)")
    (add_net "Net-(R1008-Pad2)")
    (add_net "Net-(R506-Pad1)")
    (add_net "Net-(R507-Pad2)")
    (add_net "Net-(R509-Pad2)")
    (add_net "Net-(R510-Pad2)")
    (add_net "Net-(R511-Pad2)")
    (add_net "Net-(R601-Pad1)")
    (add_net "Net-(R802-Pad1)")
    (add_net "Net-(R803-Pad1)")
    (add_net "Net-(R809-Pad2)")
    (add_net "Net-(U801-Pad46)")
    (add_net "Net-(U801-Pad47)")
    (add_net PWM_MB1)
    (add_net PWM_MB2)
    (add_net RESET_N)
    (add_net RST_MB1)
    (add_net RST_MB2)
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net USER1)
    (add_net VDD)
    (add_net VDDS)
    (add_net V_ALT)
    (add_net ~CHG)
    (add_net ~FLASH_CS)
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 214.88 142.1)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 66.88 142.1)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 66.88 48.1)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 214.88 48.1)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Fiducial:Fiducial_1.5mm_Mask3mm (layer F.Cu) (tedit 5C18CB26)
    (at 209.88 142.1)
    (descr "Circular Fiducial, 1.5mm bare copper, 3mm soldermask opening")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 -2.4765) (layer F.SilkS) hide)
    (fp_text value Fiducial_1.5mm_Mask3mm (at 0 2.6035) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (solder_mask_margin 0.75) (clearance 0.75))
  )
  (module Fiducial:Fiducial_1.5mm_Mask3mm (layer B.Cu) (tedit 5C18CB26)
    (at 214.88 137.1)
    (descr "Circular Fiducial, 1.5mm bare copper, 3mm soldermask opening")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 2.4765) (layer B.SilkS) hide)
    (fp_text value Fiducial_1.5mm_Mask3mm (at 0 -2.6035) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad "" smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (solder_mask_margin 0.75) (clearance 0.75))
  )
  (module Fiducial:Fiducial_1.5mm_Mask3mm (layer B.Cu) (tedit 5C18CB26)
    (at 66.88 53.1)
    (descr "Circular Fiducial, 1.5mm bare copper, 3mm soldermask opening")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 2.4765) (layer B.SilkS) hide)
    (fp_text value Fiducial_1.5mm_Mask3mm (at 0 -2.6035) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad "" smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (solder_mask_margin 0.75) (clearance 0.75))
  )
  (module Fiducial:Fiducial_1.5mm_Mask3mm (layer F.Cu) (tedit 5C18CB26)
    (at 71.88 48.1)
    (descr "Circular Fiducial, 1.5mm bare copper, 3mm soldermask opening")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 -2.4765) (layer F.SilkS) hide)
    (fp_text value Fiducial_1.5mm_Mask3mm (at 0 2.6035) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (solder_mask_margin 0.75) (clearance 0.75))
  )
  (module Fiducial:Fiducial_1.5mm_Mask3mm (layer F.Cu) (tedit 5C18CB26)
    (at 66.88 137.1)
    (descr "Circular Fiducial, 1.5mm bare copper, 3mm soldermask opening")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 -2.4765) (layer F.SilkS) hide)
    (fp_text value Fiducial_1.5mm_Mask3mm (at 0 2.6035) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (solder_mask_margin 0.75) (clearance 0.75))
  )
  (module Fiducial:Fiducial_1.5mm_Mask3mm (layer B.Cu) (tedit 5C18CB26)
    (at 71.88 142.1)
    (descr "Circular Fiducial, 1.5mm bare copper, 3mm soldermask opening")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 2.4765) (layer B.SilkS) hide)
    (fp_text value Fiducial_1.5mm_Mask3mm (at 0 -2.6035) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad "" smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (solder_mask_margin 0.75) (clearance 0.75))
  )
  (module leash:MikroBus-SMD locked (layer F.Cu) (tedit 5E541D62)
    (at 156.68 65.6 90)
    (fp_text reference J701 (at -0.074182 -1.275144 90) (layer F.SilkS) hide)
    (fp_text value mikroBUS (at -0.074182 -0.005144 90) (layer F.Fab))
    (fp_text user %R (at 11.355818 -0.005144 180) (layer F.Fab) hide)
    (fp_text user %R (at 11.43 0 180) (layer F.Fab))
    (pad 5 smd rect (at -9.78 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -9.78 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 51 CS_MB1))
    (pad 7 smd rect (at -9.78 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 20 3V3))
    (pad 4 smd rect (at -13.08 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 35 SCK))
    (pad 1 smd rect (at -9.78 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 50 AN_MB1))
    (pad 2 smd rect (at -13.08 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 49 RST_MB1))
    (pad 6 smd rect (at -13.08 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 38 MOSI))
    (pad 8 smd rect (at -13.08 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 9.78 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 48 INT_MB1))
    (pad 13 smd rect (at 9.78 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 47 CC1352_RX_MB1_TX))
    (pad 11 smd rect (at 9.78 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 9 smd rect (at 9.78 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 13.08 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM_MB1))
    (pad 14 smd rect (at 13.08 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 45 CC1352_TX_MB1_RX))
    (pad 12 smd rect (at 13.08 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 13.08 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 211.39 65.09 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C506 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 202.96 59.22 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R501 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(P501-PadB5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N48_EP5.15x5.15mm (layer B.Cu) (tedit 5E4C745D)
    (at 171.05 100.15 180)
    (descr "QFN, 48 Pin (http://www.ti.com/lit/ds/symlink/msp430f5232.pdf#page=112), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U501 (at 0 4.82) (layer B.SilkS) hide)
    (fp_text value MSP430F5500IRGZ (at 0 -4.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 48 smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 47 smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 46 smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 45 smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 44 smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 43 smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 42 smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 41 smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 40 smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 39 smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 38 smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 37 smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 36 smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 35 smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 34 smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 33 smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 32 smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 31 smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 30 smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 29 smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 28 smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 27 smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 26 smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 25 smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 24 smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 23 smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 22 smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 21 smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 20 smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 19 smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 18 smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 17 smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 16 smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 15 smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 14 smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 12 smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 10 smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 6 smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad 49 smd roundrect (at 0 0 180) (size 5.15 5.15) (layers B.Cu B.Mask) (roundrect_rratio 0.049)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N48_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:0900PC15A0036 (layer F.Cu) (tedit 5E41EA1D)
    (at 150.14 95.44 270)
    (fp_text reference B801 (at 0.025 4.2 90) (layer F.SilkS) hide)
    (fp_text value 0900PC15A0036E (at -0.05 -3.025 90) (layer F.Fab))
    (pad 10 smd roundrect (at -1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 smd roundrect (at 1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 9 smd roundrect (at -0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 8 smd roundrect (at -0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 7 smd roundrect (at 0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 6 smd roundrect (at 0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 1 smd roundrect (at -0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 2 smd roundrect (at -0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at 0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at 0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (model ${KIPRJMOD}/mech/0900PC15J0013.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 143.38 82.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H103 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 181.2 67.3 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L804 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:X2SON-8_1.4x1mm_P0.35mm (layer B.Cu) (tedit 5A02F1D8)
    (at 188.63 59.85 180)
    (descr "X2SON-8 1.4x1mm Pitch0.35mm http://www.ti.com/lit/ds/symlink/pca9306.pdf")
    (tags "X2SON-8 1.4x1mm Pitch0.35mm")
    (attr smd)
    (fp_text reference U1002 (at 0 2) (layer B.SilkS) hide)
    (fp_text value SN74AUP2G32 (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 8 smd rect (at 0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 19 VDDS))
    (pad 7 smd rect (at 0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 6 smd rect (at 0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 5 smd rect (at 0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 94 INT_SENSOR))
    (pad 2 smd rect (at -0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd rect (at -0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 95 INT_HDC2010))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 186.21 58.29 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1002 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer F.Cu) (tedit 5E4C72AA)
    (at 200.4 65.5 270)
    (attr virtual)
    (fp_text reference J301 (at 0.302285 2.603303 270) (layer F.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at -0.967715 -2.222697 270) (layer F.Fab))
    (pad 4 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 32 CC1352_TCK))
    (pad 5 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 31 CC1352_TDO))
    (pad 7 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 1 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 20 3V3))
    (pad 10 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 17 RESET_N))
    (pad 2 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 30 CC1352_TMS))
    (pad 9 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 3 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 8 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 29 CC1352_TDI))
  )
  (module leash:MX25R8035FZUIL0 (layer B.Cu) (tedit 5E42FFC6)
    (at 152.775 101.08 270)
    (fp_text reference U802 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value MX25R8035FZUIL0 (at 0 -2 90) (layer B.Fab))
    (pad 9 smd custom (at 0 0 270) (size 0.2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0 0.8) (xy 0.1 0.8) (xy 0.1 -0.8) (xy -0.1 -0.8) (xy -0.1 0.7)
) (width 0))
      ))
    (pad 8 smd rect (at 1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C811-Pad2)"))
    (pad 7 smd rect (at 1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 6 smd rect (at 1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 5 smd rect (at 1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 4 smd rect (at -1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R809-Pad2)"))
    (pad 2 smd rect (at -1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 1 smd rect (at -1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 109 ~FLASH_CS))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.9 80.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D404 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 162.25 95.625)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L801 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.725 71.525)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 179.85 67.95 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C817 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "5.6 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD (layer B.Cu) (tedit 5E541D54)
    (at 156.6 95.6 90)
    (fp_text reference J702 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value mikroBUS (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at -11.43 0) (layer B.Fab))
    (fp_text user %R (at 11.43 0) (layer B.Fab))
    (pad 5 smd rect (at -9.78 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -9.78 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 34 CS_MB2))
    (pad 7 smd rect (at -9.78 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 20 3V3))
    (pad 4 smd rect (at -13.08 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 1 smd rect (at -9.78 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 36 AN_MB2))
    (pad 2 smd rect (at -13.08 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 37 RST_MB2))
    (pad 6 smd rect (at -13.08 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 8 smd rect (at -13.08 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 9.78 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 39 INT_MB2))
    (pad 13 smd rect (at 9.78 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 40 CC1352_RX_MB2_TX))
    (pad 11 smd rect (at 9.78 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 41 SDA))
    (pad 9 smd rect (at 9.78 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 13.08 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 42 PWM_MB2))
    (pad 14 smd rect (at 13.08 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 43 CC1352_TX_MB2_RX))
    (pad 12 smd rect (at 13.08 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 13.08 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer B.Cu) (tedit 5A0FD1B2)
    (at 209.805 62.475)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y501 (at 0 2.45) (layer B.SilkS) hide)
    (fp_text value 24MHz (at 0 -2.45) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 4 smd rect (at -1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 "/USB Input/XTAL2"))
    (pad 2 smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 "/USB Input/XTAL1"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 155.6 132.925 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:USON6 (layer B.Cu) (tedit 5E4DAB76)
    (at 193.16 61.09 180)
    (fp_text reference U1003 (at 0.11 -3.68) (layer B.SilkS) hide)
    (fp_text value OPT3001 (at -0.16 3.7) (layer B.Fab))
    (pad 7 thru_hole circle (at 0 -0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 smd rect (at 0 0 180) (size 0.65 1.35) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.02))
    (pad 6 smd roundrect (at 0.95 0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 41 SDA) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at 0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 100 INT_OPT3001) (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at 0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 44 SCL) (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 101 "Net-(R1008-Pad2)") (solder_mask_margin 0.07))
    (pad 1 smd roundrect (at -0.95 0.675 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 19 VDDS) (solder_mask_margin 0.07))
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 168.63 82.575 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D501 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.32 94.11 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C814 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 160.025 125.1 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C804 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 191.21 57.74)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1004 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(R1004-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:L_0806_2012Metric (layer B.Cu) (tedit 5D2F3EE6)
    (at 168.985 89.9 90)
    (descr "Inductor SMD 0806 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L601 (at 0 1.65 90) (layer B.SilkS) hide)
    (fp_text value INDUCTOR (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(L601-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 160.43 88.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R802 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 CC1352_TX_MB2_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 155.6 102.925 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer B.Cu) (tedit 5D409D35)
    (at 164.4 95.5 270)
    (attr virtual)
    (fp_text reference J501 (at 3.81 -2.413 90) (layer B.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at 2.54 2.413 90) (layer B.Fab))
    (pad 4 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 5 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 6 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 7 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 1 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 20 3V3))
    (pad 10 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 2 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 9 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 3 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 8 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 10 "/USB Input/MSP430_TDI"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.84 95.49 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R508 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1.5K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 147.825 96.175 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C813 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 146.3 92.1 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C816 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 200.05 120.75)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U502 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value BQ21040 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R506-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 ~CHG))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 158.05 88.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R803 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 CC1352_RX_MB2_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:0900PC15A0036 (layer F.Cu) (tedit 5E41EA1D)
    (at 186.14 125.44 270)
    (fp_text reference B801 (at 0.025 4.2 90) (layer F.SilkS) hide)
    (fp_text value 0900PC15A0036E (at -0.05 -3.025 90) (layer F.Fab))
    (pad 10 smd roundrect (at -1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 smd roundrect (at 1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 9 smd roundrect (at -0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 8 smd roundrect (at -0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 7 smd roundrect (at 0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 6 smd roundrect (at 0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 1 smd roundrect (at -0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 2 smd roundrect (at -0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at 0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at 0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (model ${KIPRJMOD}/mech/0900PC15J0013.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 159.38 102.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C803 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 173 95.57 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C504 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 220N (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 194.38 72.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C805 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 190.63 58.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1002 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.725 99.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R809 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R809-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 169.98 107.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R507 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 142.28 91.315 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C822 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(AE801-Pad3)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 205.255 52.75 270)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW901 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 1 smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 2 smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 187.39 57.76 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1005 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(R1005-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 166.44 100.55 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R509 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 205.255 112.75 270)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW901 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 1 smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 2 smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 162.25 125.625)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L801 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 158.38 102.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C805 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 143.25 102.85 90)
    (fp_text reference J802 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C821-Pad2)"))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 144.88 91.4 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C818 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C818-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 191.58 58.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1001 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.505 88.3 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R604 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 182.3 62.1 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C816 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 143.85 97.95 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C817 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "5.6 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 155.58 88.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1001 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:TPS62821DLC (layer B.Cu) (tedit 5D2676FA)
    (at 166.885 91.1)
    (fp_text reference U601 (at 0.1 1.975 180) (layer B.SilkS) hide)
    (fp_text value TPS62821DLC (at 0 0.5 180) (layer B.Fab))
    (pad 8 smd roundrect (at 0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 74 "Net-(R601-Pad1)"))
    (pad 7 smd roundrect (at 0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 6 smd roundrect (at 0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 73 "Net-(L601-Pad1)"))
    (pad 5 smd roundrect (at 0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 4 smd roundrect (at -0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2))
    (pad 3 smd roundrect (at -0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1.3 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.875 95.925 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C815 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2.7 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 188.805 72.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C806 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 186.855 131.125 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C802 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.55 102.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 169.255 82.75 270)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW901 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 1 smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 2 smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 203.14 123.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F801 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value Polyfuse (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.36 118.01)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F501 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value Polyfuse (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 202.97 90.16 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C508 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.63 70.5 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C801 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 169.18 137.25 90)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW902 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 1 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 161.975 123.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R805 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 159.145 110.58)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D402 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.95 122.05 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R502 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(P501-PadA5)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 181.25 69.375 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C820 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(AE802-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 195.68 121.11 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1008 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(R1008-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 193.525 132.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 196.025 125.1 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C804 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.63 130.5 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C801 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 192.25 110.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R401 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 171.08 100.2 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J201 (at 0 -5.8 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.95 90) (layer F.Fab) hide)
    (pad MP smd roundrect (at 3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at -3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad 2 smd roundrect (at 1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.step
      (offset (xyz -1 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 202.97 60.16 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C508 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 200.23 119.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R603 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 190.88 121.9 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C809 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 186.725 133.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 186.855 71.125 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C802 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 191.21 117.74)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1004 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(R1004-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 171.655 89.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R503 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 90 "/USB Input/D_N"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 188.4 91.3 180)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y802 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Crystal_GND2 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U801-Pad46)"))
    (pad 2 smd rect (at 0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U801-Pad47)"))
    (pad 4 smd rect (at -0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 156.25 110.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D401 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 192.55 102.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 193.525 102.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.725 131.525)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 191.6 72.925 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 191.21 87.74)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1004 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(R1004-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 196.025 95.1 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C804 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LGA:LGA-12_2x2mm_P0.5mm (layer F.Cu) (tedit 5A0AAFFD)
    (at 152.01 118.69 180)
    (descr LGA12)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U1004 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value LIS2DE12 (at 0 1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at -0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 9 smd rect (at 0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 8 smd rect (at 0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 7 smd rect (at 0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 5 smd rect (at -0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 99 INT_LIS2DE12_2))
    (pad 12 smd rect (at -0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 149.755 129.575 315)
    (descr "SMD Crystal 2012/2 http://txccrystal.com/images/pdf/9ht11.pdf, 2.0x1.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y801 (at 0 -1.8 135) (layer F.SilkS) hide)
    (fp_text value Crystal (at 0 1.8 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C801-Pad1)"))
    (pad 2 smd rect (at 0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_AX_8045-2Pin_8.0x4.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.25 0.3 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.725 72.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.9 110.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D404 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 166.4 125.99 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R505 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:L_0806_2012Metric (layer B.Cu) (tedit 5D2F3EE6)
    (at 204.985 119.9 90)
    (descr "Inductor SMD 0806 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L601 (at 0 1.65 90) (layer B.SilkS) hide)
    (fp_text value INDUCTOR (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(L601-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 179.325 129.625 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C821 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C821-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 194.475 72.95 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.535 122.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(R601-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 201.685 59.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 165.49 123.7)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D201 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 202.45 98.65 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R510 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 201.13 50.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D406 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 200.05 60.75)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U502 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value BQ21040 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R506-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 ~CHG))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 181.875 65.925 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C815 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2.7 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 187.23 59.33 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1003 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(R1003-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 157.5 127.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C810 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "22 uF" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 169.755 135.55 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L501 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 167.88 137.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R511 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 179.38 112.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H103 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 146.3 122.1 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C816 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 205.955 76.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C501 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.805 132.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C806 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 201.12 50.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R406 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 ~CHG))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 198.25 125.625)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L801 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm (layer F.Cu) (tedit 5C26A111)
    (at 156.13 127.44)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U801 (at 0 -4.82) (layer F.SilkS) hide)
    (fp_text value CC1352R (at 0 4.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 49 smd roundrect (at 0 0) (size 5.15 5.15) (layers F.Cu F.Mask) (roundrect_rratio 0.048544)
      (net 1 GND))
    (pad "" smd roundrect (at -1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad 1 smd roundrect (at -3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 2 smd roundrect (at -3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 3 smd roundrect (at -3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 4 smd roundrect (at -3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 5 smd roundrect (at -3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 6 smd roundrect (at -3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 7 smd roundrect (at -3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 8 smd roundrect (at -3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 9 smd roundrect (at -3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 10 smd roundrect (at -3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 RST_MB2))
    (pad 11 smd roundrect (at -3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 RST_MB1))
    (pad 12 smd roundrect (at -3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 INT_SENSOR))
    (pad 13 smd roundrect (at -2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 14 smd roundrect (at -2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 15 smd roundrect (at -1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 16 smd roundrect (at -1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 17 smd roundrect (at -0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 18 smd roundrect (at -0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 CS_MB2))
    (pad 19 smd roundrect (at 0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 CS_MB1))
    (pad 20 smd roundrect (at 0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 21 smd roundrect (at 1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 22 smd roundrect (at 1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 23 smd roundrect (at 2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 24 smd roundrect (at 2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 CC1352_TMS))
    (pad 25 smd roundrect (at 3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 CC1352_TCK))
    (pad 26 smd roundrect (at 3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 CC1352_TDO))
    (pad 27 smd roundrect (at 3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 CC1352_TDI))
    (pad 28 smd roundrect (at 3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 29 smd roundrect (at 3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 PWM_MB2))
    (pad 30 smd roundrect (at 3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 INT_MB2))
    (pad 31 smd roundrect (at 3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 32 smd roundrect (at 3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 33 smd roundrect (at 3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 34 smd roundrect (at 3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 35 smd roundrect (at 3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 36 smd roundrect (at 3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 AN_MB1))
    (pad 37 smd roundrect (at 2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 AN_MB2))
    (pad 38 smd roundrect (at 2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 39 smd roundrect (at 1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 40 smd roundrect (at 1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 41 smd roundrect (at 0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 42 smd roundrect (at 0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 INT_MB1))
    (pad 43 smd roundrect (at -0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 PWM_MB1))
    (pad 44 smd roundrect (at -0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 45 smd roundrect (at -1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 46 smd roundrect (at -1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U801-Pad46)"))
    (pad 47 smd roundrect (at -2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U801-Pad47)"))
    (pad 48 smd roundrect (at -2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 169.955 136.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C501 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 202.97 120.16 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C508 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 202.4 95.99 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R505 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MX25R8035FZUIL0 (layer B.Cu) (tedit 5E42FFC6)
    (at 152.775 131.08 270)
    (fp_text reference U802 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value MX25R8035FZUIL0 (at 0 -2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 109 ~FLASH_CS))
    (pad 2 smd rect (at -1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R809-Pad2)"))
    (pad 4 smd rect (at -1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 6 smd rect (at 1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at 1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 8 smd rect (at 1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C811-Pad2)"))
    (pad 9 smd custom (at 0 0 270) (size 0.2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0 0.8) (xy 0.1 0.8) (xy 0.1 -0.8) (xy -0.1 -0.8) (xy -0.1 0.7)
) (width 0))
      ))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 152.4 121.3 180)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y802 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Crystal_GND2 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U801-Pad46)"))
    (pad 2 smd rect (at 0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U801-Pad47)"))
    (pad 4 smd rect (at -0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.47 120.665 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1006 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 INT_LIS2DE12_2))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.96 119.22 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R501 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(P501-PadB5)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 147.825 126.175 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C813 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 209.38 107.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H102 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module leash:HDC2010 (layer F.Cu) (tedit 5E4D6772)
    (at 154.58 88.95)
    (fp_text reference U1001 (at -0.025 2.025) (layer F.SilkS) hide)
    (fp_text value HDC2010 (at 0 -3.8) (layer F.Fab))
    (pad A1 smd circle (at -0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS) (solder_mask_margin 0.05))
    (pad B1 smd circle (at -0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R1004-Pad1)") (solder_mask_margin 0.05))
    (pad C1 smd circle (at -0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad C2 smd circle (at 0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 95 INT_HDC2010) (solder_mask_margin 0.05))
    (pad B2 smd circle (at 0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL) (solder_mask_margin 0.05))
    (pad A2 smd circle (at 0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA) (solder_mask_margin 0.05))
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 157.68 125.9)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L802 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Palconn_UTC16-G (layer F.Cu) (tedit 5CF432E0)
    (at 171.5 120.3 90)
    (descr http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf)
    (tags "USB C Type-C Receptacle USB2.0")
    (attr smd)
    (fp_text reference P501 (at 0 -4.58 90) (layer F.SilkS) hide)
    (fp_text value USB_C_Plug_USB2.0 (at 0 6.24 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.43 90) (layer Dwgs.User))
    (fp_text user %R (at 0 1.18 90) (layer F.Fab))
    (pad A12 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B1 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B4 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B12 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A1 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B9 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A4 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad "" np_thru_hole circle (at -2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad B5 smd rect (at 1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(P501-PadB5)"))
    (pad B6 smd rect (at 0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A8 smd rect (at 1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at -1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P501-PadA5)"))
    (pad B8 smd rect (at -1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A7 smd rect (at 0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 90 "/USB Input/D_N"))
    (pad A6 smd rect (at -0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 91 "/USB Input/D_P"))
    (pad B7 smd rect (at -0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad S1 thru_hole oval (at 4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/1054500101.stp
      (offset (xyz 0 -0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module leash:RFECA3216060A1T (layer F.Cu) (tedit 5E42DF6C)
    (at 178.28 124 270)
    (fp_text reference AE801 (at 0 1.85 90) (layer F.SilkS) hide)
    (fp_text value Antenna_Dipole (at 0.05 -1.7 90) (layer F.Fab))
    (pad 3 smd rect (at -1.4 0 270) (size 0.35 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(AE801-Pad3)"))
    (pad 2 smd rect (at 1.4 0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.4 -0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AE801-Pad1)"))
    (model ${KIPRJMOD}/mech/2450AT18D0100.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.84 125.49 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R508 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1.5K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 187.39 87.76 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1005 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 158.475 102.95 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 161.965 122.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R804 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 182.9 102.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference AE802 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(AE802-Pad1)"))
  )
  (module Package_SON:X2SON-8_1.4x1mm_P0.35mm (layer B.Cu) (tedit 5A02F1D8)
    (at 188.63 89.85 180)
    (descr "X2SON-8 1.4x1mm Pitch0.35mm http://www.ti.com/lit/ds/symlink/pca9306.pdf")
    (tags "X2SON-8 1.4x1mm Pitch0.35mm")
    (attr smd)
    (fp_text reference U1002 (at 0 2) (layer B.SilkS) hide)
    (fp_text value SN74AUP2G32 (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 95 INT_HDC2010))
    (pad 2 smd rect (at -0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 3 smd rect (at -0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 94 INT_SENSOR))
    (pad 4 smd rect (at -0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 7 smd rect (at 0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 8 smd rect (at 0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 195.14 110.57)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R402 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer B.Cu) (tedit 5D409D35)
    (at 164.4 125.5 270)
    (attr virtual)
    (fp_text reference J501 (at 3.81 -2.413 90) (layer B.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at 2.54 2.413 90) (layer B.Fab))
    (pad 8 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 3 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 9 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 2 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 10 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 1 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 20 3V3))
    (pad "" np_thru_hole circle (at 7.62 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 7 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 6 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 5 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 4 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 "/USB Input/MSP430_TCK"))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.25 99.375 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C820 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(AE802-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.805 102.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C806 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 162.96 88.76 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C603 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value "10 uF" (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 156.48 93 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 171.17 93.035 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C507 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 210.68 134.74)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C502 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 10U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 171.08 130.2 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J201 (at 0 -5.8 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.95 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (pad 2 smd roundrect (at 1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad MP smd roundrect (at -3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at 3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.step
      (offset (xyz -1 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.725 132.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 209 125.57 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C504 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 220N (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 149.4 80.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R405 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 185.41 110.6)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D405 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 198.05 110.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R403 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 194.05 118.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R803 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 CC1352_RX_MB2_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 165.13 80.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D406 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD locked (layer F.Cu) (tedit 5E541D62)
    (at 192.68 65.6 90)
    (fp_text reference J701 (at -0.074182 -1.275144 90) (layer F.SilkS) hide)
    (fp_text value mikroBUS (at -0.074182 -0.005144 90) (layer F.Fab))
    (fp_text user %R (at 11.43 0 180) (layer F.Fab))
    (fp_text user %R (at 11.355818 -0.005144 180) (layer F.Fab) hide)
    (pad 10 smd rect (at 13.08 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 12 smd rect (at 13.08 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 14 smd rect (at 13.08 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 45 CC1352_TX_MB1_RX))
    (pad 16 smd rect (at 13.08 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM_MB1))
    (pad 9 smd rect (at 9.78 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 9.78 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 13 smd rect (at 9.78 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 47 CC1352_RX_MB1_TX))
    (pad 15 smd rect (at 9.78 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 48 INT_MB1))
    (pad 8 smd rect (at -13.08 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -13.08 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 38 MOSI))
    (pad 2 smd rect (at -13.08 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 49 RST_MB1))
    (pad 1 smd rect (at -9.78 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 50 AN_MB1))
    (pad 4 smd rect (at -13.08 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at -9.78 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 20 3V3))
    (pad 3 smd rect (at -9.78 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 51 CS_MB1))
    (pad 5 smd rect (at -9.78 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 33 MISO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 201.685 118.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "100 pF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N48_EP5.15x5.15mm (layer B.Cu) (tedit 5E4C745D)
    (at 207.05 130.15 180)
    (descr "QFN, 48 Pin (http://www.ti.com/lit/ds/symlink/msp430f5232.pdf#page=112), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U501 (at 0 4.82) (layer B.SilkS) hide)
    (fp_text value MSP430F5500IRGZ (at 0 -4.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 48 smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 47 smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 46 smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 45 smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 44 smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 43 smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 42 smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 41 smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 40 smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 39 smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 38 smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 37 smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 36 smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 35 smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 34 smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 33 smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 32 smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 31 smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 30 smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 29 smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 28 smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 27 smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 26 smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 25 smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 24 smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 23 smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 22 smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 21 smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 20 smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 19 smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 18 smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 17 smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 16 smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 15 smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 14 smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 12 smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 10 smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 6 smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad 49 smd roundrect (at 0 0 180) (size 5.15 5.15) (layers B.Cu B.Mask) (roundrect_rratio 0.049)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N48_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 204.63 112.575 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D501 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N48_EP5.15x5.15mm (layer B.Cu) (tedit 5E4C745D)
    (at 207.05 100.15 180)
    (descr "QFN, 48 Pin (http://www.ti.com/lit/ds/symlink/msp430f5232.pdf#page=112), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U501 (at 0 4.82) (layer B.SilkS) hide)
    (fp_text value MSP430F5500IRGZ (at 0 -4.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 49 smd roundrect (at 0 0 180) (size 5.15 5.15) (layers B.Cu B.Mask) (roundrect_rratio 0.049)
      (net 1 GND))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad 1 smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 8 smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 12 smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 13 smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 14 smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 15 smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 16 smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 17 smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 18 smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 19 smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 20 smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 21 smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 22 smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 23 smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 24 smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 25 smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 26 smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 27 smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 28 smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 29 smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 30 smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 31 smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 32 smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 33 smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 34 smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 35 smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 36 smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 37 smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 38 smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 39 smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 40 smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 41 smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 42 smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 43 smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 44 smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 45 smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 46 smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 47 smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 48 smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 "/USB Input/MSP430_RST_N"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N48_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.32 124.11 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C814 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 165.12 80.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R406 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 ~CHG))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 196.43 88.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R802 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 CC1352_TX_MB2_RX))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 143.48 87.8 270)
    (fp_text reference J801 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 1 smd rect (at 1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C818-Pad2)"))
    (pad 2 smd rect (at 0 -1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 172.82 104.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C505 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0.47U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 195.68 91.11 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1008 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(R1008-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 195.38 132.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C803 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer B.Cu) (tedit 5D409D35)
    (at 200.4 95.5 270)
    (attr virtual)
    (fp_text reference J501 (at 3.81 -2.413 90) (layer B.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at 2.54 2.413 90) (layer B.Fab))
    (pad 8 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 3 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 9 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 2 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 10 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 1 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 20 3V3))
    (pad "" np_thru_hole circle (at 7.62 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 7 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 6 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 5 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 4 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 "/USB Input/MSP430_TCK"))
  )
  (module leash:L_0806_2012Metric (layer B.Cu) (tedit 5D2F3EE6)
    (at 204.985 89.9 90)
    (descr "Inductor SMD 0806 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L601 (at 0 1.65 90) (layer B.SilkS) hide)
    (fp_text value INDUCTOR (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(L601-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 143.38 107.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H104 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module leash:MikroBus-SMD (layer B.Cu) (tedit 5E541D54)
    (at 192.6 125.6 90)
    (fp_text reference J702 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value mikroBUS (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at -11.43 0) (layer B.Fab))
    (fp_text user %R (at 11.43 0) (layer B.Fab))
    (pad 5 smd rect (at -9.78 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -9.78 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 34 CS_MB2))
    (pad 7 smd rect (at -9.78 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 20 3V3))
    (pad 4 smd rect (at -13.08 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 1 smd rect (at -9.78 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 36 AN_MB2))
    (pad 2 smd rect (at -13.08 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 37 RST_MB2))
    (pad 6 smd rect (at -13.08 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 8 smd rect (at -13.08 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 9.78 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 39 INT_MB2))
    (pad 13 smd rect (at 9.78 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 40 CC1352_RX_MB2_TX))
    (pad 11 smd rect (at 9.78 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 41 SDA))
    (pad 9 smd rect (at 9.78 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 13.08 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 42 PWM_MB2))
    (pad 14 smd rect (at 13.08 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 43 CC1352_TX_MB2_RX))
    (pad 12 smd rect (at 13.08 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 13.08 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 152.9 80.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R404 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 209.38 77.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H102 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module leash:Tag-Connect-10 locked (layer F.Cu) (tedit 5E4C72AA)
    (at 200.4 95.5 270)
    (attr virtual)
    (fp_text reference J301 (at 0.302285 2.603303 270) (layer F.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at -0.967715 -2.222697 270) (layer F.Fab))
    (pad 8 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 29 CC1352_TDI))
    (pad 3 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 9 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 30 CC1352_TMS))
    (pad 10 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 17 RESET_N))
    (pad 1 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 20 3V3))
    (pad 7 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 6 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 31 CC1352_TDO))
    (pad 5 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 32 CC1352_TCK))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 195.68 61.11 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1008 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(R1008-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 162.05 80.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R403 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 149.41 80.6)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D405 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.535 92.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(R601-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 159.14 80.57)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R402 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.25 80.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R401 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 209.38 112.56)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H101 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 181.65 64.12 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C819 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(AE801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 173.38 82.56)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H101 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.63 100.5 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C801 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 209.905 58.875 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference D502 (at 0 2.9 270) (layer B.SilkS) hide)
    (fp_text value TPD2E001 (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 91 "/USB Input/D_P"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 90 "/USB Input/D_N"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 150.855 101.125 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C802 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm (layer F.Cu) (tedit 5C26A111)
    (at 192.13 67.44)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U801 (at 0 -4.82) (layer F.SilkS) hide)
    (fp_text value CC1352R (at 0 4.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 48 smd roundrect (at -2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 47 smd roundrect (at -2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U801-Pad47)"))
    (pad 46 smd roundrect (at -1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U801-Pad46)"))
    (pad 45 smd roundrect (at -1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 44 smd roundrect (at -0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 43 smd roundrect (at -0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 PWM_MB1))
    (pad 42 smd roundrect (at 0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 INT_MB1))
    (pad 41 smd roundrect (at 0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 40 smd roundrect (at 1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 39 smd roundrect (at 1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 38 smd roundrect (at 2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 37 smd roundrect (at 2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 AN_MB2))
    (pad 36 smd roundrect (at 3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 AN_MB1))
    (pad 35 smd roundrect (at 3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 34 smd roundrect (at 3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 33 smd roundrect (at 3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 32 smd roundrect (at 3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 31 smd roundrect (at 3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 30 smd roundrect (at 3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 INT_MB2))
    (pad 29 smd roundrect (at 3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 PWM_MB2))
    (pad 28 smd roundrect (at 3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 27 smd roundrect (at 3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 CC1352_TDI))
    (pad 26 smd roundrect (at 3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 CC1352_TDO))
    (pad 25 smd roundrect (at 3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 CC1352_TCK))
    (pad 24 smd roundrect (at 2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 CC1352_TMS))
    (pad 23 smd roundrect (at 2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 22 smd roundrect (at 1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 21 smd roundrect (at 1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 20 smd roundrect (at 0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 19 smd roundrect (at 0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 CS_MB1))
    (pad 18 smd roundrect (at -0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 CS_MB2))
    (pad 17 smd roundrect (at -0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 16 smd roundrect (at -1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 15 smd roundrect (at -1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 14 smd roundrect (at -2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 13 smd roundrect (at -2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 12 smd roundrect (at -3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 INT_SENSOR))
    (pad 11 smd roundrect (at -3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 RST_MB1))
    (pad 10 smd roundrect (at -3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 RST_MB2))
    (pad 9 smd roundrect (at -3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 8 smd roundrect (at -3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 7 smd roundrect (at -3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 6 smd roundrect (at -3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 5 smd roundrect (at -3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 4 smd roundrect (at -3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 3 smd roundrect (at -3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 2 smd roundrect (at -3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 1 smd roundrect (at -3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad "" smd roundrect (at 1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad 49 smd roundrect (at 0 0) (size 5.15 5.15) (layers F.Cu F.Mask) (roundrect_rratio 0.048544)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 164.23 89.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R603 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 200.23 59.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R603 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 202.45 68.65 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R510 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 164.05 90.75)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U502 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value BQ21040 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R506-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 ~CHG))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 165.49 93.7)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D201 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 192.55 72.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 165.685 89.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 165.585 92.7 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.95 91.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R506 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(R506-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 174.68 104.74)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C502 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 10U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 207.655 59.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R503 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 90 "/USB Input/D_N"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 199.295 58.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C509 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 190.63 60.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1007 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 INT_OPT3001))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 162.055 80.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D403 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 165.685 88.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "100 pF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 161.975 93.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R805 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 159.145 80.58)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D402 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 154.88 91.9 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C809 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 156.25 80.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D401 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 167.88 107.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R511 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 162.28 98.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 161.965 92.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R804 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.47 90.665 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1006 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 INT_LIS2DE12_2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 179.325 69.625 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C821 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C821-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.725 70.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R810 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.96 89.22 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R501 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(P501-PadB5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MX25R8035FZUIL0 (layer B.Cu) (tedit 5E42FFC6)
    (at 188.775 101.08 270)
    (fp_text reference U802 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value MX25R8035FZUIL0 (at 0 -2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 109 ~FLASH_CS))
    (pad 2 smd rect (at -1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R809-Pad2)"))
    (pad 4 smd rect (at -1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 6 smd rect (at 1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at 1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 8 smd rect (at 1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C811-Pad2)"))
    (pad 9 smd custom (at 0 0 270) (size 0.2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0 0.8) (xy 0.1 0.8) (xy 0.1 -0.8) (xy -0.1 -0.8) (xy -0.1 0.7)
) (width 0))
      ))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 188.9 80.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D404 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 198.25 95.625)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L801 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.32 94.11 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C814 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 191.6 132.925 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 186.21 88.29 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1002 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:0900PC15A0036 (layer F.Cu) (tedit 5E41EA1D)
    (at 186.14 95.44 270)
    (fp_text reference B801 (at 0.025 4.2 90) (layer F.SilkS) hide)
    (fp_text value 0900PC15A0036E (at -0.05 -3.025 90) (layer F.Fab))
    (pad 4 smd roundrect (at 0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (pad 3 smd roundrect (at 0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 6 smd roundrect (at 0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 7 smd roundrect (at 0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 8 smd roundrect (at -0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 9 smd roundrect (at -0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 5 smd roundrect (at 1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 10 smd roundrect (at -1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/0900PC15J0013.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD (layer B.Cu) (tedit 5E541D54)
    (at 192.6 95.6 90)
    (fp_text reference J702 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value mikroBUS (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at 11.43 0) (layer B.Fab))
    (fp_text user %R (at -11.43 0) (layer B.Fab))
    (pad 10 smd rect (at 13.08 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 28 5V))
    (pad 12 smd rect (at 13.08 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 44 SCL))
    (pad 14 smd rect (at 13.08 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 43 CC1352_TX_MB2_RX))
    (pad 16 smd rect (at 13.08 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 42 PWM_MB2))
    (pad 9 smd rect (at 9.78 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 9.78 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 41 SDA))
    (pad 13 smd rect (at 9.78 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 40 CC1352_RX_MB2_TX))
    (pad 15 smd rect (at 9.78 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 39 INT_MB2))
    (pad 8 smd rect (at -13.08 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -13.08 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 2 smd rect (at -13.08 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 37 RST_MB2))
    (pad 1 smd rect (at -9.78 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 36 AN_MB2))
    (pad 4 smd rect (at -13.08 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at -9.78 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 20 3V3))
    (pad 3 smd rect (at -9.78 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 34 CS_MB2))
    (pad 5 smd rect (at -9.78 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 179.38 82.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H103 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 204.63 82.575 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D501 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 210.68 74.74)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C502 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 10U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 193.525 72.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 150.725 103.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 190.63 118.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1002 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 162.28 128.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 169.755 105.55 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L501 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 157.5 97.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C810 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "22 uF" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Palconn_UTC16-G (layer F.Cu) (tedit 5CF432E0)
    (at 171.5 90.3 90)
    (descr http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf)
    (tags "USB C Type-C Receptacle USB2.0")
    (attr smd)
    (fp_text reference P501 (at 0 -4.58 90) (layer F.SilkS) hide)
    (fp_text value USB_C_Plug_USB2.0 (at 0 6.24 90) (layer F.Fab))
    (fp_text user %R (at 0 1.18 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.43 90) (layer Dwgs.User))
    (pad S1 thru_hole oval (at -4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B7 smd rect (at -0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A6 smd rect (at -0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 91 "/USB Input/D_P"))
    (pad A7 smd rect (at 0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 90 "/USB Input/D_N"))
    (pad B8 smd rect (at -1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at -1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P501-PadA5)"))
    (pad A8 smd rect (at 1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad B6 smd rect (at 0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad B5 smd rect (at 1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(P501-PadB5)"))
    (pad "" np_thru_hole circle (at 2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad A4 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B9 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A1 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B12 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B4 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B1 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A12 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/1054500101.stp
      (offset (xyz 0 -0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Package_LGA:LGA-12_2x2mm_P0.5mm (layer F.Cu) (tedit 5A0AAFFD)
    (at 152.01 88.69 180)
    (descr LGA12)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U1004 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value LIS2DE12 (at 0 1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 12 smd rect (at -0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 99 INT_LIS2DE12_2))
    (pad 6 smd rect (at 0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 1 smd rect (at -0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 7 smd rect (at 0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 8 smd rect (at 0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 3 smd rect (at -0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 2 smd rect (at -0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 157.68 95.9)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L802 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.36 88.01)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F501 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value Polyfuse (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:HDC2010 (layer F.Cu) (tedit 5E4D6772)
    (at 190.58 58.95)
    (fp_text reference U1001 (at -0.025 2.025) (layer F.SilkS) hide)
    (fp_text value HDC2010 (at 0 -3.8) (layer F.Fab))
    (pad A1 smd circle (at -0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS) (solder_mask_margin 0.05))
    (pad B1 smd circle (at -0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R1004-Pad1)") (solder_mask_margin 0.05))
    (pad C1 smd circle (at -0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad C2 smd circle (at 0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 95 INT_HDC2010) (solder_mask_margin 0.05))
    (pad B2 smd circle (at 0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL) (solder_mask_margin 0.05))
    (pad A2 smd circle (at 0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA) (solder_mask_margin 0.05))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 188.28 93.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C808 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 162.055 110.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D403 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 152.4 91.3 180)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y802 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Crystal_GND2 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U801-Pad47)"))
    (pad 2 smd rect (at 0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U801-Pad46)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.725 100.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R810 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 182.99 63.44 315)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L803 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2 nH" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer B.Cu) (tedit 5D409D35)
    (at 200.4 65.5 270)
    (attr virtual)
    (fp_text reference J501 (at 3.81 -2.413 90) (layer B.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at 2.54 2.413 90) (layer B.Fab))
    (pad 4 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 5 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 6 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 7 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 1 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 20 3V3))
    (pad 10 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 2 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 9 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 3 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 8 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 10 "/USB Input/MSP430_TDI"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.21 117.74)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1004 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(R1004-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 150.725 133.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 211.39 95.09 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C506 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 182.9 132.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference AE802 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(AE802-Pad1)"))
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer B.Cu) (tedit 5A0FD1B2)
    (at 209.805 92.475)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y501 (at 0 2.45) (layer B.SilkS) hide)
    (fp_text value 24MHz (at 0 -2.45) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 "/USB Input/XTAL1"))
    (pad 2 smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 "/USB Input/XTAL2"))
    (pad 4 smd rect (at -1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 154.88 121.9 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C809 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 190.63 120.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1007 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 INT_OPT3001))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.25 110.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R401 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 173.38 112.56)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H101 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.63 130.5 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C801 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 150.855 131.125 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C802 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 164.23 119.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R603 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 164.05 120.75)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U502 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value BQ21040 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 ~CHG))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R506-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 183.825 96.175 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C813 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 190.63 90.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1007 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 INT_OPT3001))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 211.39 125.09 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C506 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 165.685 119.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 165.585 122.7 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.95 121.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R506 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(R506-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 169.955 106.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C501 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 166.4 95.99 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R505 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 202.95 61.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R506 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(R506-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 169.255 112.75 270)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW901 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 1 smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 143.325 129.625 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C821 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C821-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 206.68 119.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R504 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 "/USB Input/D_P"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.21 87.74)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1004 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(R1004-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 160.025 95.1 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C804 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:BeagleBoard.org-20mm (layer B.Cu) (tedit 0)
    (at 179.38 65.3 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 203.14 63.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F801 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value Polyfuse (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 193.5 127.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C810 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "22 uF" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.055 110.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D403 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 152.28 93.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C808 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 202.44 130.55 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R509 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 174.68 134.74)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C502 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 10U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 159.14 110.57)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R402 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 210.68 104.74)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C502 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 10U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:X2SON-8_1.4x1mm_P0.35mm (layer B.Cu) (tedit 5A02F1D8)
    (at 152.63 89.85 180)
    (descr "X2SON-8 1.4x1mm Pitch0.35mm http://www.ti.com/lit/ds/symlink/pca9306.pdf")
    (tags "X2SON-8 1.4x1mm Pitch0.35mm")
    (attr smd)
    (fp_text reference U1002 (at 0 2) (layer B.SilkS) hide)
    (fp_text value SN74AUP2G32 (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 8 smd rect (at 0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 19 VDDS))
    (pad 7 smd rect (at 0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 6 smd rect (at 0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 5 smd rect (at 0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 94 INT_SENSOR))
    (pad 2 smd rect (at -0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd rect (at -0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 95 INT_HDC2010))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 146.9 102.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference AE802 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(AE802-Pad1)"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 151.39 87.76 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1005 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(R1005-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:RFECA3216060A1T (layer F.Cu) (tedit 5E42DF6C)
    (at 142.28 124 270)
    (fp_text reference AE801 (at 0 1.85 90) (layer F.SilkS) hide)
    (fp_text value Antenna_Dipole (at 0.05 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at 1.4 -0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AE801-Pad1)"))
    (pad 2 smd rect (at 1.4 0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.4 0 270) (size 0.35 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(AE801-Pad3)"))
    (model ${KIPRJMOD}/mech/2450AT18D0100.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 173.38 107.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H102 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 199.295 88.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C509 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 170.68 119.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R504 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 "/USB Input/D_P"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 193.68 65.9)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L802 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MX25R8035FZUIL0 (layer B.Cu) (tedit 5E42FFC6)
    (at 188.775 71.08 270)
    (fp_text reference U802 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value MX25R8035FZUIL0 (at 0 -2 90) (layer B.Fab))
    (pad 9 smd custom (at 0 0 270) (size 0.2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0 0.8) (xy 0.1 0.8) (xy 0.1 -0.8) (xy -0.1 -0.8) (xy -0.1 0.7)
) (width 0))
      ))
    (pad 8 smd rect (at 1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C811-Pad2)"))
    (pad 7 smd rect (at 1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 6 smd rect (at 1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 5 smd rect (at 1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 4 smd rect (at -1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R809-Pad2)"))
    (pad 2 smd rect (at -1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 1 smd rect (at -1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 109 ~FLASH_CS))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.65 124.12 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C819 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(AE801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 188.9 50.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D404 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 166.44 132.43 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C503 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:BeagleBoard.org-20mm (layer B.Cu) (tedit 0)
    (at 143.38 125.3 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 208.82 134.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C505 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0.47U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 202.95 62.05 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R502 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(P501-PadA5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 202.36 58.01)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F501 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value Polyfuse (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 151.39 117.76 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1005 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 150.21 118.29 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1002 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:USON6 (layer B.Cu) (tedit 5E4DAB76)
    (at 193.16 91.09 180)
    (fp_text reference U1003 (at 0.11 -3.68) (layer B.SilkS) hide)
    (fp_text value OPT3001 (at -0.16 3.7) (layer B.Fab))
    (pad 1 smd roundrect (at -0.95 0.675 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 19 VDDS) (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 101 "Net-(R1008-Pad2)") (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at 0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 44 SCL) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at 0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 100 INT_OPT3001) (solder_mask_margin 0.07))
    (pad 6 smd roundrect (at 0.95 0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 41 SDA) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 0 0 180) (size 0.65 1.35) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 -0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 201.685 89.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 146.99 93.44 315)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L803 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2 nH" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 150.725 101.525)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 173.905 118.875 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference D502 (at 0 2.9 270) (layer B.SilkS) hide)
    (fp_text value TPD2E001 (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 90 "/USB Input/D_N"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 91 "/USB Input/D_P"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 79 "/USB Input/VBUS"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 145.2 127.3 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L804 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 163.295 118.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C509 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 188.805 102.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C806 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LGA:LGA-12_2x2mm_P0.5mm (layer F.Cu) (tedit 5A0AAFFD)
    (at 188.01 118.69 180)
    (descr LGA12)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U1004 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value LIS2DE12 (at 0 1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 12 smd rect (at -0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 99 INT_LIS2DE12_2))
    (pad 6 smd rect (at 0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 1 smd rect (at -0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 7 smd rect (at 0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 8 smd rect (at 0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 3 smd rect (at -0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 2 smd rect (at -0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 154.63 88.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1002 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 187.23 89.33 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1003 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(R1003-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 150.725 130.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R810 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 191.6 102.925 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 150.725 102.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 170.68 89.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R504 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 "/USB Input/D_P"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.65 94.12 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C819 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(AE801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 189.28 87.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1001 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 150.725 129.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R809 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R809-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 166.45 98.65 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R510 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 154.63 120.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1007 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 INT_OPT3001))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer F.Cu) (tedit 5E4C72AA)
    (at 200.4 125.5 270)
    (attr virtual)
    (fp_text reference J301 (at 0.302285 2.603303 270) (layer F.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at -0.967715 -2.222697 270) (layer F.Fab))
    (pad 4 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 32 CC1352_TCK))
    (pad 5 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 31 CC1352_TDO))
    (pad 7 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 1 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 20 3V3))
    (pad 10 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 17 RESET_N))
    (pad 2 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 30 CC1352_TMS))
    (pad 9 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 3 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 8 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 29 CC1352_TDI))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 150.725 100.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R810 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD locked (layer F.Cu) (tedit 5E541D62)
    (at 192.68 95.6 90)
    (fp_text reference J701 (at -0.074182 -1.275144 90) (layer F.SilkS) hide)
    (fp_text value mikroBUS (at -0.074182 -0.005144 90) (layer F.Fab))
    (fp_text user %R (at 11.355818 -0.005144 180) (layer F.Fab) hide)
    (fp_text user %R (at 11.43 0 180) (layer F.Fab))
    (pad 5 smd rect (at -9.78 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -9.78 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 51 CS_MB1))
    (pad 7 smd rect (at -9.78 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 20 3V3))
    (pad 4 smd rect (at -13.08 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 35 SCK))
    (pad 1 smd rect (at -9.78 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 50 AN_MB1))
    (pad 2 smd rect (at -13.08 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 49 RST_MB1))
    (pad 6 smd rect (at -13.08 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 38 MOSI))
    (pad 8 smd rect (at -13.08 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 9.78 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 48 INT_MB1))
    (pad 13 smd rect (at 9.78 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 47 CC1352_RX_MB1_TX))
    (pad 11 smd rect (at 9.78 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 9 smd rect (at 9.78 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 13.08 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM_MB1))
    (pad 14 smd rect (at 13.08 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 45 CC1352_TX_MB1_RX))
    (pad 12 smd rect (at 13.08 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 13.08 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 154.63 90.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1007 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 INT_OPT3001))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 198.96 118.76 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C603 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value "10 uF" (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 203.535 122.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(R601-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 175.39 125.09 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C506 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 166.97 120.16 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C508 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 182.99 123.44 315)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L803 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2 nH" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 191.58 118.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1001 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 150.725 131.525)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 201.12 80.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R406 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 ~CHG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 201.49 123.7)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D201 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 154.63 118.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1002 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 194.38 102.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C805 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 157.525 132.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 192.25 50.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D401 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:HDC2010 (layer F.Cu) (tedit 5E4D6772)
    (at 190.58 118.95)
    (fp_text reference U1001 (at -0.025 2.025) (layer F.SilkS) hide)
    (fp_text value HDC2010 (at 0 -3.8) (layer F.Fab))
    (pad A1 smd circle (at -0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS) (solder_mask_margin 0.05))
    (pad B1 smd circle (at -0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R1004-Pad1)") (solder_mask_margin 0.05))
    (pad C1 smd circle (at -0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad C2 smd circle (at 0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 95 INT_HDC2010) (solder_mask_margin 0.05))
    (pad B2 smd circle (at 0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL) (solder_mask_margin 0.05))
    (pad A2 smd circle (at 0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA) (solder_mask_margin 0.05))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 190.88 91.9 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C809 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 180.88 91.4 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C818 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C818-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 192.48 123 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 189.28 117.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1001 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 209.905 88.875 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference D502 (at 0 2.9 270) (layer B.SilkS) hide)
    (fp_text value TPD2E001 (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 90 "/USB Input/D_N"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 91 "/USB Input/D_P"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 79 "/USB Input/VBUS"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 175.39 95.09 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C506 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N48_EP5.15x5.15mm (layer B.Cu) (tedit 5E4C745D)
    (at 207.05 70.15 180)
    (descr "QFN, 48 Pin (http://www.ti.com/lit/ds/symlink/msp430f5232.pdf#page=112), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U501 (at 0 4.82) (layer B.SilkS) hide)
    (fp_text value MSP430F5500IRGZ (at 0 -4.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 48 smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 47 smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 46 smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 45 smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 44 smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 43 smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 42 smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 41 smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 40 smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 39 smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 38 smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 37 smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 36 smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 35 smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 34 smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 33 smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 32 smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 31 smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 30 smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 29 smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 28 smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 27 smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 26 smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 25 smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 24 smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 23 smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 22 smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 21 smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 20 smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 19 smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 18 smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 17 smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 16 smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 15 smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 14 smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 12 smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 10 smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 6 smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad 49 smd roundrect (at 0 0 180) (size 5.15 5.15) (layers B.Cu B.Mask) (roundrect_rratio 0.049)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N48_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 192.48 93 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 179.38 52.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H103 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 146.9 132.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference AE802 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(AE802-Pad1)"))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 166.97 90.16 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C508 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 193.68 95.9)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L802 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 203.14 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F801 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value Polyfuse (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 185.755 99.575 315)
    (descr "SMD Crystal 2012/2 http://txccrystal.com/images/pdf/9ht11.pdf, 2.0x1.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y801 (at 0 -1.8 135) (layer F.SilkS) hide)
    (fp_text value Crystal (at 0 1.8 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C801-Pad1)"))
    (pad 2 smd rect (at 0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_AX_8045-2Pin_8.0x4.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.25 0.3 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 209.38 137.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H102 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 150.725 99.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R809 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R809-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 194.475 132.95 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.14 123.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F801 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value Polyfuse (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 198.96 58.76 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C603 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value "10 uF" (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 196.43 58.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R802 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 CC1352_TX_MB2_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 181.25 99.375 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C820 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(AE802-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 195.145 110.58)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D402 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 188.805 132.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C806 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 181.2 97.3 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L804 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 207.08 100.2 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J201 (at 0 -5.8 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.95 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (pad 2 smd roundrect (at 1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad MP smd roundrect (at -3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at 3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.step
      (offset (xyz -1 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 188.4 61.3 180)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y802 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Crystal_GND2 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U801-Pad47)"))
    (pad 2 smd rect (at 0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U801-Pad46)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 190.88 61.9 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C809 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 195.145 50.58)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D402 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 203.505 58.3 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R604 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 201.13 80.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D406 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 193.68 125.9)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L802 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 203.505 118.3 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R604 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 188.9 110.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R404 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 193.5 97.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C810 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "22 uF" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 205.98 137.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R507 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 208.82 74.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C505 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0.47U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 185.755 129.575 315)
    (descr "SMD Crystal 2012/2 http://txccrystal.com/images/pdf/9ht11.pdf, 2.0x1.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y801 (at 0 -1.8 135) (layer F.SilkS) hide)
    (fp_text value Crystal (at 0 1.8 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C802-Pad1)"))
    (pad 1 smd rect (at -0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C801-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_AX_8045-2Pin_8.0x4.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.25 0.3 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 207.17 63.035 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C507 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 205.255 82.75 270)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW901 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 1 smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 159.68 121.11 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1008 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(R1008-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 202.96 119.22 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R501 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(P501-PadB5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 157.525 102.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 166.44 102.43 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C503 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 209 65.57 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C504 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 220N (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 197.965 62.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R804 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.055 80.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D403 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 205.98 107.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R507 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 195.14 80.57)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R402 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:X2SON-8_1.4x1mm_P0.35mm (layer B.Cu) (tedit 5A02F1D8)
    (at 188.63 119.85 180)
    (descr "X2SON-8 1.4x1mm Pitch0.35mm http://www.ti.com/lit/ds/symlink/pca9306.pdf")
    (tags "X2SON-8 1.4x1mm Pitch0.35mm")
    (attr smd)
    (fp_text reference U1002 (at 0 2) (layer B.SilkS) hide)
    (fp_text value SN74AUP2G32 (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 8 smd rect (at 0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 19 VDDS))
    (pad 7 smd rect (at 0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 6 smd rect (at 0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 5 smd rect (at 0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 94 INT_SENSOR))
    (pad 2 smd rect (at -0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd rect (at -0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 95 INT_HDC2010))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 150.725 132.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:USON6 (layer B.Cu) (tedit 5E4DAB76)
    (at 193.16 121.09 180)
    (fp_text reference U1003 (at 0.11 -3.68) (layer B.SilkS) hide)
    (fp_text value OPT3001 (at -0.16 3.7) (layer B.Fab))
    (pad 7 thru_hole circle (at 0 -0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 smd rect (at 0 0 180) (size 0.65 1.35) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.02))
    (pad 6 smd roundrect (at 0.95 0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 41 SDA) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at 0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 100 INT_OPT3001) (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at 0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 44 SCL) (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 101 "Net-(R1008-Pad2)") (solder_mask_margin 0.07))
    (pad 1 smd roundrect (at -0.95 0.675 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 19 VDDS) (solder_mask_margin 0.07))
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 179.48 87.8 270)
    (fp_text reference J801 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 4 smd rect (at 0 1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C818-Pad2)"))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 151.23 89.33 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1003 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(R1003-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 186.47 60.665 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1006 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 INT_LIS2DE12_2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 181.25 129.375 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C820 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(AE802-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 186.47 90.665 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1006 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 INT_LIS2DE12_2))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 205.98 77.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R507 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 203.88 137.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R511 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 205.955 136.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C501 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 192.25 110.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D401 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 149.62 97.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C812 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer B.Cu) (tedit 5A0FD1B2)
    (at 209.805 122.475)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y501 (at 0 2.45) (layer B.SilkS) hide)
    (fp_text value 24MHz (at 0 -2.45) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 4 smd rect (at -1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 "/USB Input/XTAL2"))
    (pad 2 smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 "/USB Input/XTAL1"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:X2SON-8_1.4x1mm_P0.35mm (layer B.Cu) (tedit 5A02F1D8)
    (at 152.63 119.85 180)
    (descr "X2SON-8 1.4x1mm Pitch0.35mm http://www.ti.com/lit/ds/symlink/pca9306.pdf")
    (tags "X2SON-8 1.4x1mm Pitch0.35mm")
    (attr smd)
    (fp_text reference U1002 (at 0 2) (layer B.SilkS) hide)
    (fp_text value SN74AUP2G32 (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 95 INT_HDC2010))
    (pad 2 smd rect (at -0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 3 smd rect (at -0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 94 INT_SENSOR))
    (pad 4 smd rect (at -0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 7 smd rect (at 0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 8 smd rect (at 0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD locked (layer F.Cu) (tedit 5E541D62)
    (at 156.68 95.6 90)
    (fp_text reference J701 (at -0.074182 -1.275144 90) (layer F.SilkS) hide)
    (fp_text value mikroBUS (at -0.074182 -0.005144 90) (layer F.Fab))
    (fp_text user %R (at 11.43 0 180) (layer F.Fab))
    (fp_text user %R (at 11.355818 -0.005144 180) (layer F.Fab) hide)
    (pad 10 smd rect (at 13.08 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 12 smd rect (at 13.08 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 14 smd rect (at 13.08 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 45 CC1352_TX_MB1_RX))
    (pad 16 smd rect (at 13.08 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM_MB1))
    (pad 9 smd rect (at 9.78 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 9.78 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 13 smd rect (at 9.78 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 47 CC1352_RX_MB1_TX))
    (pad 15 smd rect (at 9.78 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 48 INT_MB1))
    (pad 8 smd rect (at -13.08 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -13.08 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 38 MOSI))
    (pad 2 smd rect (at -13.08 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 49 RST_MB1))
    (pad 1 smd rect (at -9.78 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 50 AN_MB1))
    (pad 4 smd rect (at -13.08 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at -9.78 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 20 3V3))
    (pad 3 smd rect (at -9.78 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 51 CS_MB1))
    (pad 5 smd rect (at -9.78 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 33 MISO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 179.325 99.625 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C821 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C821-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 207.655 89.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R503 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 90 "/USB Input/D_N"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:BeagleBoard.org-20mm (layer B.Cu) (tedit 0)
    (at 179.38 95.3 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 202.44 70.55 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R509 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 197.965 122.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R804 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 194.05 58.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R803 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 CC1352_RX_MB2_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 203.88 77.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R511 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 200.23 89.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R603 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 187.23 119.33 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1003 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(R1003-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.14 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F801 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value Polyfuse (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 186.725 103.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 173.38 137.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H102 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module leash:MikroBus-SMD locked (layer F.Cu) (tedit 5E541D62)
    (at 156.68 125.6 90)
    (fp_text reference J701 (at -0.074182 -1.275144 90) (layer F.SilkS) hide)
    (fp_text value mikroBUS (at -0.074182 -0.005144 90) (layer F.Fab))
    (fp_text user %R (at 11.355818 -0.005144 180) (layer F.Fab) hide)
    (fp_text user %R (at 11.43 0 180) (layer F.Fab))
    (pad 5 smd rect (at -9.78 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -9.78 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 51 CS_MB1))
    (pad 7 smd rect (at -9.78 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 20 3V3))
    (pad 4 smd rect (at -13.08 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 35 SCK))
    (pad 1 smd rect (at -9.78 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 50 AN_MB1))
    (pad 2 smd rect (at -13.08 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 49 RST_MB1))
    (pad 6 smd rect (at -13.08 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 38 MOSI))
    (pad 8 smd rect (at -13.08 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 9.78 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 48 INT_MB1))
    (pad 13 smd rect (at 9.78 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 47 CC1352_RX_MB1_TX))
    (pad 11 smd rect (at 9.78 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 9 smd rect (at 9.78 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 13.08 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM_MB1))
    (pad 14 smd rect (at 13.08 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 45 CC1352_TX_MB1_RX))
    (pad 12 smd rect (at 13.08 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 13.08 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD (layer B.Cu) (tedit 5E541D54)
    (at 192.6 65.6 90)
    (fp_text reference J702 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value mikroBUS (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at -11.43 0) (layer B.Fab))
    (fp_text user %R (at 11.43 0) (layer B.Fab))
    (pad 5 smd rect (at -9.78 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -9.78 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 34 CS_MB2))
    (pad 7 smd rect (at -9.78 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 20 3V3))
    (pad 4 smd rect (at -13.08 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 1 smd rect (at -9.78 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 36 AN_MB2))
    (pad 2 smd rect (at -13.08 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 37 RST_MB2))
    (pad 6 smd rect (at -13.08 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 8 smd rect (at -13.08 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 9.78 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 39 INT_MB2))
    (pad 13 smd rect (at 9.78 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 40 CC1352_RX_MB2_TX))
    (pad 11 smd rect (at 9.78 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 41 SDA))
    (pad 9 smd rect (at 9.78 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 13.08 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 42 PWM_MB2))
    (pad 14 smd rect (at 13.08 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 43 CC1352_TX_MB2_RX))
    (pad 12 smd rect (at 13.08 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 13.08 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Palconn_UTC16-G (layer F.Cu) (tedit 5CF432E0)
    (at 207.5 60.3 90)
    (descr http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf)
    (tags "USB C Type-C Receptacle USB2.0")
    (attr smd)
    (fp_text reference P501 (at 0 -4.58 90) (layer F.SilkS) hide)
    (fp_text value USB_C_Plug_USB2.0 (at 0 6.24 90) (layer F.Fab))
    (fp_text user %R (at 0 1.18 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.43 90) (layer Dwgs.User))
    (pad S1 thru_hole oval (at -4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B7 smd rect (at -0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A6 smd rect (at -0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 91 "/USB Input/D_P"))
    (pad A7 smd rect (at 0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 90 "/USB Input/D_N"))
    (pad B8 smd rect (at -1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at -1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P501-PadA5)"))
    (pad A8 smd rect (at 1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad B6 smd rect (at 0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad B5 smd rect (at 1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(P501-PadB5)"))
    (pad "" np_thru_hole circle (at 2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad A4 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B9 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A1 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B12 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B4 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B1 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A12 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/1054500101.stp
      (offset (xyz 0 -0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 202.4 125.99 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R505 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:TPS62821DLC (layer B.Cu) (tedit 5D2676FA)
    (at 202.885 91.1)
    (fp_text reference U601 (at 0.1 1.975 180) (layer B.SilkS) hide)
    (fp_text value TPS62821DLC (at 0 0.5 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 2 smd roundrect (at -0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(C602-Pad2)"))
    (pad 3 smd roundrect (at -0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 4 smd roundrect (at -0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2))
    (pad 5 smd roundrect (at 0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 6 smd roundrect (at 0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 73 "Net-(L601-Pad1)"))
    (pad 7 smd roundrect (at 0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 8 smd roundrect (at 0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 74 "Net-(R601-Pad1)"))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1.3 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:RFECA3216060A1T (layer F.Cu) (tedit 5E42DF6C)
    (at 178.28 94 270)
    (fp_text reference AE801 (at 0 1.85 90) (layer F.SilkS) hide)
    (fp_text value Antenna_Dipole (at 0.05 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at 1.4 -0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AE801-Pad1)"))
    (pad 2 smd rect (at 1.4 0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.4 0 270) (size 0.35 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(AE801-Pad3)"))
    (model ${KIPRJMOD}/mech/2450AT18D0100.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 203.505 88.3 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R604 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.28 128.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 180.88 61.4 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C818 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C818-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 153.28 87.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1001 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 205.755 105.55 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L501 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 202.96 89.22 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R501 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(P501-PadB5)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm (layer F.Cu) (tedit 5C26A111)
    (at 192.13 97.44)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U801 (at 0 -4.82) (layer F.SilkS) hide)
    (fp_text value CC1352R (at 0 4.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 49 smd roundrect (at 0 0) (size 5.15 5.15) (layers F.Cu F.Mask) (roundrect_rratio 0.048544)
      (net 1 GND))
    (pad "" smd roundrect (at -1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad 1 smd roundrect (at -3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 2 smd roundrect (at -3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 3 smd roundrect (at -3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 4 smd roundrect (at -3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 5 smd roundrect (at -3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 6 smd roundrect (at -3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 7 smd roundrect (at -3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 8 smd roundrect (at -3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 9 smd roundrect (at -3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 10 smd roundrect (at -3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 RST_MB2))
    (pad 11 smd roundrect (at -3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 RST_MB1))
    (pad 12 smd roundrect (at -3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 INT_SENSOR))
    (pad 13 smd roundrect (at -2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 14 smd roundrect (at -2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 15 smd roundrect (at -1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 16 smd roundrect (at -1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 17 smd roundrect (at -0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 18 smd roundrect (at -0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 CS_MB2))
    (pad 19 smd roundrect (at 0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 CS_MB1))
    (pad 20 smd roundrect (at 0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 21 smd roundrect (at 1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 22 smd roundrect (at 1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 23 smd roundrect (at 2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 24 smd roundrect (at 2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 CC1352_TMS))
    (pad 25 smd roundrect (at 3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 CC1352_TCK))
    (pad 26 smd roundrect (at 3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 CC1352_TDO))
    (pad 27 smd roundrect (at 3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 CC1352_TDI))
    (pad 28 smd roundrect (at 3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 29 smd roundrect (at 3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 PWM_MB2))
    (pad 30 smd roundrect (at 3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 INT_MB2))
    (pad 31 smd roundrect (at 3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 32 smd roundrect (at 3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 33 smd roundrect (at 3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 34 smd roundrect (at 3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 35 smd roundrect (at 3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 36 smd roundrect (at 3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 AN_MB1))
    (pad 37 smd roundrect (at 2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 AN_MB2))
    (pad 38 smd roundrect (at 2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 39 smd roundrect (at 1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 40 smd roundrect (at 1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 41 smd roundrect (at 0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 42 smd roundrect (at 0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 INT_MB1))
    (pad 43 smd roundrect (at -0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 PWM_MB1))
    (pad 44 smd roundrect (at -0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 45 smd roundrect (at -1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 46 smd roundrect (at -1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U801-Pad46)"))
    (pad 47 smd roundrect (at -2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U801-Pad47)"))
    (pad 48 smd roundrect (at -2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 202.44 72.43 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C503 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:BeagleBoard.org-20mm (layer B.Cu) (tedit 0)
    (at 143.38 95.3 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 202.4 65.99 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R505 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 179.48 57.8 270)
    (fp_text reference J801 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 1 smd rect (at 1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C818-Pad2)"))
    (pad 2 smd rect (at 0 -1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 153.28 117.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1001 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 202.45 128.65 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R510 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:USON6 (layer B.Cu) (tedit 5E4DAB76)
    (at 157.16 91.09 180)
    (fp_text reference U1003 (at 0.11 -3.68) (layer B.SilkS) hide)
    (fp_text value OPT3001 (at -0.16 3.7) (layer B.Fab))
    (pad 7 thru_hole circle (at 0 -0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 smd rect (at 0 0 180) (size 0.65 1.35) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.02))
    (pad 6 smd roundrect (at 0.95 0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 41 SDA) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at 0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 100 INT_OPT3001) (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at 0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 44 SCL) (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 101 "Net-(R1008-Pad2)") (solder_mask_margin 0.07))
    (pad 1 smd roundrect (at -0.95 0.675 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 19 VDDS) (solder_mask_margin 0.07))
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 173.905 88.875 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference D502 (at 0 2.9 270) (layer B.SilkS) hide)
    (fp_text value TPD2E001 (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 91 "/USB Input/D_P"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 90 "/USB Input/D_N"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 179.85 97.95 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C817 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "5.6 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 197.975 63.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R805 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 183.825 66.175 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C813 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer F.Cu) (tedit 5E4C72AA)
    (at 164.4 125.5 270)
    (attr virtual)
    (fp_text reference J301 (at 0.302285 2.603303 270) (layer F.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at -0.967715 -2.222697 270) (layer F.Fab))
    (pad 8 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 29 CC1352_TDI))
    (pad 3 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 9 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 30 CC1352_TMS))
    (pad 10 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 17 RESET_N))
    (pad 1 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 20 3V3))
    (pad 7 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 6 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 31 CC1352_TDO))
    (pad 5 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 32 CC1352_TCK))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 195.38 102.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C803 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 209 95.57 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C504 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 220N (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 179.25 102.85 90)
    (fp_text reference J802 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 4 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C821-Pad2)"))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 179.38 137.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H104 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 146.99 123.44 315)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L803 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2 nH" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 179.25 72.85 90)
    (fp_text reference J802 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C821-Pad2)"))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 178.28 61.315 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C822 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(AE801-Pad3)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 204.63 52.575 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D501 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.95 92.05 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R502 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(P501-PadA5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 203.84 125.49 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R508 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1.5K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 201.49 63.7)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D201 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer B.Cu) (tedit 5D409D35)
    (at 200.4 125.5 270)
    (attr virtual)
    (fp_text reference J501 (at 3.81 -2.413 90) (layer B.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at 2.54 2.413 90) (layer B.Fab))
    (pad 4 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 5 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 6 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 7 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 1 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 20 3V3))
    (pad 10 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 2 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 9 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 3 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 8 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 10 "/USB Input/MSP430_TDI"))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 201.585 92.7 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer B.Cu) (tedit 5A0FD1B2)
    (at 173.805 122.475)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y501 (at 0 2.45) (layer B.SilkS) hide)
    (fp_text value 24MHz (at 0 -2.45) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 "/USB Input/XTAL1"))
    (pad 2 smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 "/USB Input/XTAL2"))
    (pad 4 smd rect (at -1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:TPS62821DLC (layer B.Cu) (tedit 5D2676FA)
    (at 202.885 61.1)
    (fp_text reference U601 (at 0.1 1.975 180) (layer B.SilkS) hide)
    (fp_text value TPS62821DLC (at 0 0.5 180) (layer B.Fab))
    (pad 8 smd roundrect (at 0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 74 "Net-(R601-Pad1)"))
    (pad 7 smd roundrect (at 0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 6 smd roundrect (at 0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 73 "Net-(L601-Pad1)"))
    (pad 5 smd roundrect (at 0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 4 smd roundrect (at -0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2))
    (pad 3 smd roundrect (at -0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1.3 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 143.325 99.625 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C821 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C821-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 203.84 95.49 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R508 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1.5K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 186.855 101.125 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C802 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 186.47 120.665 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1006 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 INT_LIS2DE12_2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 185.755 69.575 315)
    (descr "SMD Crystal 2012/2 http://txccrystal.com/images/pdf/9ht11.pdf, 2.0x1.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y801 (at 0 -1.8 135) (layer F.SilkS) hide)
    (fp_text value Crystal (at 0 1.8 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C802-Pad1)"))
    (pad 1 smd rect (at -0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C801-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_AX_8045-2Pin_8.0x4.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.25 0.3 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MX25R8035FZUIL0 (layer B.Cu) (tedit 5E42FFC6)
    (at 188.775 131.08 270)
    (fp_text reference U802 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value MX25R8035FZUIL0 (at 0 -2 90) (layer B.Fab))
    (pad 9 smd custom (at 0 0 270) (size 0.2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0 0.8) (xy 0.1 0.8) (xy 0.1 -0.8) (xy -0.1 -0.8) (xy -0.1 0.7)
) (width 0))
      ))
    (pad 8 smd rect (at 1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C811-Pad2)"))
    (pad 7 smd rect (at 1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 6 smd rect (at 1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 5 smd rect (at 1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 4 smd rect (at -1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R809-Pad2)"))
    (pad 2 smd rect (at -1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 1 smd rect (at -1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 109 ~FLASH_CS))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LGA:LGA-12_2x2mm_P0.5mm (layer F.Cu) (tedit 5A0AAFFD)
    (at 188.01 58.69 180)
    (descr LGA12)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U1004 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value LIS2DE12 (at 0 1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 12 smd rect (at -0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 99 INT_LIS2DE12_2))
    (pad 6 smd rect (at 0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 1 smd rect (at -0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 7 smd rect (at 0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 8 smd rect (at 0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 3 smd rect (at -0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 2 smd rect (at -0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 188.9 80.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R404 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.28 68.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 179.38 107.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H104 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module leash:0900PC15A0036 (layer F.Cu) (tedit 5E41EA1D)
    (at 186.14 65.44 270)
    (fp_text reference B801 (at 0.025 4.2 90) (layer F.SilkS) hide)
    (fp_text value 0900PC15A0036E (at -0.05 -3.025 90) (layer F.Fab))
    (pad 10 smd roundrect (at -1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 smd roundrect (at 1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 9 smd roundrect (at -0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 8 smd roundrect (at -0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 7 smd roundrect (at 0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 6 smd roundrect (at 0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 1 smd roundrect (at -0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 2 smd roundrect (at -0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at 0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at 0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (model ${KIPRJMOD}/mech/0900PC15J0013.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 197.975 123.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R805 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 183.825 126.175 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C813 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm (layer F.Cu) (tedit 5C26A111)
    (at 192.13 127.44)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U801 (at 0 -4.82) (layer F.SilkS) hide)
    (fp_text value CC1352R (at 0 4.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 48 smd roundrect (at -2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 47 smd roundrect (at -2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U801-Pad47)"))
    (pad 46 smd roundrect (at -1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U801-Pad46)"))
    (pad 45 smd roundrect (at -1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 44 smd roundrect (at -0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 43 smd roundrect (at -0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 PWM_MB1))
    (pad 42 smd roundrect (at 0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 INT_MB1))
    (pad 41 smd roundrect (at 0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 40 smd roundrect (at 1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 39 smd roundrect (at 1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 38 smd roundrect (at 2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 37 smd roundrect (at 2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 AN_MB2))
    (pad 36 smd roundrect (at 3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 AN_MB1))
    (pad 35 smd roundrect (at 3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 34 smd roundrect (at 3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 33 smd roundrect (at 3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 32 smd roundrect (at 3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 31 smd roundrect (at 3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 30 smd roundrect (at 3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 INT_MB2))
    (pad 29 smd roundrect (at 3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 PWM_MB2))
    (pad 28 smd roundrect (at 3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 27 smd roundrect (at 3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 CC1352_TDI))
    (pad 26 smd roundrect (at 3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 CC1352_TDO))
    (pad 25 smd roundrect (at 3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 CC1352_TCK))
    (pad 24 smd roundrect (at 2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 CC1352_TMS))
    (pad 23 smd roundrect (at 2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 22 smd roundrect (at 1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 21 smd roundrect (at 1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 20 smd roundrect (at 0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 19 smd roundrect (at 0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 CS_MB1))
    (pad 18 smd roundrect (at -0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 CS_MB2))
    (pad 17 smd roundrect (at -0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 16 smd roundrect (at -1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 15 smd roundrect (at -1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 14 smd roundrect (at -2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 13 smd roundrect (at -2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 12 smd roundrect (at -3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 INT_SENSOR))
    (pad 11 smd roundrect (at -3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 RST_MB1))
    (pad 10 smd roundrect (at -3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 RST_MB2))
    (pad 9 smd roundrect (at -3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 8 smd roundrect (at -3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 7 smd roundrect (at -3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 6 smd roundrect (at -3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 5 smd roundrect (at -3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 4 smd roundrect (at -3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 3 smd roundrect (at -3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 2 smd roundrect (at -3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 1 smd roundrect (at -3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad "" smd roundrect (at 1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad 49 smd roundrect (at 0 0) (size 5.15 5.15) (layers F.Cu F.Mask) (roundrect_rratio 0.048544)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 201.12 110.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R406 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 ~CHG))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 201.685 88.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "100 pF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:USON6 (layer B.Cu) (tedit 5E4DAB76)
    (at 157.16 121.09 180)
    (fp_text reference U1003 (at 0.11 -3.68) (layer B.SilkS) hide)
    (fp_text value OPT3001 (at -0.16 3.7) (layer B.Fab))
    (pad 1 smd roundrect (at -0.95 0.675 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 19 VDDS) (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 101 "Net-(R1008-Pad2)") (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at 0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 44 SCL) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at 0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 100 INT_OPT3001) (solder_mask_margin 0.07))
    (pad 6 smd roundrect (at 0.95 0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 41 SDA) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 0 0 180) (size 0.65 1.35) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 -0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 185.62 127.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C812 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 185.41 80.6)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D405 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 207.655 119.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R503 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 90 "/USB Input/D_N"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 205.755 135.55 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L501 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 198.25 65.625)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L801 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 192.25 80.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D401 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 194.05 88.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R803 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 CC1352_RX_MB2_TX))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 179.85 127.95 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C817 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "5.6 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 163.295 88.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C509 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 180.88 121.4 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C818 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C818-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 150.21 88.29 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1002 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 202.36 118.01)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F501 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value Polyfuse (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 198.96 88.76 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C603 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value "10 uF" (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 149.62 67.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C812 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 175.39 65.09 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C506 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 170.68 59.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R504 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 "/USB Input/D_P"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 150.725 72.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 150.725 70.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R810 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 150.725 69.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R809 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R809-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 150.725 71.525)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 146.99 63.44 315)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L803 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2 nH" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 143.85 67.95 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C817 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "5.6 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.875 65.925 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C815 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2.7 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 146.3 62.1 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C816 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.21 57.74)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1004 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(R1004-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 166.4 65.99 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R505 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 171.08 70.2 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J201 (at 0 -5.8 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.95 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (pad 2 smd roundrect (at 1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad MP smd roundrect (at -3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at 3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.step
      (offset (xyz -1 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 151.39 57.76 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1005 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 158.38 72.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C805 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 155.58 58.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1001 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 201.13 110.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D406 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 179.48 117.8 270)
    (fp_text reference J801 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 1 smd rect (at 1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C818-Pad2)"))
    (pad 2 smd rect (at 0 -1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.32 64.11 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C814 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer B.Cu) (tedit 5A0FD1B2)
    (at 173.805 92.475)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y501 (at 0 2.45) (layer B.SilkS) hide)
    (fp_text value 24MHz (at 0 -2.45) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 4 smd rect (at -1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 "/USB Input/XTAL2"))
    (pad 2 smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 "/USB Input/XTAL1"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 181.875 125.925 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C815 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2.7 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 196.43 118.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R802 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 CC1352_TX_MB2_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 166.44 70.55 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R509 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 171.17 63.035 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C507 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 147.825 66.175 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C813 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.25 69.375 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C820 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(AE802-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.805 72.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C806 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 169.955 76.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C501 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 155.6 72.925 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 174.68 74.74)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C502 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 10U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.96 59.22 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R501 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(P501-PadB5)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 158.475 72.95 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer B.Cu) (tedit 5D409D35)
    (at 164.4 65.5 270)
    (attr virtual)
    (fp_text reference J501 (at 3.81 -2.413 90) (layer B.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at 2.54 2.413 90) (layer B.Fab))
    (pad 8 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 3 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 9 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 2 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 10 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 1 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 20 3V3))
    (pad "" np_thru_hole circle (at 7.62 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 7 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 6 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 5 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 4 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 "/USB Input/MSP430_TCK"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 151.23 59.33 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1003 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(R1003-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 154.63 58.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1002 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.14 63.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F801 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value Polyfuse (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 153.28 57.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1001 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:BeagleBoard.org-20mm (layer B.Cu) (tedit 0)
    (at 143.38 65.3 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module leash:HDC2010 (layer F.Cu) (tedit 5E4D6772)
    (at 154.58 58.95)
    (fp_text reference U1001 (at -0.025 2.025) (layer F.SilkS) hide)
    (fp_text value HDC2010 (at 0 -3.8) (layer F.Fab))
    (pad A2 smd circle (at 0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA) (solder_mask_margin 0.05))
    (pad B2 smd circle (at 0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL) (solder_mask_margin 0.05))
    (pad C2 smd circle (at 0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 95 INT_HDC2010) (solder_mask_margin 0.05))
    (pad C1 smd circle (at -0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad B1 smd circle (at -0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R1004-Pad1)") (solder_mask_margin 0.05))
    (pad A1 smd circle (at -0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS) (solder_mask_margin 0.05))
  )
  (module leash:USON6 (layer B.Cu) (tedit 5E4DAB76)
    (at 157.16 61.09 180)
    (fp_text reference U1003 (at 0.11 -3.68) (layer B.SilkS) hide)
    (fp_text value OPT3001 (at -0.16 3.7) (layer B.Fab))
    (pad 1 smd roundrect (at -0.95 0.675 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 19 VDDS) (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 101 "Net-(R1008-Pad2)") (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at 0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 44 SCL) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at 0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 100 INT_OPT3001) (solder_mask_margin 0.07))
    (pad 6 smd roundrect (at 0.95 0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 41 SDA) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 0 0 180) (size 0.65 1.35) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 -0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 157.525 72.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.95 62.05 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R502 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(P501-PadA5)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 143.325 69.625 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C821 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C821-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 150.21 58.29 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1002 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 145.2 67.3 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L804 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:X2SON-8_1.4x1mm_P0.35mm (layer B.Cu) (tedit 5A02F1D8)
    (at 152.63 59.85 180)
    (descr "X2SON-8 1.4x1mm Pitch0.35mm http://www.ti.com/lit/ds/symlink/pca9306.pdf")
    (tags "X2SON-8 1.4x1mm Pitch0.35mm")
    (attr smd)
    (fp_text reference U1002 (at 0 2) (layer B.SilkS) hide)
    (fp_text value SN74AUP2G32 (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 95 INT_HDC2010))
    (pad 2 smd rect (at -0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 3 smd rect (at -0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 94 INT_SENSOR))
    (pad 4 smd rect (at -0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 7 smd rect (at 0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 8 smd rect (at 0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer F.Cu) (tedit 5E4C72AA)
    (at 164.4 65.5 270)
    (attr virtual)
    (fp_text reference J301 (at 0.302285 2.603303 270) (layer F.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at -0.967715 -2.222697 270) (layer F.Fab))
    (pad 8 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 29 CC1352_TDI))
    (pad 3 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 9 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 30 CC1352_TMS))
    (pad 10 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 17 RESET_N))
    (pad 1 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 20 3V3))
    (pad 7 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 6 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 31 CC1352_TDO))
    (pad 5 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 32 CC1352_TCK))
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer B.Cu) (tedit 5A0FD1B2)
    (at 173.805 62.475)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y501 (at 0 2.45) (layer B.SilkS) hide)
    (fp_text value 24MHz (at 0 -2.45) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 "/USB Input/XTAL1"))
    (pad 2 smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 "/USB Input/XTAL2"))
    (pad 4 smd rect (at -1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 166.45 68.65 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R510 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 163.295 58.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C509 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 154.63 60.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1007 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 INT_OPT3001))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.55 72.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 171.655 59.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R503 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 90 "/USB Input/D_N"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 202.95 92.05 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R502 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(P501-PadA5)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 169.255 52.75 270)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW901 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 1 smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.65 64.12 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C819 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(AE801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 173.905 58.875 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference D502 (at 0 2.9 270) (layer B.SilkS) hide)
    (fp_text value TPD2E001 (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 90 "/USB Input/D_N"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 91 "/USB Input/D_P"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 79 "/USB Input/VBUS"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm (layer F.Cu) (tedit 5C26A111)
    (at 156.13 67.44)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U801 (at 0 -4.82) (layer F.SilkS) hide)
    (fp_text value CC1352R (at 0 4.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 49 smd roundrect (at 0 0) (size 5.15 5.15) (layers F.Cu F.Mask) (roundrect_rratio 0.048544)
      (net 1 GND))
    (pad "" smd roundrect (at -1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad 1 smd roundrect (at -3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 2 smd roundrect (at -3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 3 smd roundrect (at -3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 4 smd roundrect (at -3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 5 smd roundrect (at -3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 6 smd roundrect (at -3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 7 smd roundrect (at -3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 8 smd roundrect (at -3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 9 smd roundrect (at -3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 10 smd roundrect (at -3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 RST_MB2))
    (pad 11 smd roundrect (at -3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 RST_MB1))
    (pad 12 smd roundrect (at -3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 INT_SENSOR))
    (pad 13 smd roundrect (at -2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 14 smd roundrect (at -2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 15 smd roundrect (at -1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 16 smd roundrect (at -1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 17 smd roundrect (at -0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 18 smd roundrect (at -0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 CS_MB2))
    (pad 19 smd roundrect (at 0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 CS_MB1))
    (pad 20 smd roundrect (at 0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 21 smd roundrect (at 1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 22 smd roundrect (at 1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 23 smd roundrect (at 2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 24 smd roundrect (at 2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 CC1352_TMS))
    (pad 25 smd roundrect (at 3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 CC1352_TCK))
    (pad 26 smd roundrect (at 3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 CC1352_TDO))
    (pad 27 smd roundrect (at 3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 CC1352_TDI))
    (pad 28 smd roundrect (at 3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 29 smd roundrect (at 3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 PWM_MB2))
    (pad 30 smd roundrect (at 3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 INT_MB2))
    (pad 31 smd roundrect (at 3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 32 smd roundrect (at 3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 33 smd roundrect (at 3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 34 smd roundrect (at 3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 35 smd roundrect (at 3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 36 smd roundrect (at 3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 AN_MB1))
    (pad 37 smd roundrect (at 2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 AN_MB2))
    (pad 38 smd roundrect (at 2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 39 smd roundrect (at 1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 40 smd roundrect (at 1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 41 smd roundrect (at 0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 42 smd roundrect (at 0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 INT_MB1))
    (pad 43 smd roundrect (at -0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 PWM_MB1))
    (pad 44 smd roundrect (at -0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 45 smd roundrect (at -1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 46 smd roundrect (at -1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U801-Pad46)"))
    (pad 47 smd roundrect (at -2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U801-Pad47)"))
    (pad 48 smd roundrect (at -2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 185.4 110.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R405 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 166.97 60.16 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C508 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 201.585 62.7 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 208.82 104.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C505 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0.47U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 188.4 121.3 180)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y802 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Crystal_GND2 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U801-Pad47)"))
    (pad 2 smd rect (at 0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U801-Pad46)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 149.62 127.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C812 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 202.95 91.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R506 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(R506-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 152.28 123.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C808 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:HDC2010 (layer F.Cu) (tedit 5E4D6772)
    (at 190.58 88.95)
    (fp_text reference U1001 (at -0.025 2.025) (layer F.SilkS) hide)
    (fp_text value HDC2010 (at 0 -3.8) (layer F.Fab))
    (pad A2 smd circle (at 0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA) (solder_mask_margin 0.05))
    (pad B2 smd circle (at 0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL) (solder_mask_margin 0.05))
    (pad C2 smd circle (at 0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 95 INT_HDC2010) (solder_mask_margin 0.05))
    (pad C1 smd circle (at -0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad B1 smd circle (at -0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R1004-Pad1)") (solder_mask_margin 0.05))
    (pad A1 smd circle (at -0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS) (solder_mask_margin 0.05))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 186.725 73.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Palconn_UTC16-G (layer F.Cu) (tedit 5CF432E0)
    (at 207.5 90.3 90)
    (descr http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf)
    (tags "USB C Type-C Receptacle USB2.0")
    (attr smd)
    (fp_text reference P501 (at 0 -4.58 90) (layer F.SilkS) hide)
    (fp_text value USB_C_Plug_USB2.0 (at 0 6.24 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.43 90) (layer Dwgs.User))
    (fp_text user %R (at 0 1.18 90) (layer F.Fab))
    (pad A12 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B1 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B4 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B12 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A1 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B9 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A4 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad "" np_thru_hole circle (at -2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad B5 smd rect (at 1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(P501-PadB5)"))
    (pad B6 smd rect (at 0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A8 smd rect (at 1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at -1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P501-PadA5)"))
    (pad B8 smd rect (at -1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A7 smd rect (at 0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 90 "/USB Input/D_N"))
    (pad A6 smd rect (at -0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 91 "/USB Input/D_P"))
    (pad B7 smd rect (at -0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad S1 thru_hole oval (at 4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/1054500101.stp
      (offset (xyz 0 -0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Package_LGA:LGA-12_2x2mm_P0.5mm (layer F.Cu) (tedit 5A0AAFFD)
    (at 188.01 88.69 180)
    (descr LGA12)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U1004 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value LIS2DE12 (at 0 1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at -0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 9 smd rect (at 0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 8 smd rect (at 0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 7 smd rect (at 0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 5 smd rect (at -0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 99 INT_LIS2DE12_2))
    (pad 12 smd rect (at -0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:RFECA3216060A1T (layer F.Cu) (tedit 5E42DF6C)
    (at 142.28 64 270)
    (fp_text reference AE801 (at 0 1.85 90) (layer F.SilkS) hide)
    (fp_text value Antenna_Dipole (at 0.05 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at 1.4 -0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AE801-Pad1)"))
    (pad 2 smd rect (at 1.4 0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.4 0 270) (size 0.35 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(AE801-Pad3)"))
    (model ${KIPRJMOD}/mech/2450AT18D0100.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 173.38 77.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H102 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 159.68 61.11 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1008 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(R1008-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 205.18 137.25 90)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW902 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 1 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 2 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.725 69.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R809 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R809-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 200.05 90.75)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U502 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value BQ21040 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 ~CHG))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R506-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 197.975 93.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R805 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 207.08 130.2 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J201 (at 0 -5.8 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.95 90) (layer F.Fab) hide)
    (pad MP smd roundrect (at 3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at -3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad 2 smd roundrect (at 1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.step
      (offset (xyz -1 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer F.Cu) (tedit 5E4C72AA)
    (at 164.4 95.5 270)
    (attr virtual)
    (fp_text reference J301 (at 0.302285 2.603303 270) (layer F.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at -0.967715 -2.222697 270) (layer F.Fab))
    (pad 4 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 32 CC1352_TCK))
    (pad 5 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 31 CC1352_TDO))
    (pad 7 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 1 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 20 3V3))
    (pad 10 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 17 RESET_N))
    (pad 2 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 30 CC1352_TMS))
    (pad 9 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 3 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 8 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 29 CC1352_TDI))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 182.3 122.1 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C816 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 186.21 118.29 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1002 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 159.68 91.11 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1008 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(R1008-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 198.05 80.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R403 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 149.41 110.6)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D405 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 162.05 110.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R403 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 185.62 97.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C812 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.725 129.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R809 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R809-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 158.05 118.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R803 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 CC1352_RX_MB2_TX))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 165.685 118.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "100 pF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 202.44 102.43 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C503 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 192.25 50.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R401 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 195.14 50.57)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R402 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 185.41 50.6)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D405 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 203.535 62.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(R601-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 185.4 50.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R405 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 188.9 50.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R404 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 198.05 50.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R403 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 201.685 119.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 194.38 132.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C805 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 185.62 67.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C812 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 201.585 122.7 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 202.95 121.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R506 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(R506-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N48_EP5.15x5.15mm (layer B.Cu) (tedit 5E4C745D)
    (at 171.05 130.15 180)
    (descr "QFN, 48 Pin (http://www.ti.com/lit/ds/symlink/msp430f5232.pdf#page=112), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U501 (at 0 4.82) (layer B.SilkS) hide)
    (fp_text value MSP430F5500IRGZ (at 0 -4.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 49 smd roundrect (at 0 0 180) (size 5.15 5.15) (layers B.Cu B.Mask) (roundrect_rratio 0.049)
      (net 1 GND))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad 1 smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 8 smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 12 smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 13 smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 14 smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 15 smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 16 smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 17 smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 18 smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 19 smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 20 smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 21 smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 22 smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 23 smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 24 smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 25 smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 26 smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 27 smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 28 smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 29 smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 30 smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 31 smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 32 smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 33 smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 34 smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 35 smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 36 smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 37 smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 38 smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 39 smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 40 smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 41 smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 42 smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 43 smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 44 smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 45 smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 46 smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 47 smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 48 smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 "/USB Input/MSP430_RST_N"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N48_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:0900PC15A0036 (layer F.Cu) (tedit 5E41EA1D)
    (at 150.14 125.44 270)
    (fp_text reference B801 (at 0.025 4.2 90) (layer F.SilkS) hide)
    (fp_text value 0900PC15A0036E (at -0.05 -3.025 90) (layer F.Fab))
    (pad 4 smd roundrect (at 0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (pad 3 smd roundrect (at 0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 6 smd roundrect (at 0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 7 smd roundrect (at 0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 8 smd roundrect (at -0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 9 smd roundrect (at -0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 5 smd roundrect (at 1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 10 smd roundrect (at -1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/0900PC15J0013.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 205.955 106.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C501 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 143.38 112.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H103 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 178.28 121.315 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C822 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(AE801-Pad3)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD (layer B.Cu) (tedit 5E541D54)
    (at 156.6 125.6 90)
    (fp_text reference J702 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value mikroBUS (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at 11.43 0) (layer B.Fab))
    (fp_text user %R (at -11.43 0) (layer B.Fab))
    (pad 10 smd rect (at 13.08 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 28 5V))
    (pad 12 smd rect (at 13.08 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 44 SCL))
    (pad 14 smd rect (at 13.08 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 43 CC1352_TX_MB2_RX))
    (pad 16 smd rect (at 13.08 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 42 PWM_MB2))
    (pad 9 smd rect (at 9.78 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 9.78 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 41 SDA))
    (pad 13 smd rect (at 9.78 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 40 CC1352_RX_MB2_TX))
    (pad 15 smd rect (at 9.78 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 39 INT_MB2))
    (pad 8 smd rect (at -13.08 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -13.08 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 2 smd rect (at -13.08 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 37 RST_MB2))
    (pad 1 smd rect (at -9.78 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 36 AN_MB2))
    (pad 4 smd rect (at -13.08 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at -9.78 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 20 3V3))
    (pad 3 smd rect (at -9.78 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 34 CS_MB2))
    (pad 5 smd rect (at -9.78 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 168.63 112.575 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D501 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 179.25 132.85 90)
    (fp_text reference J802 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C821-Pad2)"))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.32 124.11 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C814 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:L_0806_2012Metric (layer B.Cu) (tedit 5D2F3EE6)
    (at 168.985 119.9 90)
    (descr "Inductor SMD 0806 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L601 (at 0 1.65 90) (layer B.SilkS) hide)
    (fp_text value INDUCTOR (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(L601-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 160.43 118.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R802 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 CC1352_TX_MB2_RX))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 159.38 132.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C803 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 173 125.57 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C504 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 220N (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 181.65 124.12 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C819 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(AE801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 169.98 137.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R507 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 142.28 121.315 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C822 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(AE801-Pad3)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 202.44 132.43 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C503 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 166.44 130.55 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R509 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 158.38 132.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C805 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:BeagleBoard.org-20mm (layer B.Cu) (tedit 0)
    (at 179.38 125.3 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 207.08 70.2 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J201 (at 0 -5.8 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.95 90) (layer F.Fab) hide)
    (pad MP smd roundrect (at 3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at -3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad 2 smd roundrect (at 1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.step
      (offset (xyz -1 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 143.25 132.85 90)
    (fp_text reference J802 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 4 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C821-Pad2)"))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 144.88 121.4 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C818 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C818-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 187.39 117.76 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1005 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(R1005-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.505 118.3 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R604 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 143.85 127.95 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C817 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "5.6 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 155.58 118.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1001 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 182.99 93.44 315)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L803 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2 nH" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:TPS62821DLC (layer B.Cu) (tedit 5D2676FA)
    (at 166.885 121.1)
    (fp_text reference U601 (at 0.1 1.975 180) (layer B.SilkS) hide)
    (fp_text value TPS62821DLC (at 0 0.5 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 2 smd roundrect (at -0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(C602-Pad2)"))
    (pad 3 smd roundrect (at -0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 4 smd roundrect (at -0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2))
    (pad 5 smd roundrect (at 0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 6 smd roundrect (at 0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 73 "Net-(L601-Pad1)"))
    (pad 7 smd roundrect (at 0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 8 smd roundrect (at 0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 74 "Net-(R601-Pad1)"))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1.3 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.875 125.925 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C815 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2.7 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.725 101.525)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.55 132.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 209.905 118.875 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference D502 (at 0 2.9 270) (layer B.SilkS) hide)
    (fp_text value TPD2E001 (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 91 "/USB Input/D_P"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 90 "/USB Input/D_N"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 181.2 127.3 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L804 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 171.655 119.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R503 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 90 "/USB Input/D_N"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:HDC2010 (layer F.Cu) (tedit 5E4D6772)
    (at 154.58 118.95)
    (fp_text reference U1001 (at -0.025 2.025) (layer F.SilkS) hide)
    (fp_text value HDC2010 (at 0 -3.8) (layer F.Fab))
    (pad A2 smd circle (at 0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA) (solder_mask_margin 0.05))
    (pad B2 smd circle (at 0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL) (solder_mask_margin 0.05))
    (pad C2 smd circle (at 0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 95 INT_HDC2010) (solder_mask_margin 0.05))
    (pad C1 smd circle (at -0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad B1 smd circle (at -0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R1004-Pad1)") (solder_mask_margin 0.05))
    (pad A1 smd circle (at -0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS) (solder_mask_margin 0.05))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 158.475 132.95 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 145.25 129.375 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C820 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(AE802-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 162.96 118.76 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C603 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value "10 uF" (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 199.295 118.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C509 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 156.48 123 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 190.63 88.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1002 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 206.68 59.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R504 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 "/USB Input/D_P"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 171.17 123.035 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C507 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 149.4 110.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R405 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.725 130.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R810 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 165.13 110.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D406 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 165.12 110.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R406 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 ~CHG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 143.48 117.8 270)
    (fp_text reference J801 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 4 smd rect (at 0 1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C818-Pad2)"))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 186.725 102.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 172.82 134.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C505 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0.47U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 143.38 137.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H104 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 206.68 89.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R504 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 "/USB Input/D_P"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 152.9 110.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R404 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 181.65 94.12 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C819 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(AE801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:L_0806_2012Metric (layer B.Cu) (tedit 5D2F3EE6)
    (at 204.985 59.9 90)
    (descr "Inductor SMD 0806 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L601 (at 0 1.65 90) (layer B.SilkS) hide)
    (fp_text value INDUCTOR (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(L601-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 196.025 65.1 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C804 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 202.36 88.01)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F501 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value Polyfuse (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 189.28 57.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1001 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 181.875 95.925 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C815 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2.7 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 205.18 77.25 90)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW902 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 1 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 2 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 184.63 100.5 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C801 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 201.685 58.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "100 pF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 178.28 91.315 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C822 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(AE801-Pad3)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 182.9 72.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference AE802 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(AE802-Pad1)"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 202.44 100.55 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R509 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 195.145 80.58)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D402 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 192.55 132.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 193.5 67.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C810 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "22 uF" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:TPS62821DLC (layer B.Cu) (tedit 5D2676FA)
    (at 202.885 121.1)
    (fp_text reference U601 (at 0.1 1.975 180) (layer B.SilkS) hide)
    (fp_text value TPS62821DLC (at 0 0.5 180) (layer B.Fab))
    (pad 8 smd roundrect (at 0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 74 "Net-(R601-Pad1)"))
    (pad 7 smd roundrect (at 0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 6 smd roundrect (at 0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 73 "Net-(L601-Pad1)"))
    (pad 5 smd roundrect (at 0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 4 smd roundrect (at -0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2))
    (pad 3 smd roundrect (at -0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1.3 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 182.3 92.1 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C816 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.28 98.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:RFECA3216060A1T (layer F.Cu) (tedit 5E42DF6C)
    (at 142.28 94 270)
    (fp_text reference AE801 (at 0 1.85 90) (layer F.SilkS) hide)
    (fp_text value Antenna_Dipole (at 0.05 -1.7 90) (layer F.Fab))
    (pad 3 smd rect (at -1.4 0 270) (size 0.35 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(AE801-Pad3)"))
    (pad 2 smd rect (at 1.4 0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.4 -0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AE801-Pad1)"))
    (model ${KIPRJMOD}/mech/2450AT18D0100.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 195.38 72.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C803 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 151.23 119.33 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1003 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(R1003-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 192.25 80.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R401 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 203.535 92.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(R601-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 207.17 93.035 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C507 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 205.755 75.55 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L501 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 198.055 50.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D403 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 207.17 123.035 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C507 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 209.38 82.56)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H101 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 185.4 80.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R405 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 194.475 102.95 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 192.48 63 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 188.9 110.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D404 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 149.755 99.575 315)
    (descr "SMD Crystal 2012/2 http://txccrystal.com/images/pdf/9ht11.pdf, 2.0x1.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y801 (at 0 -1.8 135) (layer F.SilkS) hide)
    (fp_text value Crystal (at 0 1.8 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C802-Pad1)"))
    (pad 1 smd rect (at -0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C801-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_AX_8045-2Pin_8.0x4.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.25 0.3 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 197.965 92.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R804 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 209.38 52.56)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H101 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 202.95 122.05 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R502 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(P501-PadA5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm (layer F.Cu) (tedit 5C26A111)
    (at 156.13 97.44)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U801 (at 0 -4.82) (layer F.SilkS) hide)
    (fp_text value CC1352R (at 0 4.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 48 smd roundrect (at -2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 47 smd roundrect (at -2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U801-Pad47)"))
    (pad 46 smd roundrect (at -1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U801-Pad46)"))
    (pad 45 smd roundrect (at -1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 44 smd roundrect (at -0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 43 smd roundrect (at -0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 PWM_MB1))
    (pad 42 smd roundrect (at 0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 INT_MB1))
    (pad 41 smd roundrect (at 0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 40 smd roundrect (at 1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 39 smd roundrect (at 1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 38 smd roundrect (at 2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 37 smd roundrect (at 2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 AN_MB2))
    (pad 36 smd roundrect (at 3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 AN_MB1))
    (pad 35 smd roundrect (at 3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 34 smd roundrect (at 3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 33 smd roundrect (at 3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 32 smd roundrect (at 3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 31 smd roundrect (at 3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 30 smd roundrect (at 3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 INT_MB2))
    (pad 29 smd roundrect (at 3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 PWM_MB2))
    (pad 28 smd roundrect (at 3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 27 smd roundrect (at 3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 CC1352_TDI))
    (pad 26 smd roundrect (at 3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 CC1352_TDO))
    (pad 25 smd roundrect (at 3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 CC1352_TCK))
    (pad 24 smd roundrect (at 2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 CC1352_TMS))
    (pad 23 smd roundrect (at 2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 22 smd roundrect (at 1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 21 smd roundrect (at 1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 20 smd roundrect (at 0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 19 smd roundrect (at 0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 CS_MB1))
    (pad 18 smd roundrect (at -0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 CS_MB2))
    (pad 17 smd roundrect (at -0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 16 smd roundrect (at -1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 15 smd roundrect (at -1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 14 smd roundrect (at -2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 13 smd roundrect (at -2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 12 smd roundrect (at -3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 INT_SENSOR))
    (pad 11 smd roundrect (at -3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 RST_MB1))
    (pad 10 smd roundrect (at -3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 RST_MB2))
    (pad 9 smd roundrect (at -3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 8 smd roundrect (at -3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 7 smd roundrect (at -3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 6 smd roundrect (at -3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 5 smd roundrect (at -3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 4 smd roundrect (at -3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 3 smd roundrect (at -3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 2 smd roundrect (at -3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 1 smd roundrect (at -3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad "" smd roundrect (at 1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad 49 smd roundrect (at 0 0) (size 5.15 5.15) (layers F.Cu F.Mask) (roundrect_rratio 0.048544)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 188.28 63.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C808 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Palconn_UTC16-G (layer F.Cu) (tedit 5CF432E0)
    (at 207.5 120.3 90)
    (descr http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf)
    (tags "USB C Type-C Receptacle USB2.0")
    (attr smd)
    (fp_text reference P501 (at 0 -4.58 90) (layer F.SilkS) hide)
    (fp_text value USB_C_Plug_USB2.0 (at 0 6.24 90) (layer F.Fab))
    (fp_text user %R (at 0 1.18 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.43 90) (layer Dwgs.User))
    (pad S1 thru_hole oval (at -4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B7 smd rect (at -0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A6 smd rect (at -0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 91 "/USB Input/D_P"))
    (pad A7 smd rect (at 0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 90 "/USB Input/D_N"))
    (pad B8 smd rect (at -1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at -1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P501-PadA5)"))
    (pad A8 smd rect (at 1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad B6 smd rect (at 0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad B5 smd rect (at 1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(P501-PadB5)"))
    (pad "" np_thru_hole circle (at 2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad A4 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B9 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A1 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B12 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B4 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B1 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A12 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/1054500101.stp
      (offset (xyz 0 -0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module leash:MikroBus-SMD (layer B.Cu) (tedit 5E541D54)
    (at 156.6 65.6 90)
    (fp_text reference J702 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value mikroBUS (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at 11.43 0) (layer B.Fab))
    (fp_text user %R (at -11.43 0) (layer B.Fab))
    (pad 10 smd rect (at 13.08 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 28 5V))
    (pad 12 smd rect (at 13.08 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 44 SCL))
    (pad 14 smd rect (at 13.08 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 43 CC1352_TX_MB2_RX))
    (pad 16 smd rect (at 13.08 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 42 PWM_MB2))
    (pad 9 smd rect (at 9.78 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 9.78 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 41 SDA))
    (pad 13 smd rect (at 9.78 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 40 CC1352_RX_MB2_TX))
    (pad 15 smd rect (at 9.78 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 39 INT_MB2))
    (pad 8 smd rect (at -13.08 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -13.08 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 2 smd rect (at -13.08 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 37 RST_MB2))
    (pad 1 smd rect (at -9.78 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 36 AN_MB2))
    (pad 4 smd rect (at -13.08 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at -9.78 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 20 3V3))
    (pad 3 smd rect (at -9.78 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 34 CS_MB2))
    (pad 5 smd rect (at -9.78 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 169.18 107.25 90)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW902 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 1 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 2 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 191.58 88.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1001 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 166.45 128.65 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R510 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD locked (layer F.Cu) (tedit 5E541D62)
    (at 192.68 125.6 90)
    (fp_text reference J701 (at -0.074182 -1.275144 90) (layer F.SilkS) hide)
    (fp_text value mikroBUS (at -0.074182 -0.005144 90) (layer F.Fab))
    (fp_text user %R (at 11.43 0 180) (layer F.Fab))
    (fp_text user %R (at 11.355818 -0.005144 180) (layer F.Fab) hide)
    (pad 10 smd rect (at 13.08 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 12 smd rect (at 13.08 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 14 smd rect (at 13.08 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 45 CC1352_TX_MB1_RX))
    (pad 16 smd rect (at 13.08 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM_MB1))
    (pad 9 smd rect (at 9.78 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 9.78 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 13 smd rect (at 9.78 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 47 CC1352_RX_MB1_TX))
    (pad 15 smd rect (at 9.78 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 48 INT_MB1))
    (pad 8 smd rect (at -13.08 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -13.08 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 38 MOSI))
    (pad 2 smd rect (at -13.08 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 49 RST_MB1))
    (pad 1 smd rect (at -9.78 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 50 AN_MB1))
    (pad 4 smd rect (at -13.08 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at -9.78 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 20 3V3))
    (pad 3 smd rect (at -9.78 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 51 CS_MB1))
    (pad 5 smd rect (at -9.78 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 33 MISO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 201.49 93.7)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D201 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 172.82 74.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C505 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0.47U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 203.88 107.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R511 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 173 65.57 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C504 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 220N (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.84 65.49 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R508 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1.5K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 169.18 77.25 90)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW902 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 1 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 146.9 72.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference AE802 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(AE802-Pad1)"))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 142.28 61.315 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C822 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(AE801-Pad3)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 166.44 72.43 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C503 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 144.88 61.4 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C818 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C818-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 143.48 57.8 270)
    (fp_text reference J801 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 4 smd rect (at 0 1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C818-Pad2)"))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module leash:L_0806_2012Metric (layer B.Cu) (tedit 5D2F3EE6)
    (at 168.985 59.9 90)
    (descr "Inductor SMD 0806 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L601 (at 0 1.65 90) (layer B.SilkS) hide)
    (fp_text value INDUCTOR (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(L601-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 149.755 69.575 315)
    (descr "SMD Crystal 2012/2 http://txccrystal.com/images/pdf/9ht11.pdf, 2.0x1.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y801 (at 0 -1.8 135) (layer F.SilkS) hide)
    (fp_text value Crystal (at 0 1.8 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C801-Pad1)"))
    (pad 2 smd rect (at 0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_AX_8045-2Pin_8.0x4.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.25 0.3 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 152.4 61.3 180)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y802 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Crystal_GND2 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U801-Pad46)"))
    (pad 2 smd rect (at 0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U801-Pad47)"))
    (pad 4 smd rect (at -0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 162.25 65.625)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L801 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 168.63 52.575 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D501 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 158.05 58.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R803 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 CC1352_RX_MB2_TX))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 160.43 58.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R802 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 CC1352_TX_MB2_RX))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 205.18 107.25 90)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW902 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 1 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 143.25 72.85 90)
    (fp_text reference J802 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 4 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C821-Pad2)"))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module leash:MX25R8035FZUIL0 (layer B.Cu) (tedit 5E42FFC6)
    (at 152.775 71.08 270)
    (fp_text reference U802 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value MX25R8035FZUIL0 (at 0 -2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 109 ~FLASH_CS))
    (pad 2 smd rect (at -1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R809-Pad2)"))
    (pad 4 smd rect (at -1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 6 smd rect (at 1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at 1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 8 smd rect (at 1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C811-Pad2)"))
    (pad 9 smd custom (at 0 0 270) (size 0.2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0 0.8) (xy 0.1 0.8) (xy 0.1 -0.8) (xy -0.1 -0.8) (xy -0.1 0.7)
) (width 0))
      ))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:TPS62821DLC (layer B.Cu) (tedit 5D2676FA)
    (at 166.885 61.1)
    (fp_text reference U601 (at 0.1 1.975 180) (layer B.SilkS) hide)
    (fp_text value TPS62821DLC (at 0 0.5 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 2 smd roundrect (at -0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(C602-Pad2)"))
    (pad 3 smd roundrect (at -0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 4 smd roundrect (at -0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2))
    (pad 5 smd roundrect (at 0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 6 smd roundrect (at 0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 73 "Net-(L601-Pad1)"))
    (pad 7 smd roundrect (at 0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 8 smd roundrect (at 0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 74 "Net-(R601-Pad1)"))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1.3 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 162.96 58.76 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C603 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value "10 uF" (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.32 64.11 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C814 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 150.725 73.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 157.5 67.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C810 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "22 uF" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 154.88 61.9 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C809 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 152.28 63.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C808 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 156.48 63 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 160.025 65.1 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C804 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 159.38 72.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C803 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 145.2 97.3 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L804 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.36 58.01)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F501 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value Polyfuse (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.47 60.665 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1006 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 INT_LIS2DE12_2))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 203.84 65.49 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R508 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1.5K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LGA:LGA-12_2x2mm_P0.5mm (layer F.Cu) (tedit 5A0AAFFD)
    (at 152.01 58.69 180)
    (descr LGA12)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U1004 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value LIS2DE12 (at 0 1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at -0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 9 smd rect (at 0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 8 smd rect (at 0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 7 smd rect (at 0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 5 smd rect (at -0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 99 INT_LIS2DE12_2))
    (pad 12 smd rect (at -0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 167.88 77.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R511 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 169.98 77.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R507 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 169.755 75.55 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L501 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Palconn_UTC16-G (layer F.Cu) (tedit 5CF432E0)
    (at 171.5 60.3 90)
    (descr http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf)
    (tags "USB C Type-C Receptacle USB2.0")
    (attr smd)
    (fp_text reference P501 (at 0 -4.58 90) (layer F.SilkS) hide)
    (fp_text value USB_C_Plug_USB2.0 (at 0 6.24 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.43 90) (layer Dwgs.User))
    (fp_text user %R (at 0 1.18 90) (layer F.Fab))
    (pad A12 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B1 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B4 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B12 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A1 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B9 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A4 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad "" np_thru_hole circle (at -2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad B5 smd rect (at 1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(P501-PadB5)"))
    (pad B6 smd rect (at 0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A8 smd rect (at 1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at -1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P501-PadA5)"))
    (pad B8 smd rect (at -1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A7 smd rect (at 0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 90 "/USB Input/D_N"))
    (pad A6 smd rect (at -0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 91 "/USB Input/D_P"))
    (pad B7 smd rect (at -0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad S1 thru_hole oval (at 4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/1054500101.stp
      (offset (xyz 0 -0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 143.38 52.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H103 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 143.38 77.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H104 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N48_EP5.15x5.15mm (layer B.Cu) (tedit 5E4C745D)
    (at 171.05 70.15 180)
    (descr "QFN, 48 Pin (http://www.ti.com/lit/ds/symlink/msp430f5232.pdf#page=112), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U501 (at 0 4.82) (layer B.SilkS) hide)
    (fp_text value MSP430F5500IRGZ (at 0 -4.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 49 smd roundrect (at 0 0 180) (size 5.15 5.15) (layers B.Cu B.Mask) (roundrect_rratio 0.049)
      (net 1 GND))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad 1 smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 8 smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 12 smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 13 smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 14 smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 15 smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 16 smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 17 smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 18 smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 19 smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 20 smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 21 smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 22 smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 23 smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 24 smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 25 smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 26 smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 27 smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 28 smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 29 smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 30 smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 31 smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 32 smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 33 smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 34 smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 35 smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 36 smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 37 smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 38 smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 39 smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 40 smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 41 smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 42 smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 43 smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 44 smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 45 smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 46 smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 47 smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 48 smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 "/USB Input/MSP430_RST_N"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N48_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:0900PC15A0036 (layer F.Cu) (tedit 5E41EA1D)
    (at 150.14 65.44 270)
    (fp_text reference B801 (at 0.025 4.2 90) (layer F.SilkS) hide)
    (fp_text value 0900PC15A0036E (at -0.05 -3.025 90) (layer F.Fab))
    (pad 4 smd roundrect (at 0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (pad 3 smd roundrect (at 0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 6 smd roundrect (at 0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 7 smd roundrect (at 0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 8 smd roundrect (at -0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 9 smd roundrect (at -0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 5 smd roundrect (at 1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 10 smd roundrect (at -1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/0900PC15J0013.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 173.38 52.56)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H101 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 165.585 62.7 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 162.28 68.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 157.68 65.9)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L802 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 161.965 62.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R804 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 161.975 63.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R805 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.505 58.3 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R604 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 165.49 63.7)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D201 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 152.9 50.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D404 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 162.055 50.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D403 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 156.25 50.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D401 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 159.145 50.58)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D402 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 165.685 58.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "100 pF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 150.855 71.125 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C802 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 148.63 70.5 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C801 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 164.23 59.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R603 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 179.38 77.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H104 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 165.685 59.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 156.25 50.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R401 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 159.14 50.57)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R402 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 149.41 50.6)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D405 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 167.535 62.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(R601-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 149.4 50.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R405 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 152.9 50.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R404 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 162.05 50.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R403 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 164.05 60.75)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U502 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value BQ21040 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 ~CHG))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R506-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.95 61.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R506 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(R506-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:RFECA3216060A1T (layer F.Cu) (tedit 5E42DF6C)
    (at 178.28 64 270)
    (fp_text reference AE801 (at 0 1.85 90) (layer F.SilkS) hide)
    (fp_text value Antenna_Dipole (at 0.05 -1.7 90) (layer F.Fab))
    (pad 3 smd rect (at -1.4 0 270) (size 0.35 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(AE801-Pad3)"))
    (pad 2 smd rect (at 1.4 0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.4 -0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AE801-Pad1)"))
    (model ${KIPRJMOD}/mech/2450AT18D0100.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 165.12 50.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R406 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 ~CHG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 188.28 123.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C808 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 165.13 50.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D406 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD locked (layer F.Cu) (tedit 5E541D62)
    (at 120.68 65.6 90)
    (fp_text reference J701 (at -0.074182 -1.275144 90) (layer F.SilkS) hide)
    (fp_text value mikroBUS (at -0.074182 -0.005144 90) (layer F.Fab))
    (fp_text user %R (at 11.355818 -0.005144 180) (layer F.Fab) hide)
    (fp_text user %R (at 11.43 0 180) (layer F.Fab))
    (pad 5 smd rect (at -9.78 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -9.78 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 51 CS_MB1))
    (pad 7 smd rect (at -9.78 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 20 3V3))
    (pad 4 smd rect (at -13.08 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 35 SCK))
    (pad 1 smd rect (at -9.78 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 50 AN_MB1))
    (pad 2 smd rect (at -13.08 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 49 RST_MB1))
    (pad 6 smd rect (at -13.08 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 38 MOSI))
    (pad 8 smd rect (at -13.08 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 9.78 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 48 INT_MB1))
    (pad 13 smd rect (at 9.78 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 47 CC1352_RX_MB1_TX))
    (pad 11 smd rect (at 9.78 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 9 smd rect (at 9.78 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 13.08 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM_MB1))
    (pad 14 smd rect (at 13.08 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 45 CC1352_TX_MB1_RX))
    (pad 12 smd rect (at 13.08 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 13.08 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N48_EP5.15x5.15mm (layer B.Cu) (tedit 5E4C745D)
    (at 135.05 100.15 180)
    (descr "QFN, 48 Pin (http://www.ti.com/lit/ds/symlink/msp430f5232.pdf#page=112), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U501 (at 0 4.82) (layer B.SilkS) hide)
    (fp_text value MSP430F5500IRGZ (at 0 -4.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 48 smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 47 smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 46 smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 45 smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 44 smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 43 smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 42 smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 41 smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 40 smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 39 smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 38 smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 37 smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 36 smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 35 smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 34 smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 33 smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 32 smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 31 smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 30 smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 29 smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 28 smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 27 smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 26 smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 25 smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 24 smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 23 smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 22 smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 21 smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 20 smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 19 smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 18 smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 17 smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 16 smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 15 smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 14 smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 12 smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 10 smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 6 smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad 49 smd roundrect (at 0 0 180) (size 5.15 5.15) (layers B.Cu B.Mask) (roundrect_rratio 0.049)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N48_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:0900PC15A0036 (layer F.Cu) (tedit 5E41EA1D)
    (at 114.14 95.44 270)
    (fp_text reference B801 (at 0.025 4.2 90) (layer F.SilkS) hide)
    (fp_text value 0900PC15A0036E (at -0.05 -3.025 90) (layer F.Fab))
    (pad 10 smd roundrect (at -1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 smd roundrect (at 1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 9 smd roundrect (at -0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 8 smd roundrect (at -0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 7 smd roundrect (at 0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 6 smd roundrect (at 0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 1 smd roundrect (at -0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 2 smd roundrect (at -0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at 0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at 0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (model ${KIPRJMOD}/mech/0900PC15J0013.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 107.38 82.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H103 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module leash:MX25R8035FZUIL0 (layer B.Cu) (tedit 5E42FFC6)
    (at 116.775 101.08 270)
    (fp_text reference U802 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value MX25R8035FZUIL0 (at 0 -2 90) (layer B.Fab))
    (pad 9 smd custom (at 0 0 270) (size 0.2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0 0.8) (xy 0.1 0.8) (xy 0.1 -0.8) (xy -0.1 -0.8) (xy -0.1 0.7)
) (width 0))
      ))
    (pad 8 smd rect (at 1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C811-Pad2)"))
    (pad 7 smd rect (at 1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 6 smd rect (at 1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 5 smd rect (at 1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 4 smd rect (at -1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R809-Pad2)"))
    (pad 2 smd rect (at -1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 1 smd rect (at -1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 109 ~FLASH_CS))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.9 80.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D404 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 126.25 95.625)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L801 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD (layer B.Cu) (tedit 5E541D54)
    (at 120.6 95.6 90)
    (fp_text reference J702 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value mikroBUS (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at -11.43 0) (layer B.Fab))
    (fp_text user %R (at 11.43 0) (layer B.Fab))
    (pad 5 smd rect (at -9.78 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -9.78 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 34 CS_MB2))
    (pad 7 smd rect (at -9.78 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 20 3V3))
    (pad 4 smd rect (at -13.08 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 1 smd rect (at -9.78 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 36 AN_MB2))
    (pad 2 smd rect (at -13.08 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 37 RST_MB2))
    (pad 6 smd rect (at -13.08 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 8 smd rect (at -13.08 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 9.78 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 39 INT_MB2))
    (pad 13 smd rect (at 9.78 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 40 CC1352_RX_MB2_TX))
    (pad 11 smd rect (at 9.78 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 41 SDA))
    (pad 9 smd rect (at 9.78 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 13.08 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 42 PWM_MB2))
    (pad 14 smd rect (at 13.08 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 43 CC1352_TX_MB2_RX))
    (pad 12 smd rect (at 13.08 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 13.08 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 119.6 132.925 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 132.63 82.575 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D501 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 112.32 94.11 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C814 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 124.025 125.1 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C804 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:L_0806_2012Metric (layer B.Cu) (tedit 5D2F3EE6)
    (at 132.985 89.9 90)
    (descr "Inductor SMD 0806 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L601 (at 0 1.65 90) (layer B.SilkS) hide)
    (fp_text value INDUCTOR (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(L601-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 124.43 88.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R802 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 CC1352_TX_MB2_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 119.6 102.925 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer B.Cu) (tedit 5D409D35)
    (at 128.4 95.5 270)
    (attr virtual)
    (fp_text reference J501 (at 3.81 -2.413 90) (layer B.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at 2.54 2.413 90) (layer B.Fab))
    (pad 4 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 5 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 6 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 7 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 1 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 20 3V3))
    (pad 10 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 2 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 9 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 3 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 8 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 10 "/USB Input/MSP430_TDI"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.84 95.49 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R508 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1.5K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 111.825 96.175 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C813 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 110.3 92.1 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C816 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 122.05 88.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R803 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 CC1352_RX_MB2_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 123.38 102.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C803 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 137 95.57 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C504 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 220N (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 133.98 107.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R507 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 106.28 91.315 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C822 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(AE801-Pad3)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 130.44 100.55 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R509 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 126.25 125.625)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L801 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.38 102.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C805 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 107.25 102.85 90)
    (fp_text reference J802 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C821-Pad2)"))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 108.88 91.4 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C818 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C818-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.505 88.3 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R604 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 107.85 97.95 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C817 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "5.6 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 119.58 88.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1001 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:TPS62821DLC (layer B.Cu) (tedit 5D2676FA)
    (at 130.885 91.1)
    (fp_text reference U601 (at 0.1 1.975 180) (layer B.SilkS) hide)
    (fp_text value TPS62821DLC (at 0 0.5 180) (layer B.Fab))
    (pad 8 smd roundrect (at 0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 74 "Net-(R601-Pad1)"))
    (pad 7 smd roundrect (at 0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 6 smd roundrect (at 0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 73 "Net-(L601-Pad1)"))
    (pad 5 smd roundrect (at 0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 4 smd roundrect (at -0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2))
    (pad 3 smd roundrect (at -0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1.3 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.875 95.925 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C815 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2.7 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 120.55 102.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 133.255 82.75 270)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW901 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 1 smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 2 smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.36 118.01)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F501 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value Polyfuse (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 133.18 137.25 90)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW902 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 1 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 125.975 123.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R805 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 123.145 110.58)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D402 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.95 122.05 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R502 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(P501-PadA5)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 135.08 100.2 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J201 (at 0 -5.8 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.95 90) (layer F.Fab) hide)
    (pad MP smd roundrect (at 3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at -3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad 2 smd roundrect (at 1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.step
      (offset (xyz -1 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 135.655 89.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R503 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 90 "/USB Input/D_N"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 120.25 110.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D401 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LGA:LGA-12_2x2mm_P0.5mm (layer F.Cu) (tedit 5A0AAFFD)
    (at 116.01 118.69 180)
    (descr LGA12)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U1004 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value LIS2DE12 (at 0 1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at -0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 9 smd rect (at 0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 8 smd rect (at 0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 7 smd rect (at 0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 5 smd rect (at -0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 99 INT_LIS2DE12_2))
    (pad 12 smd rect (at -0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 113.755 129.575 315)
    (descr "SMD Crystal 2012/2 http://txccrystal.com/images/pdf/9ht11.pdf, 2.0x1.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y801 (at 0 -1.8 135) (layer F.SilkS) hide)
    (fp_text value Crystal (at 0 1.8 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C801-Pad1)"))
    (pad 2 smd rect (at 0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_AX_8045-2Pin_8.0x4.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.25 0.3 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.9 110.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D404 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 130.4 125.99 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R505 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.535 122.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(R601-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 129.49 123.7)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D201 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 121.5 127.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C810 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "22 uF" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 133.755 135.55 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L501 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 131.88 137.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R511 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 110.3 122.1 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C816 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.805 132.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C806 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm (layer F.Cu) (tedit 5C26A111)
    (at 120.13 127.44)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U801 (at 0 -4.82) (layer F.SilkS) hide)
    (fp_text value CC1352R (at 0 4.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 49 smd roundrect (at 0 0) (size 5.15 5.15) (layers F.Cu F.Mask) (roundrect_rratio 0.048544)
      (net 1 GND))
    (pad "" smd roundrect (at -1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad 1 smd roundrect (at -3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 2 smd roundrect (at -3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 3 smd roundrect (at -3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 4 smd roundrect (at -3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 5 smd roundrect (at -3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 6 smd roundrect (at -3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 7 smd roundrect (at -3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 8 smd roundrect (at -3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 9 smd roundrect (at -3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 10 smd roundrect (at -3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 RST_MB2))
    (pad 11 smd roundrect (at -3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 RST_MB1))
    (pad 12 smd roundrect (at -3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 INT_SENSOR))
    (pad 13 smd roundrect (at -2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 14 smd roundrect (at -2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 15 smd roundrect (at -1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 16 smd roundrect (at -1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 17 smd roundrect (at -0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 18 smd roundrect (at -0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 CS_MB2))
    (pad 19 smd roundrect (at 0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 CS_MB1))
    (pad 20 smd roundrect (at 0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 21 smd roundrect (at 1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 22 smd roundrect (at 1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 23 smd roundrect (at 2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 24 smd roundrect (at 2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 CC1352_TMS))
    (pad 25 smd roundrect (at 3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 CC1352_TCK))
    (pad 26 smd roundrect (at 3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 CC1352_TDO))
    (pad 27 smd roundrect (at 3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 CC1352_TDI))
    (pad 28 smd roundrect (at 3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 29 smd roundrect (at 3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 PWM_MB2))
    (pad 30 smd roundrect (at 3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 INT_MB2))
    (pad 31 smd roundrect (at 3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 32 smd roundrect (at 3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 33 smd roundrect (at 3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 34 smd roundrect (at 3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 35 smd roundrect (at 3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 36 smd roundrect (at 3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 AN_MB1))
    (pad 37 smd roundrect (at 2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 AN_MB2))
    (pad 38 smd roundrect (at 2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 39 smd roundrect (at 1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 40 smd roundrect (at 1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 41 smd roundrect (at 0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 42 smd roundrect (at 0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 INT_MB1))
    (pad 43 smd roundrect (at -0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 PWM_MB1))
    (pad 44 smd roundrect (at -0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 45 smd roundrect (at -1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 46 smd roundrect (at -1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U801-Pad46)"))
    (pad 47 smd roundrect (at -2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U801-Pad47)"))
    (pad 48 smd roundrect (at -2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 133.955 136.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C501 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MX25R8035FZUIL0 (layer B.Cu) (tedit 5E42FFC6)
    (at 116.775 131.08 270)
    (fp_text reference U802 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value MX25R8035FZUIL0 (at 0 -2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 109 ~FLASH_CS))
    (pad 2 smd rect (at -1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R809-Pad2)"))
    (pad 4 smd rect (at -1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 6 smd rect (at 1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at 1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 8 smd rect (at 1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C811-Pad2)"))
    (pad 9 smd custom (at 0 0 270) (size 0.2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0 0.8) (xy 0.1 0.8) (xy 0.1 -0.8) (xy -0.1 -0.8) (xy -0.1 0.7)
) (width 0))
      ))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 116.4 121.3 180)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y802 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Crystal_GND2 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U801-Pad46)"))
    (pad 2 smd rect (at 0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U801-Pad47)"))
    (pad 4 smd rect (at -0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.47 120.665 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1006 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 INT_LIS2DE12_2))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.96 119.22 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R501 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(P501-PadB5)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 111.825 126.175 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C813 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:HDC2010 (layer F.Cu) (tedit 5E4D6772)
    (at 118.58 88.95)
    (fp_text reference U1001 (at -0.025 2.025) (layer F.SilkS) hide)
    (fp_text value HDC2010 (at 0 -3.8) (layer F.Fab))
    (pad A1 smd circle (at -0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS) (solder_mask_margin 0.05))
    (pad B1 smd circle (at -0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R1004-Pad1)") (solder_mask_margin 0.05))
    (pad C1 smd circle (at -0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad C2 smd circle (at 0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 95 INT_HDC2010) (solder_mask_margin 0.05))
    (pad B2 smd circle (at 0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL) (solder_mask_margin 0.05))
    (pad A2 smd circle (at 0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA) (solder_mask_margin 0.05))
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 121.68 125.9)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L802 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Palconn_UTC16-G (layer F.Cu) (tedit 5CF432E0)
    (at 135.5 120.3 90)
    (descr http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf)
    (tags "USB C Type-C Receptacle USB2.0")
    (attr smd)
    (fp_text reference P501 (at 0 -4.58 90) (layer F.SilkS) hide)
    (fp_text value USB_C_Plug_USB2.0 (at 0 6.24 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.43 90) (layer Dwgs.User))
    (fp_text user %R (at 0 1.18 90) (layer F.Fab))
    (pad A12 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B1 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B4 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B12 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A1 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B9 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A4 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad "" np_thru_hole circle (at -2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad B5 smd rect (at 1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(P501-PadB5)"))
    (pad B6 smd rect (at 0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A8 smd rect (at 1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at -1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P501-PadA5)"))
    (pad B8 smd rect (at -1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A7 smd rect (at 0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 90 "/USB Input/D_N"))
    (pad A6 smd rect (at -0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 91 "/USB Input/D_P"))
    (pad B7 smd rect (at -0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad S1 thru_hole oval (at 4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/1054500101.stp
      (offset (xyz 0 -0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.84 125.49 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R508 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1.5K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 122.475 102.95 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 125.965 122.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R804 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer B.Cu) (tedit 5D409D35)
    (at 128.4 125.5 270)
    (attr virtual)
    (fp_text reference J501 (at 3.81 -2.413 90) (layer B.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at 2.54 2.413 90) (layer B.Fab))
    (pad 8 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 3 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 9 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 2 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 10 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 1 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 20 3V3))
    (pad "" np_thru_hole circle (at 7.62 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 7 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 6 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 5 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 4 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 "/USB Input/MSP430_TCK"))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.25 99.375 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C820 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(AE802-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.805 102.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C806 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 126.96 88.76 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C603 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value "10 uF" (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 120.48 93 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 135.17 93.035 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C507 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 135.08 130.2 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J201 (at 0 -5.8 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.95 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (pad 2 smd roundrect (at 1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad MP smd roundrect (at -3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at 3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.step
      (offset (xyz -1 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 113.4 80.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R405 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 129.13 80.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D406 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 129.12 80.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R406 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 ~CHG))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 107.48 87.8 270)
    (fp_text reference J801 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 1 smd rect (at 1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C818-Pad2)"))
    (pad 2 smd rect (at 0 -1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 136.82 104.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C505 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0.47U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 107.38 107.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H104 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 116.9 80.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R404 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 126.05 80.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R403 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.41 80.6)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D405 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.535 92.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(R601-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 123.14 80.57)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R402 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 120.25 80.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R401 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 137.38 82.56)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H101 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 112.63 100.5 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C801 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.855 101.125 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C802 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 128.23 89.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R603 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 128.05 90.75)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U502 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value BQ21040 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R506-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 ~CHG))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 129.49 93.7)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D201 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 129.685 89.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 129.585 92.7 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.95 91.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R506 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(R506-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 138.68 104.74)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C502 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 10U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.055 80.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D403 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 129.685 88.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "100 pF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 125.975 93.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R805 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 123.145 80.58)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D402 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 118.88 91.9 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C809 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 120.25 80.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D401 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 131.88 107.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R511 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.28 98.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 125.965 92.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R804 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.47 90.665 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1006 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 INT_LIS2DE12_2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.96 89.22 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R501 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(P501-PadB5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 114.725 103.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.28 128.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 133.755 105.55 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L501 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 121.5 97.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C810 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "22 uF" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Palconn_UTC16-G (layer F.Cu) (tedit 5CF432E0)
    (at 135.5 90.3 90)
    (descr http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf)
    (tags "USB C Type-C Receptacle USB2.0")
    (attr smd)
    (fp_text reference P501 (at 0 -4.58 90) (layer F.SilkS) hide)
    (fp_text value USB_C_Plug_USB2.0 (at 0 6.24 90) (layer F.Fab))
    (fp_text user %R (at 0 1.18 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.43 90) (layer Dwgs.User))
    (pad S1 thru_hole oval (at -4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B7 smd rect (at -0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A6 smd rect (at -0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 91 "/USB Input/D_P"))
    (pad A7 smd rect (at 0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 90 "/USB Input/D_N"))
    (pad B8 smd rect (at -1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at -1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P501-PadA5)"))
    (pad A8 smd rect (at 1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad B6 smd rect (at 0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad B5 smd rect (at 1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(P501-PadB5)"))
    (pad "" np_thru_hole circle (at 2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad A4 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B9 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A1 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B12 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B4 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B1 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A12 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/1054500101.stp
      (offset (xyz 0 -0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Package_LGA:LGA-12_2x2mm_P0.5mm (layer F.Cu) (tedit 5A0AAFFD)
    (at 116.01 88.69 180)
    (descr LGA12)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U1004 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value LIS2DE12 (at 0 1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 12 smd rect (at -0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 99 INT_LIS2DE12_2))
    (pad 6 smd rect (at 0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 1 smd rect (at -0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 7 smd rect (at 0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 8 smd rect (at 0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 3 smd rect (at -0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 2 smd rect (at -0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 121.68 95.9)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L802 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.36 88.01)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F501 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value Polyfuse (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.055 110.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D403 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 116.4 91.3 180)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y802 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Crystal_GND2 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U801-Pad47)"))
    (pad 2 smd rect (at 0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U801-Pad46)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.21 117.74)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1004 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(R1004-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 114.725 133.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 118.88 121.9 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C809 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 120.25 110.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R401 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 137.38 112.56)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H101 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 112.63 130.5 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C801 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.855 131.125 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C802 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 128.23 119.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R603 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 128.05 120.75)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U502 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value BQ21040 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 ~CHG))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R506-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 129.685 119.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 129.585 122.7 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.95 121.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R506 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(R506-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 133.955 106.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C501 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 130.4 95.99 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R505 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 133.255 112.75 270)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW901 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 1 smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 107.325 129.625 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C821 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C821-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.21 87.74)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1004 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(R1004-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 124.025 95.1 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C804 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 116.28 93.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C808 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 138.68 134.74)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C502 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 10U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 123.14 110.57)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R402 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:X2SON-8_1.4x1mm_P0.35mm (layer B.Cu) (tedit 5A02F1D8)
    (at 116.63 89.85 180)
    (descr "X2SON-8 1.4x1mm Pitch0.35mm http://www.ti.com/lit/ds/symlink/pca9306.pdf")
    (tags "X2SON-8 1.4x1mm Pitch0.35mm")
    (attr smd)
    (fp_text reference U1002 (at 0 2) (layer B.SilkS) hide)
    (fp_text value SN74AUP2G32 (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 8 smd rect (at 0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 19 VDDS))
    (pad 7 smd rect (at 0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 6 smd rect (at 0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 5 smd rect (at 0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 94 INT_SENSOR))
    (pad 2 smd rect (at -0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd rect (at -0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 95 INT_HDC2010))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 110.9 102.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference AE802 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(AE802-Pad1)"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 115.39 87.76 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1005 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(R1005-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:RFECA3216060A1T (layer F.Cu) (tedit 5E42DF6C)
    (at 106.28 124 270)
    (fp_text reference AE801 (at 0 1.85 90) (layer F.SilkS) hide)
    (fp_text value Antenna_Dipole (at 0.05 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at 1.4 -0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AE801-Pad1)"))
    (pad 2 smd rect (at 1.4 0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.4 0 270) (size 0.35 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(AE801-Pad3)"))
    (model ${KIPRJMOD}/mech/2450AT18D0100.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 137.38 107.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H102 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 134.68 119.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R504 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 "/USB Input/D_P"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.65 124.12 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C819 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(AE801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 130.44 132.43 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C503 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:BeagleBoard.org-20mm (layer B.Cu) (tedit 0)
    (at 107.38 125.3 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 115.39 117.76 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1005 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.21 118.29 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1002 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 110.99 93.44 315)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L803 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2 nH" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 114.725 101.525)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 137.905 118.875 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference D502 (at 0 2.9 270) (layer B.SilkS) hide)
    (fp_text value TPD2E001 (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 90 "/USB Input/D_N"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 91 "/USB Input/D_P"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 79 "/USB Input/VBUS"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 109.2 127.3 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L804 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 127.295 118.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C509 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 118.63 88.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1002 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 114.725 130.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R810 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 114.725 102.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 134.68 89.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R504 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 "/USB Input/D_P"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.65 94.12 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C819 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(AE801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 114.725 129.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R809 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R809-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 130.45 98.65 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R510 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 118.63 120.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1007 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 INT_OPT3001))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 114.725 100.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R810 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 118.63 90.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1007 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 INT_OPT3001))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 139.39 125.09 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C506 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.97 120.16 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C508 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 114.725 131.525)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 118.63 118.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1002 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 121.525 132.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 139.39 95.09 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C506 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 110.9 132.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference AE802 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(AE802-Pad1)"))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.97 90.16 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C508 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 114.725 99.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R809 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R809-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.14 123.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F801 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value Polyfuse (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 123.68 121.11 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1008 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(R1008-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 121.525 102.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 130.44 102.43 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C503 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 114.725 132.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 115.23 89.33 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1003 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(R1003-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.62 97.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C812 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:X2SON-8_1.4x1mm_P0.35mm (layer B.Cu) (tedit 5A02F1D8)
    (at 116.63 119.85 180)
    (descr "X2SON-8 1.4x1mm Pitch0.35mm http://www.ti.com/lit/ds/symlink/pca9306.pdf")
    (tags "X2SON-8 1.4x1mm Pitch0.35mm")
    (attr smd)
    (fp_text reference U1002 (at 0 2) (layer B.SilkS) hide)
    (fp_text value SN74AUP2G32 (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 95 INT_HDC2010))
    (pad 2 smd rect (at -0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 3 smd rect (at -0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 94 INT_SENSOR))
    (pad 4 smd rect (at -0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 7 smd rect (at 0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 8 smd rect (at 0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD locked (layer F.Cu) (tedit 5E541D62)
    (at 120.68 95.6 90)
    (fp_text reference J701 (at -0.074182 -1.275144 90) (layer F.SilkS) hide)
    (fp_text value mikroBUS (at -0.074182 -0.005144 90) (layer F.Fab))
    (fp_text user %R (at 11.43 0 180) (layer F.Fab))
    (fp_text user %R (at 11.355818 -0.005144 180) (layer F.Fab) hide)
    (pad 10 smd rect (at 13.08 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 12 smd rect (at 13.08 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 14 smd rect (at 13.08 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 45 CC1352_TX_MB1_RX))
    (pad 16 smd rect (at 13.08 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM_MB1))
    (pad 9 smd rect (at 9.78 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 9.78 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 13 smd rect (at 9.78 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 47 CC1352_RX_MB1_TX))
    (pad 15 smd rect (at 9.78 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 48 INT_MB1))
    (pad 8 smd rect (at -13.08 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -13.08 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 38 MOSI))
    (pad 2 smd rect (at -13.08 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 49 RST_MB1))
    (pad 1 smd rect (at -9.78 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 50 AN_MB1))
    (pad 4 smd rect (at -13.08 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at -9.78 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 20 3V3))
    (pad 3 smd rect (at -9.78 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 51 CS_MB1))
    (pad 5 smd rect (at -9.78 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 33 MISO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.14 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F801 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value Polyfuse (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 137.38 137.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H102 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module leash:MikroBus-SMD locked (layer F.Cu) (tedit 5E541D62)
    (at 120.68 125.6 90)
    (fp_text reference J701 (at -0.074182 -1.275144 90) (layer F.SilkS) hide)
    (fp_text value mikroBUS (at -0.074182 -0.005144 90) (layer F.Fab))
    (fp_text user %R (at 11.355818 -0.005144 180) (layer F.Fab) hide)
    (fp_text user %R (at 11.43 0 180) (layer F.Fab))
    (pad 5 smd rect (at -9.78 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -9.78 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 51 CS_MB1))
    (pad 7 smd rect (at -9.78 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 20 3V3))
    (pad 4 smd rect (at -13.08 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 35 SCK))
    (pad 1 smd rect (at -9.78 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 50 AN_MB1))
    (pad 2 smd rect (at -13.08 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 49 RST_MB1))
    (pad 6 smd rect (at -13.08 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 38 MOSI))
    (pad 8 smd rect (at -13.08 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 9.78 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 48 INT_MB1))
    (pad 13 smd rect (at 9.78 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 47 CC1352_RX_MB1_TX))
    (pad 11 smd rect (at 9.78 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 9 smd rect (at 9.78 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 13.08 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM_MB1))
    (pad 14 smd rect (at 13.08 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 45 CC1352_TX_MB1_RX))
    (pad 12 smd rect (at 13.08 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 13.08 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 117.28 87.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1001 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:BeagleBoard.org-20mm (layer B.Cu) (tedit 0)
    (at 107.38 95.3 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 117.28 117.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1001 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:USON6 (layer B.Cu) (tedit 5E4DAB76)
    (at 121.16 91.09 180)
    (fp_text reference U1003 (at 0.11 -3.68) (layer B.SilkS) hide)
    (fp_text value OPT3001 (at -0.16 3.7) (layer B.Fab))
    (pad 7 thru_hole circle (at 0 -0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 smd rect (at 0 0 180) (size 0.65 1.35) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.02))
    (pad 6 smd roundrect (at 0.95 0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 41 SDA) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at 0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 100 INT_OPT3001) (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at 0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 44 SCL) (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 101 "Net-(R1008-Pad2)") (solder_mask_margin 0.07))
    (pad 1 smd roundrect (at -0.95 0.675 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 19 VDDS) (solder_mask_margin 0.07))
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 137.905 88.875 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference D502 (at 0 2.9 270) (layer B.SilkS) hide)
    (fp_text value TPD2E001 (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 91 "/USB Input/D_P"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 90 "/USB Input/D_N"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer F.Cu) (tedit 5E4C72AA)
    (at 128.4 125.5 270)
    (attr virtual)
    (fp_text reference J301 (at 0.302285 2.603303 270) (layer F.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at -0.967715 -2.222697 270) (layer F.Fab))
    (pad 8 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 29 CC1352_TDI))
    (pad 3 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 9 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 30 CC1352_TMS))
    (pad 10 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 17 RESET_N))
    (pad 1 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 20 3V3))
    (pad 7 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 6 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 31 CC1352_TDO))
    (pad 5 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 32 CC1352_TCK))
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 110.99 123.44 315)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L803 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2 nH" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.95 92.05 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R502 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(P501-PadA5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer B.Cu) (tedit 5A0FD1B2)
    (at 137.805 122.475)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y501 (at 0 2.45) (layer B.SilkS) hide)
    (fp_text value 24MHz (at 0 -2.45) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 "/USB Input/XTAL1"))
    (pad 2 smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 "/USB Input/XTAL2"))
    (pad 4 smd rect (at -1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 107.325 99.625 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C821 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C821-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:USON6 (layer B.Cu) (tedit 5E4DAB76)
    (at 121.16 121.09 180)
    (fp_text reference U1003 (at 0.11 -3.68) (layer B.SilkS) hide)
    (fp_text value OPT3001 (at -0.16 3.7) (layer B.Fab))
    (pad 1 smd roundrect (at -0.95 0.675 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 19 VDDS) (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 101 "Net-(R1008-Pad2)") (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at 0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 44 SCL) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at 0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 100 INT_OPT3001) (solder_mask_margin 0.07))
    (pad 6 smd roundrect (at 0.95 0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 41 SDA) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 0 0 180) (size 0.65 1.35) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 -0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 127.295 88.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C509 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.21 88.29 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1002 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.62 67.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C812 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 139.39 65.09 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C506 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 134.68 59.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R504 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 "/USB Input/D_P"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 114.725 72.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 114.725 70.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R810 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 114.725 69.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R809 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R809-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 114.725 71.525)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 110.99 63.44 315)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L803 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2 nH" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 107.85 67.95 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C817 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "5.6 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.875 65.925 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C815 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2.7 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 110.3 62.1 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C816 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.21 57.74)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1004 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(R1004-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 130.4 65.99 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R505 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 135.08 70.2 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J201 (at 0 -5.8 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.95 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (pad 2 smd roundrect (at 1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad MP smd roundrect (at -3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at 3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.step
      (offset (xyz -1 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 115.39 57.76 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1005 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.38 72.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C805 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 119.58 58.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1001 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer B.Cu) (tedit 5A0FD1B2)
    (at 137.805 92.475)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y501 (at 0 2.45) (layer B.SilkS) hide)
    (fp_text value 24MHz (at 0 -2.45) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 4 smd rect (at -1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 "/USB Input/XTAL2"))
    (pad 2 smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 "/USB Input/XTAL1"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 130.44 70.55 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R509 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 135.17 63.035 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C507 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 111.825 66.175 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C813 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.25 69.375 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C820 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(AE802-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.805 72.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C806 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 133.955 76.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C501 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 119.6 72.925 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 138.68 74.74)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C502 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 10U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.96 59.22 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R501 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(P501-PadB5)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 122.475 72.95 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer B.Cu) (tedit 5D409D35)
    (at 128.4 65.5 270)
    (attr virtual)
    (fp_text reference J501 (at 3.81 -2.413 90) (layer B.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at 2.54 2.413 90) (layer B.Fab))
    (pad 8 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 3 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 9 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 2 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 10 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 1 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 20 3V3))
    (pad "" np_thru_hole circle (at 7.62 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 7 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 6 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 5 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 4 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 "/USB Input/MSP430_TCK"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 115.23 59.33 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1003 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(R1003-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 118.63 58.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1002 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.14 63.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F801 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value Polyfuse (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 117.28 57.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1001 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:BeagleBoard.org-20mm (layer B.Cu) (tedit 0)
    (at 107.38 65.3 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module leash:HDC2010 (layer F.Cu) (tedit 5E4D6772)
    (at 118.58 58.95)
    (fp_text reference U1001 (at -0.025 2.025) (layer F.SilkS) hide)
    (fp_text value HDC2010 (at 0 -3.8) (layer F.Fab))
    (pad A2 smd circle (at 0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA) (solder_mask_margin 0.05))
    (pad B2 smd circle (at 0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL) (solder_mask_margin 0.05))
    (pad C2 smd circle (at 0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 95 INT_HDC2010) (solder_mask_margin 0.05))
    (pad C1 smd circle (at -0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad B1 smd circle (at -0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R1004-Pad1)") (solder_mask_margin 0.05))
    (pad A1 smd circle (at -0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS) (solder_mask_margin 0.05))
  )
  (module leash:USON6 (layer B.Cu) (tedit 5E4DAB76)
    (at 121.16 61.09 180)
    (fp_text reference U1003 (at 0.11 -3.68) (layer B.SilkS) hide)
    (fp_text value OPT3001 (at -0.16 3.7) (layer B.Fab))
    (pad 1 smd roundrect (at -0.95 0.675 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 19 VDDS) (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 101 "Net-(R1008-Pad2)") (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at 0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 44 SCL) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at 0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 100 INT_OPT3001) (solder_mask_margin 0.07))
    (pad 6 smd roundrect (at 0.95 0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 41 SDA) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 0 0 180) (size 0.65 1.35) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 -0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 121.525 72.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.95 62.05 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R502 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(P501-PadA5)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 107.325 69.625 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C821 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C821-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.21 58.29 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1002 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 109.2 67.3 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L804 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:X2SON-8_1.4x1mm_P0.35mm (layer B.Cu) (tedit 5A02F1D8)
    (at 116.63 59.85 180)
    (descr "X2SON-8 1.4x1mm Pitch0.35mm http://www.ti.com/lit/ds/symlink/pca9306.pdf")
    (tags "X2SON-8 1.4x1mm Pitch0.35mm")
    (attr smd)
    (fp_text reference U1002 (at 0 2) (layer B.SilkS) hide)
    (fp_text value SN74AUP2G32 (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 95 INT_HDC2010))
    (pad 2 smd rect (at -0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 3 smd rect (at -0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 94 INT_SENSOR))
    (pad 4 smd rect (at -0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 7 smd rect (at 0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 8 smd rect (at 0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer F.Cu) (tedit 5E4C72AA)
    (at 128.4 65.5 270)
    (attr virtual)
    (fp_text reference J301 (at 0.302285 2.603303 270) (layer F.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at -0.967715 -2.222697 270) (layer F.Fab))
    (pad 8 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 29 CC1352_TDI))
    (pad 3 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 9 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 30 CC1352_TMS))
    (pad 10 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 17 RESET_N))
    (pad 1 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 20 3V3))
    (pad 7 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 6 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 31 CC1352_TDO))
    (pad 5 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 32 CC1352_TCK))
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer B.Cu) (tedit 5A0FD1B2)
    (at 137.805 62.475)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y501 (at 0 2.45) (layer B.SilkS) hide)
    (fp_text value 24MHz (at 0 -2.45) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 "/USB Input/XTAL1"))
    (pad 2 smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 "/USB Input/XTAL2"))
    (pad 4 smd rect (at -1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 130.45 68.65 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R510 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 127.295 58.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C509 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 118.63 60.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1007 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 INT_OPT3001))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 120.55 72.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 135.655 59.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R503 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 90 "/USB Input/D_N"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 133.255 52.75 270)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW901 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 1 smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.65 64.12 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C819 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(AE801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 137.905 58.875 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference D502 (at 0 2.9 270) (layer B.SilkS) hide)
    (fp_text value TPD2E001 (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 90 "/USB Input/D_N"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 91 "/USB Input/D_P"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 79 "/USB Input/VBUS"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm (layer F.Cu) (tedit 5C26A111)
    (at 120.13 67.44)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U801 (at 0 -4.82) (layer F.SilkS) hide)
    (fp_text value CC1352R (at 0 4.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 49 smd roundrect (at 0 0) (size 5.15 5.15) (layers F.Cu F.Mask) (roundrect_rratio 0.048544)
      (net 1 GND))
    (pad "" smd roundrect (at -1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad 1 smd roundrect (at -3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 2 smd roundrect (at -3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 3 smd roundrect (at -3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 4 smd roundrect (at -3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 5 smd roundrect (at -3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 6 smd roundrect (at -3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 7 smd roundrect (at -3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 8 smd roundrect (at -3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 9 smd roundrect (at -3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 10 smd roundrect (at -3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 RST_MB2))
    (pad 11 smd roundrect (at -3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 RST_MB1))
    (pad 12 smd roundrect (at -3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 INT_SENSOR))
    (pad 13 smd roundrect (at -2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 14 smd roundrect (at -2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 15 smd roundrect (at -1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 16 smd roundrect (at -1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 17 smd roundrect (at -0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 18 smd roundrect (at -0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 CS_MB2))
    (pad 19 smd roundrect (at 0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 CS_MB1))
    (pad 20 smd roundrect (at 0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 21 smd roundrect (at 1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 22 smd roundrect (at 1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 23 smd roundrect (at 2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 24 smd roundrect (at 2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 CC1352_TMS))
    (pad 25 smd roundrect (at 3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 CC1352_TCK))
    (pad 26 smd roundrect (at 3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 CC1352_TDO))
    (pad 27 smd roundrect (at 3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 CC1352_TDI))
    (pad 28 smd roundrect (at 3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 29 smd roundrect (at 3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 PWM_MB2))
    (pad 30 smd roundrect (at 3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 INT_MB2))
    (pad 31 smd roundrect (at 3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 32 smd roundrect (at 3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 33 smd roundrect (at 3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 34 smd roundrect (at 3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 35 smd roundrect (at 3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 36 smd roundrect (at 3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 AN_MB1))
    (pad 37 smd roundrect (at 2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 AN_MB2))
    (pad 38 smd roundrect (at 2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 39 smd roundrect (at 1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 40 smd roundrect (at 1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 41 smd roundrect (at 0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 42 smd roundrect (at 0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 INT_MB1))
    (pad 43 smd roundrect (at -0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 PWM_MB1))
    (pad 44 smd roundrect (at -0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 45 smd roundrect (at -1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 46 smd roundrect (at -1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U801-Pad46)"))
    (pad 47 smd roundrect (at -2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U801-Pad47)"))
    (pad 48 smd roundrect (at -2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 130.97 60.16 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C508 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.62 127.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C812 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 116.28 123.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C808 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:RFECA3216060A1T (layer F.Cu) (tedit 5E42DF6C)
    (at 106.28 64 270)
    (fp_text reference AE801 (at 0 1.85 90) (layer F.SilkS) hide)
    (fp_text value Antenna_Dipole (at 0.05 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at 1.4 -0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AE801-Pad1)"))
    (pad 2 smd rect (at 1.4 0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.4 0 270) (size 0.35 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(AE801-Pad3)"))
    (model ${KIPRJMOD}/mech/2450AT18D0100.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 137.38 77.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H102 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 123.68 61.11 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1008 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(R1008-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer F.Cu) (tedit 5E4C72AA)
    (at 128.4 95.5 270)
    (attr virtual)
    (fp_text reference J301 (at 0.302285 2.603303 270) (layer F.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at -0.967715 -2.222697 270) (layer F.Fab))
    (pad 4 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 32 CC1352_TCK))
    (pad 5 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 31 CC1352_TDO))
    (pad 7 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 1 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 20 3V3))
    (pad 10 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 17 RESET_N))
    (pad 2 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 30 CC1352_TMS))
    (pad 9 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 3 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 8 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 29 CC1352_TDI))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 123.68 91.11 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1008 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(R1008-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.41 110.6)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D405 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 126.05 110.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R403 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 122.05 118.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R803 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 CC1352_RX_MB2_TX))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 129.685 118.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "100 pF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N48_EP5.15x5.15mm (layer B.Cu) (tedit 5E4C745D)
    (at 135.05 130.15 180)
    (descr "QFN, 48 Pin (http://www.ti.com/lit/ds/symlink/msp430f5232.pdf#page=112), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U501 (at 0 4.82) (layer B.SilkS) hide)
    (fp_text value MSP430F5500IRGZ (at 0 -4.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 49 smd roundrect (at 0 0 180) (size 5.15 5.15) (layers B.Cu B.Mask) (roundrect_rratio 0.049)
      (net 1 GND))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad 1 smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 8 smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 12 smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 13 smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 14 smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 15 smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 16 smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 17 smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 18 smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 19 smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 20 smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 21 smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 22 smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 23 smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 24 smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 25 smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 26 smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 27 smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 28 smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 29 smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 30 smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 31 smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 32 smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 33 smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 34 smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 35 smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 36 smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 37 smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 38 smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 39 smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 40 smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 41 smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 42 smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 43 smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 44 smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 45 smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 46 smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 47 smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 48 smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 "/USB Input/MSP430_RST_N"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N48_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:0900PC15A0036 (layer F.Cu) (tedit 5E41EA1D)
    (at 114.14 125.44 270)
    (fp_text reference B801 (at 0.025 4.2 90) (layer F.SilkS) hide)
    (fp_text value 0900PC15A0036E (at -0.05 -3.025 90) (layer F.Fab))
    (pad 4 smd roundrect (at 0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (pad 3 smd roundrect (at 0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 6 smd roundrect (at 0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 7 smd roundrect (at 0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 8 smd roundrect (at -0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 9 smd roundrect (at -0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 5 smd roundrect (at 1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 10 smd roundrect (at -1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/0900PC15J0013.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 107.38 112.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H103 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module leash:MikroBus-SMD (layer B.Cu) (tedit 5E541D54)
    (at 120.6 125.6 90)
    (fp_text reference J702 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value mikroBUS (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at 11.43 0) (layer B.Fab))
    (fp_text user %R (at -11.43 0) (layer B.Fab))
    (pad 10 smd rect (at 13.08 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 28 5V))
    (pad 12 smd rect (at 13.08 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 44 SCL))
    (pad 14 smd rect (at 13.08 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 43 CC1352_TX_MB2_RX))
    (pad 16 smd rect (at 13.08 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 42 PWM_MB2))
    (pad 9 smd rect (at 9.78 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 9.78 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 41 SDA))
    (pad 13 smd rect (at 9.78 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 40 CC1352_RX_MB2_TX))
    (pad 15 smd rect (at 9.78 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 39 INT_MB2))
    (pad 8 smd rect (at -13.08 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -13.08 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 2 smd rect (at -13.08 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 37 RST_MB2))
    (pad 1 smd rect (at -9.78 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 36 AN_MB2))
    (pad 4 smd rect (at -13.08 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at -9.78 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 20 3V3))
    (pad 3 smd rect (at -9.78 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 34 CS_MB2))
    (pad 5 smd rect (at -9.78 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 132.63 112.575 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D501 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 112.32 124.11 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C814 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:L_0806_2012Metric (layer B.Cu) (tedit 5D2F3EE6)
    (at 132.985 119.9 90)
    (descr "Inductor SMD 0806 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L601 (at 0 1.65 90) (layer B.SilkS) hide)
    (fp_text value INDUCTOR (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(L601-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 124.43 118.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R802 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 CC1352_TX_MB2_RX))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 123.38 132.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C803 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 137 125.57 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C504 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 220N (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 133.98 137.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R507 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 106.28 121.315 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C822 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(AE801-Pad3)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 130.44 130.55 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R509 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 122.38 132.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C805 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 107.25 132.85 90)
    (fp_text reference J802 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 4 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C821-Pad2)"))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 108.88 121.4 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C818 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C818-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.505 118.3 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R604 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 107.85 127.95 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C817 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "5.6 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 119.58 118.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1001 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:TPS62821DLC (layer B.Cu) (tedit 5D2676FA)
    (at 130.885 121.1)
    (fp_text reference U601 (at 0.1 1.975 180) (layer B.SilkS) hide)
    (fp_text value TPS62821DLC (at 0 0.5 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 2 smd roundrect (at -0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(C602-Pad2)"))
    (pad 3 smd roundrect (at -0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 4 smd roundrect (at -0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2))
    (pad 5 smd roundrect (at 0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 6 smd roundrect (at 0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 73 "Net-(L601-Pad1)"))
    (pad 7 smd roundrect (at 0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 8 smd roundrect (at 0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 74 "Net-(R601-Pad1)"))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1.3 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.875 125.925 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C815 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2.7 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 120.55 132.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 135.655 119.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R503 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 90 "/USB Input/D_N"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:HDC2010 (layer F.Cu) (tedit 5E4D6772)
    (at 118.58 118.95)
    (fp_text reference U1001 (at -0.025 2.025) (layer F.SilkS) hide)
    (fp_text value HDC2010 (at 0 -3.8) (layer F.Fab))
    (pad A2 smd circle (at 0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA) (solder_mask_margin 0.05))
    (pad B2 smd circle (at 0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL) (solder_mask_margin 0.05))
    (pad C2 smd circle (at 0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 95 INT_HDC2010) (solder_mask_margin 0.05))
    (pad C1 smd circle (at -0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad B1 smd circle (at -0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R1004-Pad1)") (solder_mask_margin 0.05))
    (pad A1 smd circle (at -0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS) (solder_mask_margin 0.05))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 122.475 132.95 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.25 129.375 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C820 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(AE802-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 126.96 118.76 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C603 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value "10 uF" (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 120.48 123 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 135.17 123.035 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C507 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 113.4 110.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R405 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 129.13 110.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D406 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 129.12 110.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R406 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 ~CHG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 107.48 117.8 270)
    (fp_text reference J801 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 4 smd rect (at 0 1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C818-Pad2)"))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 136.82 134.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C505 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0.47U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 107.38 137.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H104 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 116.9 110.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R404 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:RFECA3216060A1T (layer F.Cu) (tedit 5E42DF6C)
    (at 106.28 94 270)
    (fp_text reference AE801 (at 0 1.85 90) (layer F.SilkS) hide)
    (fp_text value Antenna_Dipole (at 0.05 -1.7 90) (layer F.Fab))
    (pad 3 smd rect (at -1.4 0 270) (size 0.35 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(AE801-Pad3)"))
    (pad 2 smd rect (at 1.4 0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.4 -0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AE801-Pad1)"))
    (model ${KIPRJMOD}/mech/2450AT18D0100.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 115.23 119.33 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1003 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(R1003-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 113.755 99.575 315)
    (descr "SMD Crystal 2012/2 http://txccrystal.com/images/pdf/9ht11.pdf, 2.0x1.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y801 (at 0 -1.8 135) (layer F.SilkS) hide)
    (fp_text value Crystal (at 0 1.8 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C802-Pad1)"))
    (pad 1 smd rect (at -0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C801-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_AX_8045-2Pin_8.0x4.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.25 0.3 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm (layer F.Cu) (tedit 5C26A111)
    (at 120.13 97.44)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U801 (at 0 -4.82) (layer F.SilkS) hide)
    (fp_text value CC1352R (at 0 4.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 48 smd roundrect (at -2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 47 smd roundrect (at -2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U801-Pad47)"))
    (pad 46 smd roundrect (at -1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U801-Pad46)"))
    (pad 45 smd roundrect (at -1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 44 smd roundrect (at -0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 43 smd roundrect (at -0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 PWM_MB1))
    (pad 42 smd roundrect (at 0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 INT_MB1))
    (pad 41 smd roundrect (at 0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 40 smd roundrect (at 1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 39 smd roundrect (at 1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 38 smd roundrect (at 2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 37 smd roundrect (at 2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 AN_MB2))
    (pad 36 smd roundrect (at 3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 AN_MB1))
    (pad 35 smd roundrect (at 3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 34 smd roundrect (at 3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 33 smd roundrect (at 3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 32 smd roundrect (at 3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 31 smd roundrect (at 3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 30 smd roundrect (at 3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 INT_MB2))
    (pad 29 smd roundrect (at 3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 PWM_MB2))
    (pad 28 smd roundrect (at 3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 27 smd roundrect (at 3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 CC1352_TDI))
    (pad 26 smd roundrect (at 3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 CC1352_TDO))
    (pad 25 smd roundrect (at 3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 CC1352_TCK))
    (pad 24 smd roundrect (at 2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 CC1352_TMS))
    (pad 23 smd roundrect (at 2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 22 smd roundrect (at 1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 21 smd roundrect (at 1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 20 smd roundrect (at 0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 19 smd roundrect (at 0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 CS_MB1))
    (pad 18 smd roundrect (at -0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 CS_MB2))
    (pad 17 smd roundrect (at -0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 16 smd roundrect (at -1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 15 smd roundrect (at -1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 14 smd roundrect (at -2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 13 smd roundrect (at -2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 12 smd roundrect (at -3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 INT_SENSOR))
    (pad 11 smd roundrect (at -3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 RST_MB1))
    (pad 10 smd roundrect (at -3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 RST_MB2))
    (pad 9 smd roundrect (at -3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 8 smd roundrect (at -3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 7 smd roundrect (at -3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 6 smd roundrect (at -3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 5 smd roundrect (at -3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 4 smd roundrect (at -3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 3 smd roundrect (at -3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 2 smd roundrect (at -3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 1 smd roundrect (at -3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad "" smd roundrect (at 1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad 49 smd roundrect (at 0 0) (size 5.15 5.15) (layers F.Cu F.Mask) (roundrect_rratio 0.048544)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD (layer B.Cu) (tedit 5E541D54)
    (at 120.6 65.6 90)
    (fp_text reference J702 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value mikroBUS (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at 11.43 0) (layer B.Fab))
    (fp_text user %R (at -11.43 0) (layer B.Fab))
    (pad 10 smd rect (at 13.08 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 28 5V))
    (pad 12 smd rect (at 13.08 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 44 SCL))
    (pad 14 smd rect (at 13.08 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 43 CC1352_TX_MB2_RX))
    (pad 16 smd rect (at 13.08 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 42 PWM_MB2))
    (pad 9 smd rect (at 9.78 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 9.78 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 41 SDA))
    (pad 13 smd rect (at 9.78 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 40 CC1352_RX_MB2_TX))
    (pad 15 smd rect (at 9.78 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 39 INT_MB2))
    (pad 8 smd rect (at -13.08 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -13.08 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 2 smd rect (at -13.08 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 37 RST_MB2))
    (pad 1 smd rect (at -9.78 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 36 AN_MB2))
    (pad 4 smd rect (at -13.08 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at -9.78 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 20 3V3))
    (pad 3 smd rect (at -9.78 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 34 CS_MB2))
    (pad 5 smd rect (at -9.78 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 133.18 107.25 90)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW902 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 1 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 2 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 130.45 128.65 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R510 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 136.82 74.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C505 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0.47U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 137 65.57 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C504 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 220N (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.84 65.49 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R508 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1.5K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 133.18 77.25 90)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW902 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 1 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 110.9 72.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference AE802 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(AE802-Pad1)"))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 106.28 61.315 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C822 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(AE801-Pad3)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 130.44 72.43 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C503 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 108.88 61.4 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C818 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C818-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 107.48 57.8 270)
    (fp_text reference J801 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 4 smd rect (at 0 1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C818-Pad2)"))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module leash:L_0806_2012Metric (layer B.Cu) (tedit 5D2F3EE6)
    (at 132.985 59.9 90)
    (descr "Inductor SMD 0806 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L601 (at 0 1.65 90) (layer B.SilkS) hide)
    (fp_text value INDUCTOR (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(L601-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 113.755 69.575 315)
    (descr "SMD Crystal 2012/2 http://txccrystal.com/images/pdf/9ht11.pdf, 2.0x1.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y801 (at 0 -1.8 135) (layer F.SilkS) hide)
    (fp_text value Crystal (at 0 1.8 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C801-Pad1)"))
    (pad 2 smd rect (at 0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_AX_8045-2Pin_8.0x4.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.25 0.3 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 116.4 61.3 180)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y802 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Crystal_GND2 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U801-Pad46)"))
    (pad 2 smd rect (at 0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U801-Pad47)"))
    (pad 4 smd rect (at -0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 126.25 65.625)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L801 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 132.63 52.575 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D501 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 122.05 58.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R803 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 CC1352_RX_MB2_TX))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 124.43 58.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R802 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 CC1352_TX_MB2_RX))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 107.25 72.85 90)
    (fp_text reference J802 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 4 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C821-Pad2)"))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module leash:MX25R8035FZUIL0 (layer B.Cu) (tedit 5E42FFC6)
    (at 116.775 71.08 270)
    (fp_text reference U802 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value MX25R8035FZUIL0 (at 0 -2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 109 ~FLASH_CS))
    (pad 2 smd rect (at -1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R809-Pad2)"))
    (pad 4 smd rect (at -1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 6 smd rect (at 1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at 1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 8 smd rect (at 1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C811-Pad2)"))
    (pad 9 smd custom (at 0 0 270) (size 0.2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0 0.8) (xy 0.1 0.8) (xy 0.1 -0.8) (xy -0.1 -0.8) (xy -0.1 0.7)
) (width 0))
      ))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:TPS62821DLC (layer B.Cu) (tedit 5D2676FA)
    (at 130.885 61.1)
    (fp_text reference U601 (at 0.1 1.975 180) (layer B.SilkS) hide)
    (fp_text value TPS62821DLC (at 0 0.5 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 2 smd roundrect (at -0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(C602-Pad2)"))
    (pad 3 smd roundrect (at -0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 4 smd roundrect (at -0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2))
    (pad 5 smd roundrect (at 0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 6 smd roundrect (at 0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 73 "Net-(L601-Pad1)"))
    (pad 7 smd roundrect (at 0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 8 smd roundrect (at 0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 74 "Net-(R601-Pad1)"))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1.3 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 126.96 58.76 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C603 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value "10 uF" (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 112.32 64.11 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C814 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 114.725 73.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 121.5 67.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C810 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "22 uF" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 118.88 61.9 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C809 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 116.28 63.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C808 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 120.48 63 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 124.025 65.1 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C804 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 123.38 72.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C803 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 109.2 97.3 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L804 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.36 58.01)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F501 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value Polyfuse (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.47 60.665 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1006 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 INT_LIS2DE12_2))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LGA:LGA-12_2x2mm_P0.5mm (layer F.Cu) (tedit 5A0AAFFD)
    (at 116.01 58.69 180)
    (descr LGA12)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U1004 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value LIS2DE12 (at 0 1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at -0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 9 smd rect (at 0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 8 smd rect (at 0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 7 smd rect (at 0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 5 smd rect (at -0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 99 INT_LIS2DE12_2))
    (pad 12 smd rect (at -0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 131.88 77.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R511 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 133.98 77.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R507 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 133.755 75.55 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L501 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Palconn_UTC16-G (layer F.Cu) (tedit 5CF432E0)
    (at 135.5 60.3 90)
    (descr http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf)
    (tags "USB C Type-C Receptacle USB2.0")
    (attr smd)
    (fp_text reference P501 (at 0 -4.58 90) (layer F.SilkS) hide)
    (fp_text value USB_C_Plug_USB2.0 (at 0 6.24 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.43 90) (layer Dwgs.User))
    (fp_text user %R (at 0 1.18 90) (layer F.Fab))
    (pad A12 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B1 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B4 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B12 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A1 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B9 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A4 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad "" np_thru_hole circle (at -2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad B5 smd rect (at 1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(P501-PadB5)"))
    (pad B6 smd rect (at 0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A8 smd rect (at 1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at -1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P501-PadA5)"))
    (pad B8 smd rect (at -1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A7 smd rect (at 0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 90 "/USB Input/D_N"))
    (pad A6 smd rect (at -0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 91 "/USB Input/D_P"))
    (pad B7 smd rect (at -0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad S1 thru_hole oval (at 4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/1054500101.stp
      (offset (xyz 0 -0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 107.38 52.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H103 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 107.38 77.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H104 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N48_EP5.15x5.15mm (layer B.Cu) (tedit 5E4C745D)
    (at 135.05 70.15 180)
    (descr "QFN, 48 Pin (http://www.ti.com/lit/ds/symlink/msp430f5232.pdf#page=112), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U501 (at 0 4.82) (layer B.SilkS) hide)
    (fp_text value MSP430F5500IRGZ (at 0 -4.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 49 smd roundrect (at 0 0 180) (size 5.15 5.15) (layers B.Cu B.Mask) (roundrect_rratio 0.049)
      (net 1 GND))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad 1 smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 8 smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 12 smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 13 smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 14 smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 15 smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 16 smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 17 smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 18 smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 19 smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 20 smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 21 smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 22 smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 23 smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 24 smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 25 smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 26 smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 27 smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 28 smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 29 smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 30 smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 31 smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 32 smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 33 smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 34 smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 35 smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 36 smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 37 smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 38 smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 39 smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 40 smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 41 smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 42 smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 43 smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 44 smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 45 smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 46 smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 47 smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 48 smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 "/USB Input/MSP430_RST_N"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N48_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:0900PC15A0036 (layer F.Cu) (tedit 5E41EA1D)
    (at 114.14 65.44 270)
    (fp_text reference B801 (at 0.025 4.2 90) (layer F.SilkS) hide)
    (fp_text value 0900PC15A0036E (at -0.05 -3.025 90) (layer F.Fab))
    (pad 4 smd roundrect (at 0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (pad 3 smd roundrect (at 0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 6 smd roundrect (at 0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 7 smd roundrect (at 0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 8 smd roundrect (at -0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 9 smd roundrect (at -0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 5 smd roundrect (at 1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 10 smd roundrect (at -1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/0900PC15J0013.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 137.38 52.56)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H101 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 129.585 62.7 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.28 68.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 121.68 65.9)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L802 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 125.965 62.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R804 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 125.975 63.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R805 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.505 58.3 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R604 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 129.49 63.7)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D201 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.9 50.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D404 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.055 50.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D403 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 120.25 50.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D401 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 123.145 50.58)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D402 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 129.685 58.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "100 pF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 114.855 71.125 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C802 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 112.63 70.5 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C801 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 128.23 59.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R603 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 129.685 59.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 120.25 50.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R401 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 123.14 50.57)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R402 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.41 50.6)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D405 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 131.535 62.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(R601-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 113.4 50.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R405 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 116.9 50.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R404 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 126.05 50.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R403 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 128.05 60.75)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U502 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value BQ21040 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 ~CHG))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R506-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.95 61.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R506 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(R506-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 129.12 50.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R406 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 ~CHG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 129.13 50.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D406 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N48_EP5.15x5.15mm (layer B.Cu) (tedit 5E4C745D)
    (at 99.05 130.15 180)
    (descr "QFN, 48 Pin (http://www.ti.com/lit/ds/symlink/msp430f5232.pdf#page=112), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U501 (at 0 4.82) (layer B.SilkS) hide)
    (fp_text value MSP430F5500IRGZ (at 0 -4.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 48 smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 47 smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 46 smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 45 smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 44 smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 43 smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 42 smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 41 smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 40 smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 39 smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 38 smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 37 smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 36 smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 35 smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 34 smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 33 smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 32 smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 31 smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 30 smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 29 smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 28 smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 27 smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 26 smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 25 smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 24 smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 23 smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 22 smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 21 smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 20 smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 19 smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 18 smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 17 smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 16 smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 15 smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 14 smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 12 smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 10 smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 6 smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad 49 smd roundrect (at 0 0 180) (size 5.15 5.15) (layers B.Cu B.Mask) (roundrect_rratio 0.049)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N48_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:0900PC15A0036 (layer F.Cu) (tedit 5E41EA1D)
    (at 78.14 125.44 270)
    (fp_text reference B801 (at 0.025 4.2 90) (layer F.SilkS) hide)
    (fp_text value 0900PC15A0036E (at -0.05 -3.025 90) (layer F.Fab))
    (pad 10 smd roundrect (at -1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 smd roundrect (at 1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 9 smd roundrect (at -0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 8 smd roundrect (at -0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 7 smd roundrect (at 0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 6 smd roundrect (at 0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 1 smd roundrect (at -0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 2 smd roundrect (at -0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at 0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at 0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (model ${KIPRJMOD}/mech/0900PC15J0013.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 71.38 112.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H103 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module leash:MX25R8035FZUIL0 (layer B.Cu) (tedit 5E42FFC6)
    (at 80.775 131.08 270)
    (fp_text reference U802 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value MX25R8035FZUIL0 (at 0 -2 90) (layer B.Fab))
    (pad 9 smd custom (at 0 0 270) (size 0.2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0 0.8) (xy 0.1 0.8) (xy 0.1 -0.8) (xy -0.1 -0.8) (xy -0.1 0.7)
) (width 0))
      ))
    (pad 8 smd rect (at 1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C811-Pad2)"))
    (pad 7 smd rect (at 1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 6 smd rect (at 1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 5 smd rect (at 1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 4 smd rect (at -1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R809-Pad2)"))
    (pad 2 smd rect (at -1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 1 smd rect (at -1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 109 ~FLASH_CS))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 80.9 110.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D404 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 90.25 125.625)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L801 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD (layer B.Cu) (tedit 5E541D54)
    (at 84.6 125.6 90)
    (fp_text reference J702 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value mikroBUS (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at -11.43 0) (layer B.Fab))
    (fp_text user %R (at 11.43 0) (layer B.Fab))
    (pad 5 smd rect (at -9.78 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -9.78 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 34 CS_MB2))
    (pad 7 smd rect (at -9.78 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 20 3V3))
    (pad 4 smd rect (at -13.08 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 1 smd rect (at -9.78 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 36 AN_MB2))
    (pad 2 smd rect (at -13.08 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 37 RST_MB2))
    (pad 6 smd rect (at -13.08 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 8 smd rect (at -13.08 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 9.78 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 39 INT_MB2))
    (pad 13 smd rect (at 9.78 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 40 CC1352_RX_MB2_TX))
    (pad 11 smd rect (at 9.78 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 41 SDA))
    (pad 9 smd rect (at 9.78 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 13.08 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 42 PWM_MB2))
    (pad 14 smd rect (at 13.08 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 43 CC1352_TX_MB2_RX))
    (pad 12 smd rect (at 13.08 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 13.08 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 96.63 112.575 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D501 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 76.32 124.11 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C814 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:L_0806_2012Metric (layer B.Cu) (tedit 5D2F3EE6)
    (at 96.985 119.9 90)
    (descr "Inductor SMD 0806 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L601 (at 0 1.65 90) (layer B.SilkS) hide)
    (fp_text value INDUCTOR (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(L601-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 88.43 118.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R802 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 CC1352_TX_MB2_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 83.6 132.925 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer B.Cu) (tedit 5D409D35)
    (at 92.4 125.5 270)
    (attr virtual)
    (fp_text reference J501 (at 3.81 -2.413 90) (layer B.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at 2.54 2.413 90) (layer B.Fab))
    (pad 4 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 5 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 6 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 7 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 1 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 20 3V3))
    (pad 10 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 2 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 9 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 3 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 8 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 10 "/USB Input/MSP430_TDI"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 95.84 125.49 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R508 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1.5K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 75.825 126.175 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C813 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 74.3 122.1 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C816 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 86.05 118.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R803 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 CC1352_RX_MB2_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 87.38 132.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C803 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 101 125.57 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C504 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 220N (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 97.98 137.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R507 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 70.28 121.315 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C822 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(AE801-Pad3)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 94.44 130.55 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R509 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 86.38 132.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C805 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 71.25 132.85 90)
    (fp_text reference J802 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C821-Pad2)"))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 72.88 121.4 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C818 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C818-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 95.505 118.3 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R604 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 71.85 127.95 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C817 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "5.6 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 83.58 118.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1001 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:TPS62821DLC (layer B.Cu) (tedit 5D2676FA)
    (at 94.885 121.1)
    (fp_text reference U601 (at 0.1 1.975 180) (layer B.SilkS) hide)
    (fp_text value TPS62821DLC (at 0 0.5 180) (layer B.Fab))
    (pad 8 smd roundrect (at 0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 74 "Net-(R601-Pad1)"))
    (pad 7 smd roundrect (at 0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 6 smd roundrect (at 0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 73 "Net-(L601-Pad1)"))
    (pad 5 smd roundrect (at 0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 4 smd roundrect (at -0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2))
    (pad 3 smd roundrect (at -0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1.3 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 73.875 125.925 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C815 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2.7 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 84.55 132.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 97.255 112.75 270)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW901 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 1 smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 2 smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 99.08 130.2 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J201 (at 0 -5.8 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.95 90) (layer F.Fab) hide)
    (pad MP smd roundrect (at 3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at -3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad 2 smd roundrect (at 1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.step
      (offset (xyz -1 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 99.655 119.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R503 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 90 "/USB Input/D_N"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:HDC2010 (layer F.Cu) (tedit 5E4D6772)
    (at 82.58 118.95)
    (fp_text reference U1001 (at -0.025 2.025) (layer F.SilkS) hide)
    (fp_text value HDC2010 (at 0 -3.8) (layer F.Fab))
    (pad A1 smd circle (at -0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS) (solder_mask_margin 0.05))
    (pad B1 smd circle (at -0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R1004-Pad1)") (solder_mask_margin 0.05))
    (pad C1 smd circle (at -0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad C2 smd circle (at 0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 95 INT_HDC2010) (solder_mask_margin 0.05))
    (pad B2 smd circle (at 0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL) (solder_mask_margin 0.05))
    (pad A2 smd circle (at 0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA) (solder_mask_margin 0.05))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 86.475 132.95 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 73.25 129.375 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C820 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(AE802-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 80.805 132.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C806 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 90.96 118.76 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C603 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value "10 uF" (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 84.48 123 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 99.17 123.035 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C507 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 77.4 110.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R405 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 93.13 110.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D406 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 93.12 110.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R406 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 ~CHG))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 71.48 117.8 270)
    (fp_text reference J801 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 1 smd rect (at 1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C818-Pad2)"))
    (pad 2 smd rect (at 0 -1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 100.82 134.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C505 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0.47U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 71.38 137.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H104 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 80.9 110.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R404 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 90.05 110.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R403 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 77.41 110.6)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D405 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 95.535 122.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(R601-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 87.14 110.57)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R402 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 84.25 110.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R401 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 101.38 112.56)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H101 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 76.63 130.5 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C801 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 78.855 131.125 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C802 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 92.23 119.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R603 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 92.05 120.75)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U502 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value BQ21040 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R506-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 ~CHG))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 93.49 123.7)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D201 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 93.685 119.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 93.585 122.7 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.95 121.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R506 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(R506-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 102.68 134.74)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C502 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 10U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 90.055 110.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D403 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 93.685 118.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "100 pF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 89.975 123.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R805 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 87.145 110.58)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D402 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 82.88 121.9 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C809 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 84.25 110.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D401 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 95.88 137.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R511 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 90.28 128.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 89.965 122.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R804 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 78.47 120.665 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1006 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 INT_LIS2DE12_2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.96 119.22 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R501 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(P501-PadB5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 78.725 133.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 97.755 135.55 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L501 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 85.5 127.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C810 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "22 uF" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Palconn_UTC16-G (layer F.Cu) (tedit 5CF432E0)
    (at 99.5 120.3 90)
    (descr http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf)
    (tags "USB C Type-C Receptacle USB2.0")
    (attr smd)
    (fp_text reference P501 (at 0 -4.58 90) (layer F.SilkS) hide)
    (fp_text value USB_C_Plug_USB2.0 (at 0 6.24 90) (layer F.Fab))
    (fp_text user %R (at 0 1.18 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.43 90) (layer Dwgs.User))
    (pad S1 thru_hole oval (at -4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B7 smd rect (at -0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A6 smd rect (at -0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 91 "/USB Input/D_P"))
    (pad A7 smd rect (at 0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 90 "/USB Input/D_N"))
    (pad B8 smd rect (at -1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at -1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P501-PadA5)"))
    (pad A8 smd rect (at 1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad B6 smd rect (at 0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad B5 smd rect (at 1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(P501-PadB5)"))
    (pad "" np_thru_hole circle (at 2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad A4 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B9 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A1 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B12 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B4 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B1 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A12 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/1054500101.stp
      (offset (xyz 0 -0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Package_LGA:LGA-12_2x2mm_P0.5mm (layer F.Cu) (tedit 5A0AAFFD)
    (at 80.01 118.69 180)
    (descr LGA12)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U1004 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value LIS2DE12 (at 0 1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 12 smd rect (at -0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 99 INT_LIS2DE12_2))
    (pad 6 smd rect (at 0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 1 smd rect (at -0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 7 smd rect (at 0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 8 smd rect (at 0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 3 smd rect (at -0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 2 smd rect (at -0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 85.68 125.9)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L802 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.36 118.01)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F501 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value Polyfuse (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 80.4 121.3 180)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y802 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Crystal_GND2 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U801-Pad47)"))
    (pad 2 smd rect (at 0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U801-Pad46)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 97.955 136.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C501 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 94.4 125.99 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R505 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 83.21 117.74)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1004 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(R1004-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 88.025 125.1 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C804 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 80.28 123.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C808 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:X2SON-8_1.4x1mm_P0.35mm (layer B.Cu) (tedit 5A02F1D8)
    (at 80.63 119.85 180)
    (descr "X2SON-8 1.4x1mm Pitch0.35mm http://www.ti.com/lit/ds/symlink/pca9306.pdf")
    (tags "X2SON-8 1.4x1mm Pitch0.35mm")
    (attr smd)
    (fp_text reference U1002 (at 0 2) (layer B.SilkS) hide)
    (fp_text value SN74AUP2G32 (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 8 smd rect (at 0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 19 VDDS))
    (pad 7 smd rect (at 0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 6 smd rect (at 0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 5 smd rect (at 0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 94 INT_SENSOR))
    (pad 2 smd rect (at -0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd rect (at -0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 95 INT_HDC2010))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 74.9 132.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference AE802 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(AE802-Pad1)"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 79.39 117.76 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1005 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(R1005-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 101.38 137.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H102 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 74.99 123.44 315)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L803 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2 nH" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 78.725 131.525)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 82.63 118.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1002 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 78.725 132.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 98.68 119.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R504 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 "/USB Input/D_P"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 73.65 124.12 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C819 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(AE801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 94.45 128.65 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R510 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 78.725 130.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R810 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 82.63 120.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1007 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 INT_OPT3001))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 103.39 125.09 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C506 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 94.97 120.16 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C508 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 78.725 129.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R809 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R809-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 85.525 132.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 94.44 132.43 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C503 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 79.23 119.33 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1003 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(R1003-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 77.62 127.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C812 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD locked (layer F.Cu) (tedit 5E541D62)
    (at 84.68 125.6 90)
    (fp_text reference J701 (at -0.074182 -1.275144 90) (layer F.SilkS) hide)
    (fp_text value mikroBUS (at -0.074182 -0.005144 90) (layer F.Fab))
    (fp_text user %R (at 11.43 0 180) (layer F.Fab))
    (fp_text user %R (at 11.355818 -0.005144 180) (layer F.Fab) hide)
    (pad 10 smd rect (at 13.08 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 12 smd rect (at 13.08 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 14 smd rect (at 13.08 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 45 CC1352_TX_MB1_RX))
    (pad 16 smd rect (at 13.08 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM_MB1))
    (pad 9 smd rect (at 9.78 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 9.78 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 13 smd rect (at 9.78 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 47 CC1352_RX_MB1_TX))
    (pad 15 smd rect (at 9.78 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 48 INT_MB1))
    (pad 8 smd rect (at -13.08 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -13.08 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 38 MOSI))
    (pad 2 smd rect (at -13.08 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 49 RST_MB1))
    (pad 1 smd rect (at -9.78 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 50 AN_MB1))
    (pad 4 smd rect (at -13.08 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at -9.78 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 20 3V3))
    (pad 3 smd rect (at -9.78 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 51 CS_MB1))
    (pad 5 smd rect (at -9.78 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 33 MISO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 95.14 123.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F801 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value Polyfuse (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 81.28 117.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1001 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:BeagleBoard.org-20mm (layer B.Cu) (tedit 0)
    (at 71.38 125.3 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module leash:USON6 (layer B.Cu) (tedit 5E4DAB76)
    (at 85.16 121.09 180)
    (fp_text reference U1003 (at 0.11 -3.68) (layer B.SilkS) hide)
    (fp_text value OPT3001 (at -0.16 3.7) (layer B.Fab))
    (pad 7 thru_hole circle (at 0 -0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 smd rect (at 0 0 180) (size 0.65 1.35) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.02))
    (pad 6 smd roundrect (at 0.95 0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 41 SDA) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at 0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 100 INT_OPT3001) (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at 0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 44 SCL) (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 101 "Net-(R1008-Pad2)") (solder_mask_margin 0.07))
    (pad 1 smd roundrect (at -0.95 0.675 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 19 VDDS) (solder_mask_margin 0.07))
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 101.905 118.875 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference D502 (at 0 2.9 270) (layer B.SilkS) hide)
    (fp_text value TPD2E001 (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 91 "/USB Input/D_P"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 90 "/USB Input/D_N"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.95 122.05 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R502 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(P501-PadA5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 71.325 129.625 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C821 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C821-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 91.295 118.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C509 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 78.21 118.29 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1002 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer B.Cu) (tedit 5A0FD1B2)
    (at 101.805 122.475)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y501 (at 0 2.45) (layer B.SilkS) hide)
    (fp_text value 24MHz (at 0 -2.45) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 4 smd rect (at -1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 "/USB Input/XTAL2"))
    (pad 2 smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 "/USB Input/XTAL1"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer F.Cu) (tedit 5E4C72AA)
    (at 92.4 125.5 270)
    (attr virtual)
    (fp_text reference J301 (at 0.302285 2.603303 270) (layer F.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at -0.967715 -2.222697 270) (layer F.Fab))
    (pad 4 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 32 CC1352_TCK))
    (pad 5 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 31 CC1352_TDO))
    (pad 7 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 1 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 20 3V3))
    (pad 10 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 17 RESET_N))
    (pad 2 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 30 CC1352_TMS))
    (pad 9 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 3 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 8 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 29 CC1352_TDI))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 87.68 121.11 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1008 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(R1008-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:RFECA3216060A1T (layer F.Cu) (tedit 5E42DF6C)
    (at 70.28 124 270)
    (fp_text reference AE801 (at 0 1.85 90) (layer F.SilkS) hide)
    (fp_text value Antenna_Dipole (at 0.05 -1.7 90) (layer F.Fab))
    (pad 3 smd rect (at -1.4 0 270) (size 0.35 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(AE801-Pad3)"))
    (pad 2 smd rect (at 1.4 0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.4 -0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AE801-Pad1)"))
    (model ${KIPRJMOD}/mech/2450AT18D0100.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 77.755 129.575 315)
    (descr "SMD Crystal 2012/2 http://txccrystal.com/images/pdf/9ht11.pdf, 2.0x1.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y801 (at 0 -1.8 135) (layer F.SilkS) hide)
    (fp_text value Crystal (at 0 1.8 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C802-Pad1)"))
    (pad 1 smd rect (at -0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C801-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_AX_8045-2Pin_8.0x4.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.25 0.3 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm (layer F.Cu) (tedit 5C26A111)
    (at 84.13 127.44)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U801 (at 0 -4.82) (layer F.SilkS) hide)
    (fp_text value CC1352R (at 0 4.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 48 smd roundrect (at -2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 47 smd roundrect (at -2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U801-Pad47)"))
    (pad 46 smd roundrect (at -1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U801-Pad46)"))
    (pad 45 smd roundrect (at -1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 44 smd roundrect (at -0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 43 smd roundrect (at -0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 PWM_MB1))
    (pad 42 smd roundrect (at 0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 INT_MB1))
    (pad 41 smd roundrect (at 0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 40 smd roundrect (at 1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 39 smd roundrect (at 1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 38 smd roundrect (at 2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 37 smd roundrect (at 2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 AN_MB2))
    (pad 36 smd roundrect (at 3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 AN_MB1))
    (pad 35 smd roundrect (at 3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 34 smd roundrect (at 3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 33 smd roundrect (at 3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 32 smd roundrect (at 3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 31 smd roundrect (at 3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 30 smd roundrect (at 3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 INT_MB2))
    (pad 29 smd roundrect (at 3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 PWM_MB2))
    (pad 28 smd roundrect (at 3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 27 smd roundrect (at 3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 CC1352_TDI))
    (pad 26 smd roundrect (at 3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 CC1352_TDO))
    (pad 25 smd roundrect (at 3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 CC1352_TCK))
    (pad 24 smd roundrect (at 2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 CC1352_TMS))
    (pad 23 smd roundrect (at 2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 22 smd roundrect (at 1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 21 smd roundrect (at 1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 20 smd roundrect (at 0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 19 smd roundrect (at 0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 CS_MB1))
    (pad 18 smd roundrect (at -0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 CS_MB2))
    (pad 17 smd roundrect (at -0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 16 smd roundrect (at -1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 15 smd roundrect (at -1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 14 smd roundrect (at -2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 13 smd roundrect (at -2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 12 smd roundrect (at -3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 INT_SENSOR))
    (pad 11 smd roundrect (at -3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 RST_MB1))
    (pad 10 smd roundrect (at -3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 RST_MB2))
    (pad 9 smd roundrect (at -3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 8 smd roundrect (at -3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 7 smd roundrect (at -3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 6 smd roundrect (at -3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 5 smd roundrect (at -3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 4 smd roundrect (at -3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 3 smd roundrect (at -3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 2 smd roundrect (at -3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 1 smd roundrect (at -3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad "" smd roundrect (at 1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad 49 smd roundrect (at 0 0) (size 5.15 5.15) (layers F.Cu F.Mask) (roundrect_rratio 0.048544)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 97.18 137.25 90)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW902 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 1 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 2 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 73.2 127.3 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L804 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD locked (layer F.Cu) (tedit 5E541D62)
    (at 84.68 95.6 90)
    (fp_text reference J701 (at -0.074182 -1.275144 90) (layer F.SilkS) hide)
    (fp_text value mikroBUS (at -0.074182 -0.005144 90) (layer F.Fab))
    (fp_text user %R (at 11.355818 -0.005144 180) (layer F.Fab) hide)
    (fp_text user %R (at 11.43 0 180) (layer F.Fab))
    (pad 5 smd rect (at -9.78 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -9.78 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 51 CS_MB1))
    (pad 7 smd rect (at -9.78 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 20 3V3))
    (pad 4 smd rect (at -13.08 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 35 SCK))
    (pad 1 smd rect (at -9.78 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 50 AN_MB1))
    (pad 2 smd rect (at -13.08 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 49 RST_MB1))
    (pad 6 smd rect (at -13.08 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 38 MOSI))
    (pad 8 smd rect (at -13.08 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 9.78 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 48 INT_MB1))
    (pad 13 smd rect (at 9.78 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 47 CC1352_RX_MB1_TX))
    (pad 11 smd rect (at 9.78 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 9 smd rect (at 9.78 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 13.08 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM_MB1))
    (pad 14 smd rect (at 13.08 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 45 CC1352_TX_MB1_RX))
    (pad 12 smd rect (at 13.08 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 13.08 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 77.62 97.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C812 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 103.39 95.09 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C506 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 98.68 89.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R504 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 "/USB Input/D_P"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 78.725 102.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 78.725 100.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R810 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 78.725 99.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R809 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R809-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 78.725 101.525)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 74.99 93.44 315)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L803 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2 nH" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 71.85 97.95 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C817 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "5.6 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 73.875 95.925 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C815 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2.7 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 74.3 92.1 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C816 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 83.21 87.74)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1004 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(R1004-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 94.4 95.99 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R505 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 99.08 100.2 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J201 (at 0 -5.8 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.95 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (pad 2 smd roundrect (at 1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad MP smd roundrect (at -3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at 3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.step
      (offset (xyz -1 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 79.39 87.76 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1005 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 86.38 102.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C805 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 83.58 88.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1001 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 94.44 100.55 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R509 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 99.17 93.035 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C507 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 75.825 96.175 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C813 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 73.25 99.375 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C820 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(AE802-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 80.805 102.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C806 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 97.955 106.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C501 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 83.6 102.925 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 102.68 104.74)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C502 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 10U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.96 89.22 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R501 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(P501-PadB5)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 86.475 102.95 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer B.Cu) (tedit 5D409D35)
    (at 92.4 95.5 270)
    (attr virtual)
    (fp_text reference J501 (at 3.81 -2.413 90) (layer B.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at 2.54 2.413 90) (layer B.Fab))
    (pad 8 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 3 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 9 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 2 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 10 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 1 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 20 3V3))
    (pad "" np_thru_hole circle (at 7.62 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 7 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 6 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 5 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 4 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 "/USB Input/MSP430_TCK"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 79.23 89.33 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1003 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(R1003-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 82.63 88.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1002 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 95.14 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F801 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value Polyfuse (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 81.28 87.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1001 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:BeagleBoard.org-20mm (layer B.Cu) (tedit 0)
    (at 71.38 95.3 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module leash:HDC2010 (layer F.Cu) (tedit 5E4D6772)
    (at 82.58 88.95)
    (fp_text reference U1001 (at -0.025 2.025) (layer F.SilkS) hide)
    (fp_text value HDC2010 (at 0 -3.8) (layer F.Fab))
    (pad A2 smd circle (at 0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA) (solder_mask_margin 0.05))
    (pad B2 smd circle (at 0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL) (solder_mask_margin 0.05))
    (pad C2 smd circle (at 0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 95 INT_HDC2010) (solder_mask_margin 0.05))
    (pad C1 smd circle (at -0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad B1 smd circle (at -0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R1004-Pad1)") (solder_mask_margin 0.05))
    (pad A1 smd circle (at -0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS) (solder_mask_margin 0.05))
  )
  (module leash:USON6 (layer B.Cu) (tedit 5E4DAB76)
    (at 85.16 91.09 180)
    (fp_text reference U1003 (at 0.11 -3.68) (layer B.SilkS) hide)
    (fp_text value OPT3001 (at -0.16 3.7) (layer B.Fab))
    (pad 1 smd roundrect (at -0.95 0.675 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 19 VDDS) (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 101 "Net-(R1008-Pad2)") (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at 0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 44 SCL) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at 0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 100 INT_OPT3001) (solder_mask_margin 0.07))
    (pad 6 smd roundrect (at 0.95 0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 41 SDA) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 0 0 180) (size 0.65 1.35) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 -0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 85.525 102.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.95 92.05 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R502 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(P501-PadA5)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 71.325 99.625 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C821 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C821-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 78.21 88.29 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1002 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 73.2 97.3 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L804 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:X2SON-8_1.4x1mm_P0.35mm (layer B.Cu) (tedit 5A02F1D8)
    (at 80.63 89.85 180)
    (descr "X2SON-8 1.4x1mm Pitch0.35mm http://www.ti.com/lit/ds/symlink/pca9306.pdf")
    (tags "X2SON-8 1.4x1mm Pitch0.35mm")
    (attr smd)
    (fp_text reference U1002 (at 0 2) (layer B.SilkS) hide)
    (fp_text value SN74AUP2G32 (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 95 INT_HDC2010))
    (pad 2 smd rect (at -0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 3 smd rect (at -0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 94 INT_SENSOR))
    (pad 4 smd rect (at -0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 7 smd rect (at 0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 8 smd rect (at 0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer F.Cu) (tedit 5E4C72AA)
    (at 92.4 95.5 270)
    (attr virtual)
    (fp_text reference J301 (at 0.302285 2.603303 270) (layer F.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at -0.967715 -2.222697 270) (layer F.Fab))
    (pad 8 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 29 CC1352_TDI))
    (pad 3 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 9 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 2 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 30 CC1352_TMS))
    (pad 10 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 17 RESET_N))
    (pad 1 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 20 3V3))
    (pad 7 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 6 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 31 CC1352_TDO))
    (pad 5 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 32 CC1352_TCK))
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer B.Cu) (tedit 5A0FD1B2)
    (at 101.805 92.475)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y501 (at 0 2.45) (layer B.SilkS) hide)
    (fp_text value 24MHz (at 0 -2.45) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 "/USB Input/XTAL1"))
    (pad 2 smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 "/USB Input/XTAL2"))
    (pad 4 smd rect (at -1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 94.45 98.65 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R510 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 91.295 88.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C509 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 82.63 90.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1007 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 INT_OPT3001))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 84.55 102.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 99.655 89.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R503 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 90 "/USB Input/D_N"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 97.255 82.75 270)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW901 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 1 smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 73.65 94.12 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C819 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(AE801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 101.905 88.875 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference D502 (at 0 2.9 270) (layer B.SilkS) hide)
    (fp_text value TPD2E001 (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 90 "/USB Input/D_N"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 91 "/USB Input/D_P"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 79 "/USB Input/VBUS"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm (layer F.Cu) (tedit 5C26A111)
    (at 84.13 97.44)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U801 (at 0 -4.82) (layer F.SilkS) hide)
    (fp_text value CC1352R (at 0 4.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 49 smd roundrect (at 0 0) (size 5.15 5.15) (layers F.Cu F.Mask) (roundrect_rratio 0.048544)
      (net 1 GND))
    (pad "" smd roundrect (at -1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad 1 smd roundrect (at -3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 2 smd roundrect (at -3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 3 smd roundrect (at -3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 4 smd roundrect (at -3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 5 smd roundrect (at -3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 6 smd roundrect (at -3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 7 smd roundrect (at -3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 8 smd roundrect (at -3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 9 smd roundrect (at -3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 10 smd roundrect (at -3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 RST_MB2))
    (pad 11 smd roundrect (at -3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 RST_MB1))
    (pad 12 smd roundrect (at -3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 INT_SENSOR))
    (pad 13 smd roundrect (at -2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 14 smd roundrect (at -2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 15 smd roundrect (at -1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 16 smd roundrect (at -1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 17 smd roundrect (at -0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 18 smd roundrect (at -0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 CS_MB2))
    (pad 19 smd roundrect (at 0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 CS_MB1))
    (pad 20 smd roundrect (at 0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 21 smd roundrect (at 1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 22 smd roundrect (at 1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 23 smd roundrect (at 2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 24 smd roundrect (at 2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 CC1352_TMS))
    (pad 25 smd roundrect (at 3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 CC1352_TCK))
    (pad 26 smd roundrect (at 3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 CC1352_TDO))
    (pad 27 smd roundrect (at 3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 CC1352_TDI))
    (pad 28 smd roundrect (at 3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 29 smd roundrect (at 3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 PWM_MB2))
    (pad 30 smd roundrect (at 3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 INT_MB2))
    (pad 31 smd roundrect (at 3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 32 smd roundrect (at 3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 33 smd roundrect (at 3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 34 smd roundrect (at 3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 35 smd roundrect (at 3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 36 smd roundrect (at 3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 AN_MB1))
    (pad 37 smd roundrect (at 2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 AN_MB2))
    (pad 38 smd roundrect (at 2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 39 smd roundrect (at 1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 40 smd roundrect (at 1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 41 smd roundrect (at 0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 42 smd roundrect (at 0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 INT_MB1))
    (pad 43 smd roundrect (at -0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 PWM_MB1))
    (pad 44 smd roundrect (at -0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 45 smd roundrect (at -1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 46 smd roundrect (at -1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U801-Pad46)"))
    (pad 47 smd roundrect (at -2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U801-Pad47)"))
    (pad 48 smd roundrect (at -2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 94.97 90.16 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C508 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:RFECA3216060A1T (layer F.Cu) (tedit 5E42DF6C)
    (at 70.28 94 270)
    (fp_text reference AE801 (at 0 1.85 90) (layer F.SilkS) hide)
    (fp_text value Antenna_Dipole (at 0.05 -1.7 90) (layer F.Fab))
    (pad 1 smd rect (at 1.4 -0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AE801-Pad1)"))
    (pad 2 smd rect (at 1.4 0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.4 0 270) (size 0.35 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(AE801-Pad3)"))
    (model ${KIPRJMOD}/mech/2450AT18D0100.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 101.38 107.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H102 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 87.68 91.11 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1008 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(R1008-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD (layer B.Cu) (tedit 5E541D54)
    (at 84.6 95.6 90)
    (fp_text reference J702 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value mikroBUS (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at 11.43 0) (layer B.Fab))
    (fp_text user %R (at -11.43 0) (layer B.Fab))
    (pad 10 smd rect (at 13.08 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 28 5V))
    (pad 12 smd rect (at 13.08 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 44 SCL))
    (pad 14 smd rect (at 13.08 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 43 CC1352_TX_MB2_RX))
    (pad 16 smd rect (at 13.08 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 42 PWM_MB2))
    (pad 9 smd rect (at 9.78 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 9.78 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 41 SDA))
    (pad 13 smd rect (at 9.78 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 40 CC1352_RX_MB2_TX))
    (pad 15 smd rect (at 9.78 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 39 INT_MB2))
    (pad 8 smd rect (at -13.08 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -13.08 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 2 smd rect (at -13.08 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 37 RST_MB2))
    (pad 1 smd rect (at -9.78 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 36 AN_MB2))
    (pad 4 smd rect (at -13.08 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at -9.78 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 20 3V3))
    (pad 3 smd rect (at -9.78 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 34 CS_MB2))
    (pad 5 smd rect (at -9.78 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 100.82 104.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C505 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0.47U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 101 95.57 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C504 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 220N (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 95.84 95.49 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R508 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1.5K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 97.18 107.25 90)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW902 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 1 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 74.9 102.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference AE802 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(AE802-Pad1)"))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 70.28 91.315 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C822 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(AE801-Pad3)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 94.44 102.43 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C503 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 72.88 91.4 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C818 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C818-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 71.48 87.8 270)
    (fp_text reference J801 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 4 smd rect (at 0 1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C818-Pad2)"))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module leash:L_0806_2012Metric (layer B.Cu) (tedit 5D2F3EE6)
    (at 96.985 89.9 90)
    (descr "Inductor SMD 0806 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L601 (at 0 1.65 90) (layer B.SilkS) hide)
    (fp_text value INDUCTOR (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(L601-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 77.755 99.575 315)
    (descr "SMD Crystal 2012/2 http://txccrystal.com/images/pdf/9ht11.pdf, 2.0x1.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y801 (at 0 -1.8 135) (layer F.SilkS) hide)
    (fp_text value Crystal (at 0 1.8 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C801-Pad1)"))
    (pad 2 smd rect (at 0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_AX_8045-2Pin_8.0x4.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.25 0.3 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 80.4 91.3 180)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y802 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Crystal_GND2 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U801-Pad46)"))
    (pad 2 smd rect (at 0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U801-Pad47)"))
    (pad 4 smd rect (at -0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 90.25 95.625)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L801 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 96.63 82.575 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D501 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 86.05 88.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R803 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 CC1352_RX_MB2_TX))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 88.43 88.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R802 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 CC1352_TX_MB2_RX))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 71.25 102.85 90)
    (fp_text reference J802 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 4 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C821-Pad2)"))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module leash:MX25R8035FZUIL0 (layer B.Cu) (tedit 5E42FFC6)
    (at 80.775 101.08 270)
    (fp_text reference U802 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value MX25R8035FZUIL0 (at 0 -2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 109 ~FLASH_CS))
    (pad 2 smd rect (at -1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R809-Pad2)"))
    (pad 4 smd rect (at -1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 6 smd rect (at 1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at 1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 8 smd rect (at 1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C811-Pad2)"))
    (pad 9 smd custom (at 0 0 270) (size 0.2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0 0.8) (xy 0.1 0.8) (xy 0.1 -0.8) (xy -0.1 -0.8) (xy -0.1 0.7)
) (width 0))
      ))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:TPS62821DLC (layer B.Cu) (tedit 5D2676FA)
    (at 94.885 91.1)
    (fp_text reference U601 (at 0.1 1.975 180) (layer B.SilkS) hide)
    (fp_text value TPS62821DLC (at 0 0.5 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 2 smd roundrect (at -0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(C602-Pad2)"))
    (pad 3 smd roundrect (at -0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 4 smd roundrect (at -0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2))
    (pad 5 smd roundrect (at 0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 6 smd roundrect (at 0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 73 "Net-(L601-Pad1)"))
    (pad 7 smd roundrect (at 0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 8 smd roundrect (at 0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 74 "Net-(R601-Pad1)"))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1.3 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 90.96 88.76 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C603 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value "10 uF" (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 76.32 94.11 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C814 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 78.725 103.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 85.5 97.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C810 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "22 uF" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 82.88 91.9 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C809 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 80.28 93.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C808 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 84.48 93 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 88.025 95.1 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C804 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 87.38 102.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C803 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.36 88.01)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F501 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value Polyfuse (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 78.47 90.665 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1006 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 INT_LIS2DE12_2))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LGA:LGA-12_2x2mm_P0.5mm (layer F.Cu) (tedit 5A0AAFFD)
    (at 80.01 88.69 180)
    (descr LGA12)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U1004 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value LIS2DE12 (at 0 1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at -0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 9 smd rect (at 0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 8 smd rect (at 0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 7 smd rect (at 0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 5 smd rect (at -0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 99 INT_LIS2DE12_2))
    (pad 12 smd rect (at -0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 95.88 107.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R511 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 97.98 107.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R507 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 97.755 105.55 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L501 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Palconn_UTC16-G (layer F.Cu) (tedit 5CF432E0)
    (at 99.5 90.3 90)
    (descr http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf)
    (tags "USB C Type-C Receptacle USB2.0")
    (attr smd)
    (fp_text reference P501 (at 0 -4.58 90) (layer F.SilkS) hide)
    (fp_text value USB_C_Plug_USB2.0 (at 0 6.24 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.43 90) (layer Dwgs.User))
    (fp_text user %R (at 0 1.18 90) (layer F.Fab))
    (pad A12 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B1 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B4 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B12 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A1 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B9 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A4 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad "" np_thru_hole circle (at -2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad B5 smd rect (at 1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(P501-PadB5)"))
    (pad B6 smd rect (at 0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A8 smd rect (at 1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at -1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P501-PadA5)"))
    (pad B8 smd rect (at -1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A7 smd rect (at 0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 90 "/USB Input/D_N"))
    (pad A6 smd rect (at -0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 91 "/USB Input/D_P"))
    (pad B7 smd rect (at -0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad S1 thru_hole oval (at 4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/1054500101.stp
      (offset (xyz 0 -0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 71.38 82.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H103 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 71.38 107.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H104 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N48_EP5.15x5.15mm (layer B.Cu) (tedit 5E4C745D)
    (at 99.05 100.15 180)
    (descr "QFN, 48 Pin (http://www.ti.com/lit/ds/symlink/msp430f5232.pdf#page=112), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U501 (at 0 4.82) (layer B.SilkS) hide)
    (fp_text value MSP430F5500IRGZ (at 0 -4.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 49 smd roundrect (at 0 0 180) (size 5.15 5.15) (layers B.Cu B.Mask) (roundrect_rratio 0.049)
      (net 1 GND))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad 1 smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 8 smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 12 smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 13 smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 14 smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 15 smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 16 smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 17 smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 18 smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 19 smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 20 smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 21 smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 22 smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 23 smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 24 smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 25 smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 26 smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 27 smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 28 smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 29 smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 30 smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 31 smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 32 smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 33 smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 34 smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 35 smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 36 smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 37 smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 38 smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 39 smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 40 smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 41 smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 42 smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 43 smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 44 smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 45 smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 46 smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 47 smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 48 smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 "/USB Input/MSP430_RST_N"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N48_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:0900PC15A0036 (layer F.Cu) (tedit 5E41EA1D)
    (at 78.14 95.44 270)
    (fp_text reference B801 (at 0.025 4.2 90) (layer F.SilkS) hide)
    (fp_text value 0900PC15A0036E (at -0.05 -3.025 90) (layer F.Fab))
    (pad 4 smd roundrect (at 0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (pad 3 smd roundrect (at 0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 6 smd roundrect (at 0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 7 smd roundrect (at 0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 8 smd roundrect (at -0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 9 smd roundrect (at -0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 5 smd roundrect (at 1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 10 smd roundrect (at -1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/0900PC15J0013.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 101.38 82.56)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H101 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 93.585 92.7 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 90.28 98.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 85.68 95.9)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L802 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 89.965 92.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R804 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 89.975 93.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R805 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 95.505 88.3 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R604 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 93.49 93.7)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D201 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 80.9 80.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D404 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 90.055 80.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D403 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 84.25 80.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D401 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 87.145 80.58)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D402 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 93.685 88.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "100 pF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 78.855 101.125 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C802 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 76.63 100.5 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C801 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 92.23 89.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R603 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 93.685 89.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 84.25 80.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R401 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 87.14 80.57)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R402 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 77.41 80.6)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D405 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 95.535 92.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(R601-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 77.4 80.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R405 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 80.9 80.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R404 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 90.05 80.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R403 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 92.05 90.75)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U502 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value BQ21040 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 ~CHG))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R506-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.95 91.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R506 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(R506-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 93.12 80.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R406 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 ~CHG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 93.13 80.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D406 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD locked (layer F.Cu) (tedit 5E541D62)
    (at 84.68 65.6 90)
    (fp_text reference J701 (at -0.074182 -1.275144 90) (layer F.SilkS) hide)
    (fp_text value mikroBUS (at -0.074182 -0.005144 90) (layer F.Fab))
    (fp_text user %R (at 11.43 0 180) (layer F.Fab))
    (fp_text user %R (at 11.355818 -0.005144 180) (layer F.Fab) hide)
    (pad 10 smd rect (at 13.08 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 12 smd rect (at 13.08 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 14 smd rect (at 13.08 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 45 CC1352_TX_MB1_RX))
    (pad 16 smd rect (at 13.08 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM_MB1))
    (pad 9 smd rect (at 9.78 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 9.78 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 13 smd rect (at 9.78 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 47 CC1352_RX_MB1_TX))
    (pad 15 smd rect (at 9.78 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 48 INT_MB1))
    (pad 8 smd rect (at -13.08 8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -13.08 3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 38 MOSI))
    (pad 2 smd rect (at -13.08 -6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 49 RST_MB1))
    (pad 1 smd rect (at -9.78 -8.89 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 50 AN_MB1))
    (pad 4 smd rect (at -13.08 -1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 35 SCK))
    (pad 7 smd rect (at -9.78 6.35 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 20 3V3))
    (pad 3 smd rect (at -9.78 -3.81 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 51 CS_MB1))
    (pad 5 smd rect (at -9.78 1.27 90) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 33 MISO))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MikroBus-SMD (layer B.Cu) (tedit 5E541D54)
    (at 84.6 65.6 90)
    (fp_text reference J702 (at 0 1.27 90) (layer B.SilkS) hide)
    (fp_text value mikroBUS (at 0 0 90) (layer B.Fab))
    (fp_text user %R (at -11.43 0) (layer B.Fab))
    (fp_text user %R (at 11.43 0) (layer B.Fab))
    (pad 5 smd rect (at -9.78 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 3 smd rect (at -9.78 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 34 CS_MB2))
    (pad 7 smd rect (at -9.78 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 20 3V3))
    (pad 4 smd rect (at -13.08 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 1 smd rect (at -9.78 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 36 AN_MB2))
    (pad 2 smd rect (at -13.08 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 37 RST_MB2))
    (pad 6 smd rect (at -13.08 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 8 smd rect (at -13.08 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 9.78 6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 39 INT_MB2))
    (pad 13 smd rect (at 9.78 1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 40 CC1352_RX_MB2_TX))
    (pad 11 smd rect (at 9.78 -3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 41 SDA))
    (pad 9 smd rect (at 9.78 -8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 13.08 8.89 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 42 PWM_MB2))
    (pad 14 smd rect (at 13.08 3.81 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 43 CC1352_TX_MB2_RX))
    (pad 12 smd rect (at 13.08 -1.27 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 44 SCL))
    (pad 10 smd rect (at 13.08 -6.35 90) (size 1.9 1) (layers B.Cu B.Paste B.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz 11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (offset (xyz -11.43 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:BeagleBoard.org-20mm (layer B.Cu) (tedit 0)
    (at 71.38 65.3 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 95.88 77.2 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R511 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 97.98 77.8)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R507 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 92.05 60.75)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U502 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value BQ21040 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R506-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 104 ~CHG))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.95 61.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R506 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 105 "Net-(R506-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 93.12 50.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R406 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 104 ~CHG))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 93.13 50.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D406 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D406-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 91.295 58.15 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C509 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 94.97 60.16 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C508 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 10U (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:USON6 (layer B.Cu) (tedit 5E4DAB76)
    (at 85.16 61.09 180)
    (fp_text reference U1003 (at 0.11 -3.68) (layer B.SilkS) hide)
    (fp_text value OPT3001 (at -0.16 3.7) (layer B.Fab))
    (pad 7 thru_hole circle (at 0 -0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 thru_hole circle (at 0 0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (solder_mask_margin 0.02))
    (pad 7 smd rect (at 0 0 180) (size 0.65 1.35) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.02))
    (pad 6 smd roundrect (at 0.95 0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 41 SDA) (solder_mask_margin 0.07))
    (pad 5 smd roundrect (at 0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 100 INT_OPT3001) (solder_mask_margin 0.07))
    (pad 4 smd roundrect (at 0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 44 SCL) (solder_mask_margin 0.07))
    (pad 3 smd roundrect (at -0.95 -0.65 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 2 smd roundrect (at -0.95 0 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 101 "Net-(R1008-Pad2)") (solder_mask_margin 0.07))
    (pad 1 smd roundrect (at -0.95 0.675 180) (size 0.5 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.5)
      (net 19 VDDS) (solder_mask_margin 0.07))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 87.68 61.11 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1008 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(R1008-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LGA:LGA-12_2x2mm_P0.5mm (layer F.Cu) (tedit 5A0AAFFD)
    (at 80.01 58.69 180)
    (descr LGA12)
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U1004 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value LIS2DE12 (at 0 1.6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 12 smd rect (at -0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0.25 -0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 99 INT_LIS2DE12_2))
    (pad 6 smd rect (at 0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -0.25 0.7625 270) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 1 smd rect (at -0.7625 -0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL))
    (pad 7 smd rect (at 0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.7625 0.75 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA))
    (pad 8 smd rect (at 0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS))
    (pad 3 smd rect (at -0.7625 0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R1005-Pad1)"))
    (pad 2 smd rect (at -0.7625 -0.25 180) (size 0.375 0.35) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-12_2x2mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 82.63 60.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1007 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 100 INT_OPT3001))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 78.47 60.665 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1006 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 INT_LIS2DE12_2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 79.39 57.76 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1005 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 97 "Net-(R1005-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 83.21 57.74)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1004 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 96 "Net-(R1004-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 99.17 63.035 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C507 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 103.39 65.09 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C506 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 18P (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:X2SON-8_1.4x1mm_P0.35mm (layer B.Cu) (tedit 5A02F1D8)
    (at 80.63 59.85 180)
    (descr "X2SON-8 1.4x1mm Pitch0.35mm http://www.ti.com/lit/ds/symlink/pca9306.pdf")
    (tags "X2SON-8 1.4x1mm Pitch0.35mm")
    (attr smd)
    (fp_text reference U1002 (at 0 2) (layer B.SilkS) hide)
    (fp_text value SN74AUP2G32 (at 0 -2) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 8 smd rect (at 0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 19 VDDS))
    (pad 7 smd rect (at 0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R1003-Pad1)"))
    (pad 6 smd rect (at 0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 5 smd rect (at 0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -0.335 -0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.335 -0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 94 INT_SENSOR))
    (pad 2 smd rect (at -0.335 0.175 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R1006-Pad2)"))
    (pad 1 smd rect (at -0.335 0.525 270) (size 0.2 0.53) (layers B.Cu B.Paste B.Mask)
      (net 95 INT_HDC2010))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm (layer F.Cu) (tedit 5C26A111)
    (at 84.13 67.44)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U801 (at 0 -4.82) (layer F.SilkS) hide)
    (fp_text value CC1352R (at 0 4.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 48 smd roundrect (at -2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 47 smd roundrect (at -2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 "Net-(U801-Pad47)"))
    (pad 46 smd roundrect (at -1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 "Net-(U801-Pad46)"))
    (pad 45 smd roundrect (at -1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 44 smd roundrect (at -0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 43 smd roundrect (at -0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 PWM_MB1))
    (pad 42 smd roundrect (at 0.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 INT_MB1))
    (pad 41 smd roundrect (at 0.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (pad 40 smd roundrect (at 1.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 39 smd roundrect (at 1.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (pad 38 smd roundrect (at 2.25 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 37 smd roundrect (at 2.75 -3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 AN_MB2))
    (pad 36 smd roundrect (at 3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 AN_MB1))
    (pad 35 smd roundrect (at 3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 34 smd roundrect (at 3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 33 smd roundrect (at 3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 32 smd roundrect (at 3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 31 smd roundrect (at 3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 30 smd roundrect (at 3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 INT_MB2))
    (pad 29 smd roundrect (at 3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 PWM_MB2))
    (pad 28 smd roundrect (at 3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 27 smd roundrect (at 3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 CC1352_TDI))
    (pad 26 smd roundrect (at 3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 CC1352_TDO))
    (pad 25 smd roundrect (at 3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 CC1352_TCK))
    (pad 24 smd roundrect (at 2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 CC1352_TMS))
    (pad 23 smd roundrect (at 2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 22 smd roundrect (at 1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 21 smd roundrect (at 1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 20 smd roundrect (at 0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 19 smd roundrect (at 0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 CS_MB1))
    (pad 18 smd roundrect (at -0.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 CS_MB2))
    (pad 17 smd roundrect (at -0.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 16 smd roundrect (at -1.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 15 smd roundrect (at -1.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 14 smd roundrect (at -2.25 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 13 smd roundrect (at -2.75 3.4375) (size 0.25 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 12 smd roundrect (at -3.4375 2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 94 INT_SENSOR))
    (pad 11 smd roundrect (at -3.4375 2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 RST_MB1))
    (pad 10 smd roundrect (at -3.4375 1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 RST_MB2))
    (pad 9 smd roundrect (at -3.4375 1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 8 smd roundrect (at -3.4375 0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 7 smd roundrect (at -3.4375 0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (pad 6 smd roundrect (at -3.4375 -0.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (pad 5 smd roundrect (at -3.4375 -0.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 4 smd roundrect (at -3.4375 -1.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 3 smd roundrect (at -3.4375 -1.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 2 smd roundrect (at -3.4375 -2.25) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 1 smd roundrect (at -3.4375 -2.75) (size 0.875 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad "" smd roundrect (at 1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935) (size 1.04 1.04) (layers F.Paste) (roundrect_rratio 0.240385))
    (pad 49 smd roundrect (at 0 0) (size 5.15 5.15) (layers F.Cu F.Mask) (roundrect_rratio 0.048544)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 79.23 59.33 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1003 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 92 "Net-(R1003-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 93 "Net-(R1003-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 78.21 58.29 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1002 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:HDC2010 (layer F.Cu) (tedit 5E4D6772)
    (at 82.58 58.95)
    (fp_text reference U1001 (at -0.025 2.025) (layer F.SilkS) hide)
    (fp_text value HDC2010 (at 0 -3.8) (layer F.Fab))
    (pad A1 smd circle (at -0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 19 VDDS) (solder_mask_margin 0.05))
    (pad B1 smd circle (at -0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R1004-Pad1)") (solder_mask_margin 0.05))
    (pad C1 smd circle (at -0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad C2 smd circle (at 0.5 0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 95 INT_HDC2010) (solder_mask_margin 0.05))
    (pad B2 smd circle (at 0.5 0) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 44 SCL) (solder_mask_margin 0.05))
    (pad A2 smd circle (at 0.5 -0.5) (size 0.263 0.263) (layers F.Cu F.Paste F.Mask)
      (net 41 SDA) (solder_mask_margin 0.05))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 82.63 58.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1002 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 41 SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 83.58 58.2 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1001 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 SCL))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 81.28 57.75)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1001 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer F.Cu) (tedit 5E4C72AA)
    (at 92.4 65.5 270)
    (attr virtual)
    (fp_text reference J301 (at 0.302285 2.603303 270) (layer F.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at -0.967715 -2.222697 270) (layer F.Fab))
    (pad 4 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 32 CC1352_TCK))
    (pad 5 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 31 CC1352_TDO))
    (pad 7 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 1 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 20 3V3))
    (pad 10 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 17 RESET_N))
    (pad 2 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 30 CC1352_TMS))
    (pad 9 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask))
    (pad 3 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 8 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 29 CC1352_TDI))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.36 58.01)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F501 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value Polyfuse (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm (layer B.Cu) (tedit 5A0FD1B2)
    (at 101.805 62.475)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y501 (at 0 2.45) (layer B.SilkS) hide)
    (fp_text value 24MHz (at 0 -2.45) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 4 smd rect (at -1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 89 "/USB Input/XTAL2"))
    (pad 2 smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers B.Cu B.Paste B.Mask)
      (net 88 "/USB Input/XTAL1"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 95.14 63.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference F801 (at 0 1.43) (layer B.SilkS) hide)
    (fp_text value Polyfuse (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 99.08 70.2 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J201 (at 0 -5.8 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 5.8 90) (layer F.Fab))
    (fp_text user %R (at 0 1.95 90) (layer F.Fab) hide)
    (pad MP smd roundrect (at 3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at -3.35 2.9 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad 2 smd roundrect (at 1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 -2.85 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.step
      (offset (xyz -1 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 94.45 68.65 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R510 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 94.44 70.55 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R509 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 95.84 65.49 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R508 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1.5K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 94.4 65.99 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R505 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 1M (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 98.68 59.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R504 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 91 "/USB Input/D_P"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 99.655 59.825 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R503 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 10R0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 90 "/USB Input/D_N"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.95 62.05 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R502 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 "Net-(P501-PadA5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 94.96 59.22 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R501 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(P501-PadB5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 97.755 75.55 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L501 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer B.Cu) (tedit 5A02FF57)
    (at 101.905 58.875 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference D502 (at 0 2.9 270) (layer B.SilkS) hide)
    (fp_text value TPD2E001 (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 91 "/USB Input/D_P"))
    (pad 4 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 90 "/USB Input/D_N"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 100.82 74.76)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C505 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0.47U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 101 65.57 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C504 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 220N (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 94.44 72.43 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C503 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 102.68 74.74)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C502 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 10U (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 97.955 76.8)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C501 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:Tag-Connect-10 locked (layer B.Cu) (tedit 5D409D35)
    (at 92.4 65.5 270)
    (attr virtual)
    (fp_text reference J501 (at 3.81 -2.413 90) (layer B.SilkS) hide)
    (fp_text value TAG-CONNECT-10 (at 2.54 2.413 90) (layer B.Fab))
    (pad 4 smd circle (at 5.08 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 5 smd circle (at 6.35 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 6 smd circle (at 6.35 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 7 smd circle (at 5.08 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.62 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 1 smd circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 20 3V3))
    (pad 10 smd circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 2 smd circle (at 2.54 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 9 smd circle (at 2.54 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask))
    (pad 3 smd circle (at 3.81 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 8 smd circle (at 3.81 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 10 "/USB Input/MSP430_TDI"))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 80.805 72.1)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C806 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 86.38 72.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C805 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 85.525 72.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 84.55 72.925 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 73.2 67.3 45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference L804 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 45) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 86.475 72.95 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C902 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 USER1))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 83.6 72.925 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C901 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 71.325 69.625 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C821 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(C821-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 73.25 69.375 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C820 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(AE802-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 74.9 72.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference AE802 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(AE802-Pad1)"))
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 97.18 77.25 90)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW902 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 1 smd rect (at 2.075 1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 22 USER1))
    (pad 2 smd rect (at -2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.075 -1.075 90) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS810 (layer B.Cu) (tedit 5B0610A8)
    (at 97.255 52.75 270)
    (descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW901 (at 0 2.6 270) (layer B.SilkS) hide)
    (fp_text value SW_SPST (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 1 smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 2 smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/mech/PTS810.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 73.65 64.12 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C819 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(AE801-Pad1)"))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 70.28 61.315 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C822 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(AE801-Pad3)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 72.88 61.4 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C818 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(C818-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:RFECA3216060A1T (layer F.Cu) (tedit 5E42DF6C)
    (at 70.28 64 270)
    (fp_text reference AE801 (at 0 1.85 90) (layer F.SilkS) hide)
    (fp_text value Antenna_Dipole (at 0.05 -1.7 90) (layer F.Fab))
    (pad 3 smd rect (at -1.4 0 270) (size 0.35 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(AE801-Pad3)"))
    (pad 2 smd rect (at 1.4 0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.4 -0.5 270) (size 0.35 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(AE801-Pad1)"))
    (model ${KIPRJMOD}/mech/2450AT18D0100.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 0.5 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connector_USB:USB_C_Receptacle_Palconn_UTC16-G (layer F.Cu) (tedit 5CF432E0)
    (at 99.5 60.3 90)
    (descr http://www.palpilot.com/wp-content/uploads/2017/05/UTC027-GKN-OR-Rev-A.pdf)
    (tags "USB C Type-C Receptacle USB2.0")
    (attr smd)
    (fp_text reference P501 (at 0 -4.58 90) (layer F.SilkS) hide)
    (fp_text value USB_C_Plug_USB2.0 (at 0 6.24 90) (layer F.Fab))
    (fp_text user %R (at 0 1.18 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.43 90) (layer Dwgs.User))
    (pad S1 thru_hole oval (at -4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 -1.93 180) (size 2 0.9) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 4.32 2.24 180) (size 1.7 0.9) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B7 smd rect (at -0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A6 smd rect (at -0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 91 "/USB Input/D_P"))
    (pad A7 smd rect (at 0.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 90 "/USB Input/D_N"))
    (pad B8 smd rect (at -1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at -1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P501-PadA5)"))
    (pad A8 smd rect (at 1.25 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad B6 smd rect (at 0.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask))
    (pad B5 smd rect (at 1.75 -2.51 270) (size 0.3 1.16) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(P501-PadB5)"))
    (pad "" np_thru_hole circle (at 2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.89 -1.45 270) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad A4 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B9 smd rect (at -2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A1 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B12 smd rect (at -3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad B4 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad B1 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A9 smd rect (at 2.4 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 79 "/USB Input/VBUS"))
    (pad A12 smd rect (at 3.2 -2.51 90) (size 0.6 1.16) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/1054500101.stp
      (offset (xyz 0 -0.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 71.38 52.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H103 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 71.38 77.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H104 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 101.38 77.6)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H102 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via locked (layer F.Cu) (tedit 56DDB9C7)
    (at 101.38 52.56)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference H101 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value "Mounting Hole" (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module leash:0900PC15A0036 (layer F.Cu) (tedit 5E41EA1D)
    (at 78.14 65.44 270)
    (fp_text reference B801 (at 0.025 4.2 90) (layer F.SilkS) hide)
    (fp_text value 0900PC15A0036E (at -0.05 -3.025 90) (layer F.Fab))
    (pad 10 smd roundrect (at -1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 smd roundrect (at 1.15 0) (size 0.3 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 9 smd roundrect (at -0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RF/RF_2_4GHZ_P))
    (pad 8 smd roundrect (at -0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /RF/RF_2_4GHZ_N))
    (pad 7 smd roundrect (at 0.25 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RF/RF_SUB_1GHZ_P))
    (pad 6 smd roundrect (at 0.75 -0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /RF/RF_SUB_1GHZ_N))
    (pad 1 smd roundrect (at -0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (pad 2 smd roundrect (at -0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at 0.25 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at 0.75 0.8 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (model ${KIPRJMOD}/mech/0900PC15J0013.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:Texas_S-PVQFN-N48_EP5.15x5.15mm (layer B.Cu) (tedit 5E4C745D)
    (at 99.05 70.15 180)
    (descr "QFN, 48 Pin (http://www.ti.com/lit/ds/symlink/msp430f5232.pdf#page=112), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U501 (at 0 4.82) (layer B.SilkS) hide)
    (fp_text value MSP430F5500IRGZ (at 0 -4.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 48 smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 106 "/USB Input/MSP430_RST_N"))
    (pad 47 smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 46 smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 89 "/USB Input/XTAL2"))
    (pad 45 smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 88 "/USB Input/XTAL1"))
    (pad 44 smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 43 smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(C504-Pad2)"))
    (pad 42 smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 41 smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "/USB Input/VBUS"))
    (pad 40 smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 "/USB Input/D-"))
    (pad 39 smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 "/USB Input/MSP_PUR"))
    (pad 38 smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "/USB Input/D+"))
    (pad 37 smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 36 smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 35 smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 34 smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 33 smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 32 smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 31 smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 30 smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 87 "Net-(R510-Pad2)"))
    (pad 29 smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 86 "Net-(R509-Pad2)"))
    (pad 28 smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 27 smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 26 smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "/USB Input/MSP430_TCK"))
    (pad 25 smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "/USB Input/MSP430_TMS"))
    (pad 24 smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 "/USB Input/MSP430_TDI"))
    (pad 23 smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "/USB Input/MSP430_TDO"))
    (pad 22 smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 108 "Net-(R511-Pad2)"))
    (pad 21 smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 20 smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 SCK))
    (pad 19 smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 MOSI))
    (pad 18 smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 MISO))
    (pad 17 smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 107 "Net-(R507-Pad2)"))
    (pad 16 smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 15 smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (pad 14 smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(C505-Pad2)"))
    (pad 12 smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 10 smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 9 smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(C501-Pad2)"))
    (pad 6 smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad 49 smd roundrect (at 0 0 180) (size 5.15 5.15) (layers B.Cu B.Mask) (roundrect_rratio 0.049)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_S-PVQFN-N48_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 75.825 66.175 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C813 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(B801-Pad4)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 77.62 67.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C812 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 100P (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /RF/RX_TX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 93.49 63.7)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D201 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 102 ALT_IN))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 95.505 58.3 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R604 (at 0 1.17 90) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 89.975 63.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R805 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 CC1352_RX_MB1_TX))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 CC1352_RX_MSP430_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 89.965 62.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R804 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 53 CC1352_TX_MSP430_RX))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 45 CC1352_TX_MB1_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 85.68 65.9)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L802 (at 0 1.65 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /RF/DCDC_SW))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 90.28 68.73 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C301 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 93.585 62.7 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 93.685 58.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "100 pF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 87.145 50.58)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D402 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 LED1))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 84.25 50.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D401 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 LED2))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 90.055 50.59)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D403 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 3V3))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 80.9 50.57)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D404 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 900M))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 77.41 50.6)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D405 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 2.4G))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 87.14 50.57)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R402 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(D402-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 84.25 50.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R401 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(D401-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 90.05 50.59)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R403 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(D403-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 80.9 50.58)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R404 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(D404-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 77.4 50.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R405 (at 0 1.17) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.17) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(D405-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 95.535 62.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R601 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 V_ALT))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(R601-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 93.685 59.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R602 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 92.23 59.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R603 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 76.63 70.5 315)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C801 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(C801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 78.855 71.125 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C802 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "12 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C802-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 87.38 72.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C803 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value "1 uF" (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C803-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 88.025 65.1 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C804 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 84.48 63 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 80.28 63.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C808 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 82.88 61.9 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C809 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 85.5 67.65 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C810 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "22 uF" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /RF/VDDR))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer B.Cu) (tedit 5B301BBE)
    (at 78.725 73.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 76.32 64.11 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C814 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 74.3 62.1 225)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C816 (at 0 -1.17 45) (layer F.SilkS) hide)
    (fp_text value "1 pF" (at 0 1.17 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.485 0 225) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 73.875 65.925 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C815 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2.7 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(C813-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 71.85 67.95 135)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C817 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "5.6 pF" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(C817-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 135) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 74.99 63.44 315)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L803 (at 0 -1.17 135) (layer F.SilkS) hide)
    (fp_text value "2 nH" (at 0 1.17 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(C816-Pad2)"))
    (pad 2 smd roundrect (at 0.485 0 315) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(B801-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 78.725 71.525)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R807 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 RESET_N))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 78.725 69.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R809 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(R809-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 78.725 70.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R810 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 2.21K (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 109 ~FLASH_CS))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 78.725 72.505)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R811 (at 0 1.17 180) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C811-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 90.96 58.76 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C603 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value "10 uF" (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:TPS62821DLC (layer B.Cu) (tedit 5D2676FA)
    (at 94.885 61.1)
    (fp_text reference U601 (at 0.1 1.975 180) (layer B.SilkS) hide)
    (fp_text value TPS62821DLC (at 0 0.5 180) (layer B.Fab))
    (pad 8 smd roundrect (at 0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 74 "Net-(R601-Pad1)"))
    (pad 7 smd roundrect (at 0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (pad 6 smd roundrect (at 0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 73 "Net-(L601-Pad1)"))
    (pad 5 smd roundrect (at 0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 4 smd roundrect (at -0.675 -0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2))
    (pad 3 smd roundrect (at -0.675 -0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 2 smd roundrect (at -0.675 0.25) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(C602-Pad2)"))
    (pad 1 smd roundrect (at -0.675 0.75) (size 0.55 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 23 V_ALT))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/X2SON-8_1.4x1mm_P0.35mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1.3 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:MX25R8035FZUIL0 (layer B.Cu) (tedit 5E42FFC6)
    (at 80.775 71.08 270)
    (fp_text reference U802 (at 0 2 90) (layer B.SilkS) hide)
    (fp_text value MX25R8035FZUIL0 (at 0 -2 90) (layer B.Fab))
    (pad 9 smd custom (at 0 0 270) (size 0.2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0 0.8) (xy 0.1 0.8) (xy 0.1 -0.8) (xy -0.1 -0.8) (xy -0.1 0.7)
) (width 0))
      ))
    (pad 8 smd rect (at 1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(C811-Pad2)"))
    (pad 7 smd rect (at 1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 RESET_N))
    (pad 6 smd rect (at 1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 35 SCK))
    (pad 5 smd rect (at 1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 38 MOSI))
    (pad 4 smd rect (at -1.2 -0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.2 -0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R809-Pad2)"))
    (pad 2 smd rect (at -1.2 0.25 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 33 MISO))
    (pad 1 smd rect (at -1.2 0.75 270) (size 0.3 0.25) (layers B.Cu B.Paste B.Mask)
      (net 109 ~FLASH_CS))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.4 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 71.48 57.8 270)
    (fp_text reference J801 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 1 smd rect (at 1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C818-Pad2)"))
    (pad 2 smd rect (at 0 -1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 270) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.475 270) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module leash:A-1JB (layer F.Cu) (tedit 5C5DBBF1)
    (at 71.25 72.85 90)
    (fp_text reference J802 (at 0.28 2.82 90) (layer F.SilkS) hide)
    (fp_text value UFL (at 0.31 -2.91 90) (layer F.Fab))
    (pad 1 smd rect (at 1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C821-Pad2)"))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/mech/a_1jb_3d_model_file.stp
      (offset (xyz 0 0 1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 88.43 58.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R802 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R802-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 CC1352_TX_MB2_RX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer B.Cu) (tedit 5B301BBD)
    (at 86.05 58.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R803 (at 0 1.17 270) (layer B.SilkS) hide)
    (fp_text value 0 (at 0 -1.17 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab) hide)
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(R803-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 CC1352_RX_MB2_TX))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 96.63 52.575 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D501 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value BAT54 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 V_ALT))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 90.25 65.625)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L801 (at 0 1.43 180) (layer B.SilkS) hide)
    (fp_text value "6.8 uH" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 VDD))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 VDDS))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 80.4 61.3 180)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y802 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Crystal_GND2 (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.7 -0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U801-Pad47)"))
    (pad 2 smd rect (at 0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.7 0.55 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U801-Pad46)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_2012-2Pin_2.0x1.2mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 77.755 69.575 315)
    (descr "SMD Crystal 2012/2 http://txccrystal.com/images/pdf/9ht11.pdf, 2.0x1.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y801 (at 0 -1.8 135) (layer F.SilkS) hide)
    (fp_text value Crystal (at 0 1.8 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(C802-Pad1)"))
    (pad 1 smd rect (at -0.7 0 315) (size 0.6 1.1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C801-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_TXC_AX_8045-2Pin_8.0x4.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 0.25 0.3 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module leash:L_0806_2012Metric (layer B.Cu) (tedit 5D2F3EE6)
    (at 96.985 59.9 90)
    (descr "Inductor SMD 0806 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L601 (at 0 1.65 90) (layer B.SilkS) hide)
    (fp_text value INDUCTOR (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab) hide)
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "/Boost Converters/3V3_BUCK_VOUT"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(L601-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 100 (width 0.15) (layer Dwgs.User)
    (gr_text "100.000 mm" (at 242.3 95.1 270) (layer Dwgs.User))
    (feature1 (pts (xy 217.88 145.1) (xy 241.586421 145.1)))
    (feature2 (pts (xy 217.88 45.1) (xy 241.586421 45.1)))
    (crossbar (pts (xy 241 45.1) (xy 241 145.1)))
    (arrow1a (pts (xy 241 145.1) (xy 240.413579 143.973496)))
    (arrow1b (pts (xy 241 145.1) (xy 241.586421 143.973496)))
    (arrow2a (pts (xy 241 45.1) (xy 240.413579 46.226504)))
    (arrow2b (pts (xy 241 45.1) (xy 241.586421 46.226504)))
  )
  (dimension 154 (width 0.15) (layer Dwgs.User)
    (gr_text "154.000 mm" (at 140.88 27.7) (layer Dwgs.User))
    (feature1 (pts (xy 217.88 45.1) (xy 217.88 28.413579)))
    (feature2 (pts (xy 63.88 45.1) (xy 63.88 28.413579)))
    (crossbar (pts (xy 63.88 29) (xy 217.88 29)))
    (arrow1a (pts (xy 217.88 29) (xy 216.753496 29.586421)))
    (arrow1b (pts (xy 217.88 29) (xy 216.753496 28.413579)))
    (arrow2a (pts (xy 63.88 29) (xy 65.006504 29.586421)))
    (arrow2b (pts (xy 63.88 29) (xy 65.006504 28.413579)))
  )
  (gr_text VCUT (at 211.88 155.1) (layer Eco1.User))
  (gr_text VCUT (at 68.88 155.1) (layer Eco1.User))
  (gr_text "VCUT x 2" (at 175.88 155.1) (layer Eco1.User))
  (gr_text "VCUT x 2" (at 139.88 155.1) (layer Eco1.User))
  (gr_text "VCUT x 2" (at 103.88 155.1) (layer Eco1.User))
  (gr_text VCUT (at 52.88 110.1) (layer Eco1.User))
  (gr_text VCUT (at 52.88 140.1) (layer Eco1.User))
  (gr_text VCUT (at 225.88 140.1) (layer Eco1.User))
  (gr_text VCUT (at 225.88 110.1) (layer Eco1.User))
  (gr_text VCUT (at 225.88 80.1) (layer Eco1.User))
  (gr_text VCUT (at 225.88 50.1) (layer Eco1.User))
  (gr_text VCUT (at 211.88 36.1) (layer Eco1.User))
  (gr_text "VCUT x 2" (at 175.88 37.1) (layer Eco1.User))
  (gr_text "VCUT x 2" (at 140.88 37.1) (layer Eco1.User))
  (gr_text "VCUT x 2" (at 104.88 37.1) (layer Eco1.User))
  (gr_text VCUT (at 52.88 80.1) (layer Eco1.User))
  (gr_text VCUT (at 52.88 50.1) (layer Eco1.User))
  (gr_text VCUT (at 68.88 37.1) (layer Eco1.User))
  (gr_line (start 176.88 114.6) (end 176.88 135.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 176.88 84.6) (end 176.88 105.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 176.88 54.6) (end 176.88 75.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140.88 75.1) (end 140.88 54.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140.88 105.1) (end 140.88 84.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140.88 135.1) (end 140.88 114.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 104.88 114.6) (end 104.88 135.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 104.88 84.6) (end 104.88 105.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 104.88 54.6) (end 104.88 75.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 212.88 114.6) (end 212.88 135.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 63.88 145.1) (end 63.88 45.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 217.88 145.1) (end 63.88 145.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 217.88 45.1) (end 217.88 145.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 63.88 45.1) (end 217.88 45.1) (layer Edge.Cuts) (width 0.05))
  (gr_text CC1352R (at 196.88 96.52 270) (layer F.SilkS))
  (gr_text 2.4G (at 184.39 80.52 180) (layer F.SilkS))
  (gr_arc (start 176.38 114.6) (end 176.88 114.6) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 212.38 114.6) (end 212.88 114.6) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_text P (at 160.78 110.43 180) (layer F.SilkS))
  (gr_line (start 211.88 84.6) (end 211.88 105.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 175.88 84.6) (end 175.88 105.1) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 176.38 84.6) (end 176.88 84.6) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 176.38 135.1) (end 175.88 135.1) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_text 900 (at 187.85 110.49 180) (layer F.SilkS))
  (gr_arc (start 176.38 105.1) (end 175.88 105.1) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_text "BeagleConnect\nRev B" (at 153.72 121.53) (layer F.SilkS))
  (gr_arc (start 176.38 54.6) (end 176.88 54.6) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 212.88 54.6) (end 212.88 75.1) (layer Edge.Cuts) (width 0.05))
  (gr_text 1 (at 194.05 80.54 180) (layer F.SilkS))
  (gr_text CC1352R (at 160.88 126.52 270) (layer F.SilkS))
  (gr_arc (start 212.38 75.1) (end 211.88 75.1) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_text C (at 199.84 110.57 180) (layer F.SilkS))
  (gr_text 900 (at 187.85 80.49 180) (layer F.SilkS))
  (gr_text 1 (at 194.05 50.54 180) (layer F.SilkS))
  (gr_text 1 (at 158.05 110.54 180) (layer F.SilkS))
  (gr_text 2 (at 190.94 80.56 180) (layer F.SilkS))
  (gr_line (start 175.88 114.6) (end 175.88 135.1) (layer Edge.Cuts) (width 0.05))
  (gr_text P (at 196.78 80.43 180) (layer F.SilkS))
  (gr_text 2 (at 190.94 110.56 180) (layer F.SilkS))
  (gr_line (start 211.88 54.6) (end 211.88 75.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 175.88 54.6) (end 175.88 75.1) (layer Edge.Cuts) (width 0.05))
  (gr_text 2 (at 190.94 50.56 180) (layer F.SilkS))
  (gr_text C (at 199.84 80.57 180) (layer F.SilkS))
  (gr_line (start 212.88 84.6) (end 212.88 105.1) (layer Edge.Cuts) (width 0.05))
  (gr_text 900 (at 187.85 50.49 180) (layer F.SilkS))
  (gr_text "BeagleConnect\nRev B" (at 189.72 121.53) (layer F.SilkS))
  (gr_text CC1352R (at 196.88 126.52 270) (layer F.SilkS))
  (gr_text C (at 163.84 110.57 180) (layer F.SilkS))
  (gr_text 900 (at 151.85 80.49 180) (layer F.SilkS))
  (gr_text CC1352R (at 160.88 96.52 270) (layer F.SilkS))
  (gr_text 2.4G (at 148.39 110.52 180) (layer F.SilkS))
  (gr_text "BeagleConnect\nRev B" (at 189.72 91.53) (layer F.SilkS))
  (gr_text CC1352R (at 196.88 66.52 270) (layer F.SilkS))
  (gr_text 2 (at 154.94 80.56 180) (layer F.SilkS))
  (gr_text 2 (at 154.94 110.56 180) (layer F.SilkS))
  (gr_text C (at 163.84 80.57 180) (layer F.SilkS))
  (gr_text P (at 196.78 50.43 180) (layer F.SilkS))
  (gr_text 900 (at 151.85 110.49 180) (layer F.SilkS))
  (gr_text P (at 196.78 110.43 180) (layer F.SilkS))
  (gr_text P (at 160.78 80.43 180) (layer F.SilkS))
  (gr_text "BeagleConnect\nRev B" (at 153.72 91.53) (layer F.SilkS))
  (gr_text "BeagleConnect\nRev B" (at 189.72 61.53) (layer F.SilkS))
  (gr_arc (start 212.38 54.6) (end 212.88 54.6) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_text 2.4G (at 184.39 110.52 180) (layer F.SilkS))
  (gr_line (start 211.88 114.6) (end 211.88 135.1) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 176.38 75.1) (end 175.88 75.1) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 212.38 84.6) (end 212.88 84.6) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 212.38 135.1) (end 211.88 135.1) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 212.38 105.1) (end 211.88 105.1) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_text 1 (at 158.05 80.54 180) (layer F.SilkS))
  (gr_text C (at 199.84 50.57 180) (layer F.SilkS))
  (gr_text 2.4G (at 184.39 50.52 180) (layer F.SilkS))
  (gr_text 1 (at 194.05 110.54 180) (layer F.SilkS))
  (gr_text "BeagleConnect\nRev B" (at 153.72 61.53) (layer F.SilkS))
  (gr_text CC1352R (at 160.88 66.52 270) (layer F.SilkS))
  (gr_text 2.4G (at 148.39 50.52 180) (layer F.SilkS))
  (gr_text 900 (at 151.85 50.49 180) (layer F.SilkS))
  (gr_text 2 (at 154.94 50.56 180) (layer F.SilkS))
  (gr_text 1 (at 158.05 50.54 180) (layer F.SilkS))
  (gr_text P (at 160.78 50.43 180) (layer F.SilkS))
  (gr_text C (at 163.84 50.57 180) (layer F.SilkS))
  (gr_text 2.4G (at 148.39 80.52 180) (layer F.SilkS))
  (gr_arc (start 140.38 114.6) (end 140.88 114.6) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_text P (at 124.78 110.43 180) (layer F.SilkS))
  (gr_line (start 139.88 84.6) (end 139.88 105.1) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 140.38 84.6) (end 140.88 84.6) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 140.38 135.1) (end 139.88 135.1) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 140.38 105.1) (end 139.88 105.1) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_text "BeagleConnect\nRev B" (at 117.72 121.53) (layer F.SilkS))
  (gr_arc (start 140.38 54.6) (end 140.88 54.6) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_text CC1352R (at 124.88 126.52 270) (layer F.SilkS))
  (gr_text 1 (at 122.05 110.54 180) (layer F.SilkS))
  (gr_line (start 139.88 114.6) (end 139.88 135.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.88 54.6) (end 139.88 75.1) (layer Edge.Cuts) (width 0.05))
  (gr_text C (at 127.84 110.57 180) (layer F.SilkS))
  (gr_text 900 (at 115.85 80.49 180) (layer F.SilkS))
  (gr_text CC1352R (at 124.88 96.52 270) (layer F.SilkS))
  (gr_text 2.4G (at 112.39 110.52 180) (layer F.SilkS))
  (gr_text 2 (at 118.94 80.56 180) (layer F.SilkS))
  (gr_text 2 (at 118.94 110.56 180) (layer F.SilkS))
  (gr_text C (at 127.84 80.57 180) (layer F.SilkS))
  (gr_text 900 (at 115.85 110.49 180) (layer F.SilkS))
  (gr_text P (at 124.78 80.43 180) (layer F.SilkS))
  (gr_text "BeagleConnect\nRev B" (at 117.72 91.53) (layer F.SilkS))
  (gr_arc (start 140.38 75.1) (end 139.88 75.1) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_text 1 (at 122.05 80.54 180) (layer F.SilkS))
  (gr_text "BeagleConnect\nRev B" (at 117.72 61.53) (layer F.SilkS))
  (gr_text CC1352R (at 124.88 66.52 270) (layer F.SilkS))
  (gr_text 2.4G (at 112.39 50.52 180) (layer F.SilkS))
  (gr_text 900 (at 115.85 50.49 180) (layer F.SilkS))
  (gr_text 2 (at 118.94 50.56 180) (layer F.SilkS))
  (gr_text 1 (at 122.05 50.54 180) (layer F.SilkS))
  (gr_text P (at 124.78 50.43 180) (layer F.SilkS))
  (gr_text C (at 127.84 50.57 180) (layer F.SilkS))
  (gr_text 2.4G (at 112.39 80.52 180) (layer F.SilkS))
  (gr_line (start 103.88 114.6) (end 103.88 135.1) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 104.38 114.6) (end 104.88 114.6) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 104.38 135.1) (end 103.88 135.1) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_text 900 (at 79.85 110.49 180) (layer F.SilkS))
  (gr_text CC1352R (at 88.88 126.52 270) (layer F.SilkS))
  (gr_text 2 (at 82.94 110.56 180) (layer F.SilkS))
  (gr_text C (at 91.84 110.57 180) (layer F.SilkS))
  (gr_text P (at 88.78 110.43 180) (layer F.SilkS))
  (gr_text "BeagleConnect\nRev B" (at 81.72 121.53) (layer F.SilkS))
  (gr_text 1 (at 86.05 110.54 180) (layer F.SilkS))
  (gr_text 2.4G (at 76.39 110.52 180) (layer F.SilkS))
  (gr_arc (start 104.38 84.6) (end 104.88 84.6) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.88 84.6) (end 103.88 105.1) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 104.38 105.1) (end 103.88 105.1) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_text "BeagleConnect\nRev B" (at 81.72 91.53) (layer F.SilkS))
  (gr_text CC1352R (at 88.88 96.52 270) (layer F.SilkS))
  (gr_text 2.4G (at 76.39 80.52 180) (layer F.SilkS))
  (gr_text 900 (at 79.85 80.49 180) (layer F.SilkS))
  (gr_text 2 (at 82.94 80.56 180) (layer F.SilkS))
  (gr_text 1 (at 86.05 80.54 180) (layer F.SilkS))
  (gr_text P (at 88.78 80.43 180) (layer F.SilkS))
  (gr_text C (at 91.84 80.57 180) (layer F.SilkS))
  (gr_arc (start 104.38 75.1) (end 103.88 75.1) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.88 54.6) (end 103.88 75.1) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 104.38 54.6) (end 104.88 54.6) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_text C (at 91.84 50.57 180) (layer F.SilkS))
  (gr_text P (at 88.78 50.43 180) (layer F.SilkS))
  (gr_text 1 (at 86.05 50.54 180) (layer F.SilkS))
  (gr_text 2 (at 82.94 50.56 180) (layer F.SilkS))
  (gr_text 900 (at 79.85 50.49 180) (layer F.SilkS))
  (gr_text 2.4G (at 76.39 50.52 180) (layer F.SilkS))
  (gr_text CC1352R (at 88.88 66.52 270) (layer F.SilkS))
  (gr_text "BeagleConnect\nRev B" (at 81.72 61.53) (layer F.SilkS))
  (zone (net 0) (net_name "") (layers F.Cu GND PWR B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71.575 66.925) (xy 68.9 66.95) (xy 68.88 61.075) (xy 71.58 61.075)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.88 80.1) (xy 68.878035 80.1) (xy 68.878035 50.1) (xy 103.88 50.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.891002 80.1) (xy 68.889037 80.1) (xy 68.889037 50.1) (xy 103.891002 50.1)
      )
    )
  )
  (zone (net 20) (net_name 3V3) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.88 80.1) (xy 77.38 80.1) (xy 77.38 73.9) (xy 90.58 73.9) (xy 90.58 57.3)
        (xy 77.08 57.2) (xy 77.08 50.1) (xy 103.88 50.1)
      )
    )
  )
  (zone (net 19) (net_name VDDS) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.28 73.6) (xy 77.38 73.6) (xy 77.08 57.7) (xy 90.28 57.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.859488 80.1) (xy 68.857523 80.1) (xy 68.857523 50.1) (xy 103.859488 50.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.859488 110.1) (xy 68.857523 110.1) (xy 68.857523 80.1) (xy 103.859488 80.1)
      )
    )
  )
  (zone (net 20) (net_name 3V3) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.88 110.1) (xy 77.38 110.1) (xy 77.38 103.9) (xy 90.58 103.9) (xy 90.58 87.3)
        (xy 77.08 87.2) (xy 77.08 80.1) (xy 103.88 80.1)
      )
    )
  )
  (zone (net 19) (net_name VDDS) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.28 103.6) (xy 77.38 103.6) (xy 77.08 87.7) (xy 90.28 87.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.891002 110.1) (xy 68.889037 110.1) (xy 68.889037 80.1) (xy 103.891002 80.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.88 110.1) (xy 68.878035 110.1) (xy 68.878035 80.1) (xy 103.88 80.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu GND PWR B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71.575 96.925) (xy 68.9 96.95) (xy 68.88 91.075) (xy 71.58 91.075)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.88 140.1) (xy 68.878035 140.1) (xy 68.878035 110.1) (xy 103.88 110.1)
      )
    )
  )
  (zone (net 19) (net_name VDDS) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.28 133.6) (xy 77.38 133.6) (xy 77.08 117.7) (xy 90.28 117.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu GND PWR B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71.575 126.925) (xy 68.9 126.95) (xy 68.88 121.075) (xy 71.58 121.075)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.891002 140.1) (xy 68.889037 140.1) (xy 68.889037 110.1) (xy 103.891002 110.1)
      )
    )
  )
  (zone (net 20) (net_name 3V3) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.88 140.1) (xy 77.38 140.1) (xy 77.38 133.9) (xy 90.58 133.9) (xy 90.58 117.3)
        (xy 77.08 117.2) (xy 77.08 110.1) (xy 103.88 110.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.859488 140.1) (xy 68.857523 140.1) (xy 68.857523 110.1) (xy 103.859488 110.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.859488 80.1) (xy 104.857523 80.1) (xy 104.857523 50.1) (xy 139.859488 50.1)
      )
    )
  )
  (zone (net 20) (net_name 3V3) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.88 80.1) (xy 113.38 80.1) (xy 113.38 73.9) (xy 126.58 73.9) (xy 126.58 57.3)
        (xy 113.08 57.2) (xy 113.08 50.1) (xy 139.88 50.1)
      )
    )
  )
  (zone (net 19) (net_name VDDS) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.28 73.6) (xy 113.38 73.6) (xy 113.08 57.7) (xy 126.28 57.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.891002 80.1) (xy 104.889037 80.1) (xy 104.889037 50.1) (xy 139.891002 50.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.88 110.1) (xy 104.878035 110.1) (xy 104.878035 80.1) (xy 139.88 80.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.88 80.1) (xy 104.878035 80.1) (xy 104.878035 50.1) (xy 139.88 50.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu GND PWR B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.575 66.925) (xy 104.9 66.95) (xy 104.88 61.075) (xy 107.58 61.075)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.88 140.1) (xy 104.878035 140.1) (xy 104.878035 110.1) (xy 139.88 110.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.891002 140.1) (xy 104.889037 140.1) (xy 104.889037 110.1) (xy 139.891002 110.1)
      )
    )
  )
  (zone (net 19) (net_name VDDS) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.28 103.6) (xy 113.38 103.6) (xy 113.08 87.7) (xy 126.28 87.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu GND PWR B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.575 126.925) (xy 104.9 126.95) (xy 104.88 121.075) (xy 107.58 121.075)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.859488 140.1) (xy 104.857523 140.1) (xy 104.857523 110.1) (xy 139.859488 110.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu GND PWR B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.575 96.925) (xy 104.9 96.95) (xy 104.88 91.075) (xy 107.58 91.075)
      )
    )
  )
  (zone (net 19) (net_name VDDS) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.28 133.6) (xy 113.38 133.6) (xy 113.08 117.7) (xy 126.28 117.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.891002 110.1) (xy 104.889037 110.1) (xy 104.889037 80.1) (xy 139.891002 80.1)
      )
    )
  )
  (zone (net 20) (net_name 3V3) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.88 140.1) (xy 113.38 140.1) (xy 113.38 133.9) (xy 126.58 133.9) (xy 126.58 117.3)
        (xy 113.08 117.2) (xy 113.08 110.1) (xy 139.88 110.1)
      )
    )
  )
  (zone (net 20) (net_name 3V3) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.88 110.1) (xy 113.38 110.1) (xy 113.38 103.9) (xy 126.58 103.9) (xy 126.58 87.3)
        (xy 113.08 87.2) (xy 113.08 80.1) (xy 139.88 80.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.859488 110.1) (xy 104.857523 110.1) (xy 104.857523 80.1) (xy 139.859488 80.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.859488 80.1) (xy 140.857523 80.1) (xy 140.857523 50.1) (xy 175.859488 50.1)
      )
    )
  )
  (zone (net 20) (net_name 3V3) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.88 80.1) (xy 149.38 80.1) (xy 149.38 73.9) (xy 162.58 73.9) (xy 162.58 57.3)
        (xy 149.08 57.2) (xy 149.08 50.1) (xy 175.88 50.1)
      )
    )
  )
  (zone (net 19) (net_name VDDS) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.28 73.6) (xy 149.38 73.6) (xy 149.08 57.7) (xy 162.28 57.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.891002 80.1) (xy 140.889037 80.1) (xy 140.889037 50.1) (xy 175.891002 50.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.859488 110.1) (xy 176.857523 110.1) (xy 176.857523 80.1) (xy 211.859488 80.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.891002 140.1) (xy 176.889037 140.1) (xy 176.889037 110.1) (xy 211.891002 110.1)
      )
    )
  )
  (zone (net 20) (net_name 3V3) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.88 140.1) (xy 185.38 140.1) (xy 185.38 133.9) (xy 198.58 133.9) (xy 198.58 117.3)
        (xy 185.08 117.2) (xy 185.08 110.1) (xy 211.88 110.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.88 110.1) (xy 140.878035 110.1) (xy 140.878035 80.1) (xy 175.88 80.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.859488 80.1) (xy 176.857523 80.1) (xy 176.857523 50.1) (xy 211.859488 50.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.88 80.1) (xy 140.878035 80.1) (xy 140.878035 50.1) (xy 175.88 50.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu GND PWR B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.575 66.925) (xy 140.9 66.95) (xy 140.88 61.075) (xy 143.58 61.075)
      )
    )
  )
  (zone (net 20) (net_name 3V3) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.88 110.1) (xy 185.38 110.1) (xy 185.38 103.9) (xy 198.58 103.9) (xy 198.58 87.3)
        (xy 185.08 87.2) (xy 185.08 80.1) (xy 211.88 80.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.88 140.1) (xy 140.878035 140.1) (xy 140.878035 110.1) (xy 175.88 110.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu GND PWR B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.575 66.925) (xy 176.9 66.95) (xy 176.88 61.075) (xy 179.58 61.075)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.88 80.1) (xy 176.878035 80.1) (xy 176.878035 50.1) (xy 211.88 50.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.88 110.1) (xy 176.878035 110.1) (xy 176.878035 80.1) (xy 211.88 80.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.891002 140.1) (xy 140.889037 140.1) (xy 140.889037 110.1) (xy 175.891002 110.1)
      )
    )
  )
  (zone (net 19) (net_name VDDS) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.28 73.6) (xy 185.38 73.6) (xy 185.08 57.7) (xy 198.28 57.7)
      )
    )
  )
  (zone (net 19) (net_name VDDS) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.28 103.6) (xy 149.38 103.6) (xy 149.08 87.7) (xy 162.28 87.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu GND PWR B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.575 126.925) (xy 140.9 126.95) (xy 140.88 121.075) (xy 143.58 121.075)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.859488 140.1) (xy 140.857523 140.1) (xy 140.857523 110.1) (xy 175.859488 110.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu GND PWR B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.575 96.925) (xy 140.9 96.95) (xy 140.88 91.075) (xy 143.58 91.075)
      )
    )
  )
  (zone (net 19) (net_name VDDS) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.28 103.6) (xy 185.38 103.6) (xy 185.08 87.7) (xy 198.28 87.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu GND PWR B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.575 126.925) (xy 176.9 126.95) (xy 176.88 121.075) (xy 179.58 121.075)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.859488 140.1) (xy 176.857523 140.1) (xy 176.857523 110.1) (xy 211.859488 110.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu GND PWR B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.575 96.925) (xy 176.9 96.95) (xy 176.88 91.075) (xy 179.58 91.075)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.891002 110.1) (xy 176.889037 110.1) (xy 176.889037 80.1) (xy 211.891002 80.1)
      )
    )
  )
  (zone (net 19) (net_name VDDS) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.28 133.6) (xy 149.38 133.6) (xy 149.08 117.7) (xy 162.28 117.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.891002 110.1) (xy 140.889037 110.1) (xy 140.889037 80.1) (xy 175.891002 80.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.88 140.1) (xy 176.878035 140.1) (xy 176.878035 110.1) (xy 211.88 110.1)
      )
    )
  )
  (zone (net 20) (net_name 3V3) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.88 140.1) (xy 149.38 140.1) (xy 149.38 133.9) (xy 162.58 133.9) (xy 162.58 117.3)
        (xy 149.08 117.2) (xy 149.08 110.1) (xy 175.88 110.1)
      )
    )
  )
  (zone (net 20) (net_name 3V3) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.88 80.1) (xy 185.38 80.1) (xy 185.38 73.9) (xy 198.58 73.9) (xy 198.58 57.3)
        (xy 185.08 57.2) (xy 185.08 50.1) (xy 211.88 50.1)
      )
    )
  )
  (zone (net 20) (net_name 3V3) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.88 110.1) (xy 149.38 110.1) (xy 149.38 103.9) (xy 162.58 103.9) (xy 162.58 87.3)
        (xy 149.08 87.2) (xy 149.08 80.1) (xy 175.88 80.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer GND) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.859488 110.1) (xy 140.857523 110.1) (xy 140.857523 80.1) (xy 175.859488 80.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.891002 80.1) (xy 176.889037 80.1) (xy 176.889037 50.1) (xy 211.891002 50.1)
      )
    )
  )
  (zone (net 19) (net_name VDDS) (layer PWR) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.28 133.6) (xy 185.38 133.6) (xy 185.08 117.7) (xy 198.28 117.7)
      )
    )
  )
)
